Project Name:	DER
	Project Code:	DER	Site ID:	H200	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (TAS)
	Site Information
	Desc. By:	G.M. Dimmock	Locality:	3.2KM south west of Dysart:
	Date Desc.:	27/05/60	Elevation:	 396 metres
	Map Ref.:	Rainfall:	760
	Northing/Long.:	147.190277777778	Runoff:	Rapid
	Easting/Lat.:	-42.5916666666667	Drainage:	Imperfectly drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	 Pss	Substrate Material:	0.7 m deep,Sandstone 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	Hills
	Morph. Type:	Upper-slope	Relief:	No Data
	Elem. Type:	Hillslope	Slope Category:	Moderately inclined
	Slope:	10.5 % 	Aspect:	45 degrees
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Mesotrophic Brown Kandosol     	Principal Profile Form:	Dy4.61
	ASC Confidence:	Great Soil Group:	Grey-brown 
	All necessary analytical data are available.	podzolic soil
	Site Disturbance:	Limited clearing, for example selective logging
	Vegetation:	Low Strata - Chenopod shrub, , . *Species includes - Banksia marginata
	Mid Strata - Tree, , . *Species includes - None recorded
	Tall Strata - Tree, 20.01-35m, . *Species includes - Eucalyptus obliqua, Eucalyptus viminalis
	Surface Coarse Fragments:
	Profile Morphology
	A1	0 - 0.02 m	Very dark greyish brown (10YR3/2-Moist); ; Sand; Single grain grade of structure; Moist; Very 
	weak consistence; Many
	A1	0.02 - 0.13 m	Very dark greyish brown (10YR3/2-Moist); ; Sand; Single grain grade of structure; ManyDiffuse 
	change to - 
	A1A2	0.13 - 0.24 m	Greyish brown (10YR5/2-Moist); ; Sand; Single grain grade of structure; CommonDiffuse change
	 to - 
	A2	0.24 - 0.3 m	Greyish brown (10YR5/2-Moist); ; Sand; Single grain grade of structure; Few
	A2B	0.3 - 0.39 m	Greyish brown (10YR5/2-Moist); , 10YR53; Sand; Single grain grade of structure; 0-2%, Gravel, 
	coarse fragments; Sharp, Wavy change to - 
	B	0.39 - 0.47 m	Very dark greyish brown (10YR3/2-Moist); , 10YR56; Clayey sand; Massive grade of structure; 
	Wet; Weak consistence; Sharp change to - 
	B	0.47 - 0.58 m	Yellowish brown (10YR5/5-Moist); , 10YR66; , 10YR43; Clayey sand; Massive grade of structure;
	 Fine, (0 - 5) mm crack; Wet; Very weak consistence; 
	B	0.62 - 0.69 m	Yellowish brown (10YR5/8-Moist); ; Sandy clay loam; Massive grade of structure; Moist; Firm 
	consistence; Sharp change to - 
	Morphological Notes
	Observation Notes
	39-47CM SOFT 7.5YR56 LUMPS OF DECOMPOSED SA <25MM:47-58CM 10YR56 COATINGS DOWN CRACKS:AT 69CM THIN
	 GLEYED LAYER PM:     
	Site Notes
	MONMOUTH

	Project Name:	DER
	Project Code:	DER	Site ID:	H200	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (TAS)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.02	5.2A	 0.021A	 4.8H	 1.5	 0.24	 0.09	 8.5H	 20.7B
	 14.1E
	0.02 - 0.13	4.2A	 0.042A	 0.79H	 0.7	 0.2	 0.17	 14.4H	 20.1B
	 18.2E
	0.13 - 0.24	4.3A	 0.024A
	0.24 - 0.3	4.5A	 0.015A
	0.3 - 0.39	4.7A	 0.015A	 0.17H	 0.1	 0.06	 0.09	 14H	 2B
	 1.6E
	0.39 - 0.47	5.1A	 0.021A	 0.19H	 1.5	 0.16	 0.2	 6.8H	 12.3B
	 10.2E
	0.47 - 0.58	5.3A	 0.018A
	0.62 - 0.69	5.9A	 0.018A	 0.2H	 2	 0.4	 0.22	 2.7H	 7B
	 4.4E
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.02	 3.7D	 0.006D	 0.123A	 0	 37B	 55	 2	 2
	0.02 - 0.13	 3.1D	 0.004D	 0.095A	 0	 36B	 56	 1	 2
	0.13 - 0.24	 1.3D	 0.03A
	0.24 - 0.3
	0.3 - 0.39	 1	 35B	 61	 2	 2
	0.39 - 0.47	 0	 27D	 53	 3	 16
	0.47 - 0.58
	0.62 - 0.69	 0	 28D	 45	 3	 26
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.02
	0.02 - 0.13
	0.13 - 0.24
	0.24 - 0.3
	0.3 - 0.39
	0.39 - 0.47
	0.47 - 0.58
	0.62 - 0.69

	Project Name:	DER
	Project Code:	DER	Site ID:	H200	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (TAS)
	Laboratory Analyses Completed for this profile
	15E1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) by compulsive exchange, no pretreatment for soluble 
	15E1_K	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MG	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_NA	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15G_C_H1	Exchangeable hydrogen - meq per 100g of soil - Hydrogen By back titration of A or B
	15G1_H	Hydrogen Cation - meq per 100g of soil - 1M KCl Exch. Acidity By titration to pH 8.0
	15J_H	Sum of Ex. cations + Ex. acidity - Sum of basic exch. cations and exch. (Hydrogen)
	2_LOI	Loss on Ignition (%)
	2A1	Air-dry moisture content
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	5A2	Chloride - 1:5 soil/water extract, automated colour
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	7A2	Total nitrogen - semimicro Kjeldahl , automated colour
	9A_HCL	Total element - P(%) - By boiling HCl
	P10_GRAV	Gravel (%)
	P10_PB_C	Clay (%) - Plummet balance
	P10_PB_CS	Coarse sand (%) - Plummet balance
	P10_PB_FS	Fine sand (%) - Plummet balance
	P10_PB_Z	Silt (%) - Plummet balance
	P10A1_C	Clay (%) - Pipette
	P10A1_CS	Coarse sand (%) - Pipette
	P10A1_FS	Fine sand (%) - Pipette
	P10A1_Z	Silt (%) - Pipette