Project Name:	DER
	Project Code:	DER	Site ID:	H233	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (TAS)
	Site Information
	Desc. By:	G.M. Dimmock	Locality:	5.7KM NE of Bagdad P.O.:40M from gate along rough
	 track then 16M on LHSof track:
	Date Desc.:	04/12/61	Elevation:	 442 metres
	Map Ref.:	Rainfall:	620
	Northing/Long.:	147.270833333333	Runoff:	Moderately rapid
	Easting/Lat.:	-42.5902777777778	Drainage:	Poorly drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	  Pd	Substrate Material:	Auger boring, 0.81 m deep,Dolerite 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	No Data
	Morph. Type:	Ridge	Relief:	No Data
	Elem. Type:	Hillslope	Slope Category:	Gently inclined
	Slope:	3.5 % 	Aspect:	315 degrees
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Bleached-Vertic Eutrophic Brown Kurosol     	Principal Profile Form:	Db1.41
	ASC Confidence:	Great Soil Group:	Grey-brown 
	All necessary analytical data are available.	podzolic soil
	Site Disturbance:	Limited clearing, for example selective logging
	Vegetation:	Low Strata - Shrub, , . *Species includes - None recorded
	Mid Strata - Tree, , . *Species includes - None recorded
	Tall Strata - Tree, , . *Species includes - None Recorded
	Surface Coarse Fragments:
	Profile Morphology
	A1	0 - 0.02 m	Very dark grey (10YR3/1-Moist); Grey (10YR5/1-Dry); ; Fine sandy loam; Weak grade of structure, 
	<2 mm, Granular; Dry; Loose consistence; 10-20%, coarse gravelly, 20-60mm, Dolerite, coarse 
	fragments; ManyGradual change to - 
	A1A2	0.02 - 0.08 m	Very dark greyish brown (10YR3/2-Moist); Grey (10YR6/1-Dry); ; Fine sandy loam; Weak grade of 
	structure, <2 mm, Granular; Common (1-5 per 100mm2) Fine (1-2mm) macropores, Dry; Very 
	weak consistence; 2-10%, coarse gravelly, 20-60mm, Dolerite, coarse fragments; Common (10 -
	 20 %), Ferruginous, Fine (0 - 2 mm), ; CommonDiffuse change to - 
	A21	0.08 - 0.14 m	Greyish brown (10YR5/2-Moist); Light grey (10YR7/1-Dry); , 10YR42; Fine sandy loam; Massive 
	grade of structure; Common (1-5 per 100mm2) Fine (1-2mm) macropores, Dry; Very weak 
	consistence; Few (2 - 10 %), Ferruginous, Medium (2 -6 mm), ; FewDiffuse change to - 
	A22	0.14 - 0.23 m	Greyish brown (10YR5/2-Moist); Light grey (10YR7/2-Dry); ; Fine sandy loam; Massive grade of 
	structure; Common (1-5 per 100mm2) Fine (1-2mm) macropores, Dry; Weak consistence; 0-2%, 
	stony, 200-600mm, Dolerite, coarse fragments; Common (10 - 20 %), Ferruginous, Medium (2 -6 
	mm), ; Clear, Wavy change to - 
	AB	0.2 - 0.28 m	Greyish brown (10YR5/2-Moist); Light grey (10YR7/2-Dry); , 10YR53; Fine sandy clay loam; 
	Massive grade of structure; Common (1-5 per 100mm2) Fine (1-2mm) macropores, Dry; Strong 
	consistence; Common (10 - 20 %), Ferruginous, Medium (2 -6 mm), ; Clear, Wavy change to - 
	B21	0.28 - 0.41 m	Brown (10YR4/3-Moist); , 10YR52, 2-10% ; , 2-10% ; Heavy clay; Moderate grade of structure, 5-
	10 mm, Subangular blocky; Moderately moist; Very strong consistence; Common (10 - 20 %), 
	Ferruginous, Medium (2 -6 mm), ; Gradual change to - 
	B22	0.41 - 0.56 m	Dark greyish brown (2.5Y4/2-Moist); , 10YR58; Heavy clay; Moderate grade of structure, 10-20 
	mm, Subangular blocky; Fine, (0 - 5) mm crack; Moist; Very strong consistence; 2-10%, coarse 
	gravelly, 20-60mm, Dolerite, coarse fragments; Few (2 - 10 %), Ferruginous, , ; Gradual change 
	to - 
	BC	0.56 - 0.71 m	Greyish brown (2.5Y5/3-Moist); ; Heavy clay; Weak grade of structure, 10-20 mm, Subangular 
	blocky; Moist; Very firm consistence; 2-10%, coarse gravelly, 20-60mm, Dolerite, coarse 
	fragments; 

	Project Name:	DER
	Project Code:	DER	Site ID:	H233	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (TAS)
	C	0.71 - 0.81 m	Greyish brown (2.5Y5/3-Moist); ; Heavy clay; 10-20%, coarse gravelly, 20-60mm, Dolerite, coarse
	 fragments; 
	Morphological Notes
	Observation Notes
	2-56CM CONCENTRATION OF PISOLITIC FE IN HOLLOWS:41-81CM MANY W SPECKS:71-81CM GRAVELLY C + MEALY 
	W`D DR:                
	Site Notes
	BRIGHTON

	Project Name:	DER
	Project Code:	DER	Site ID:	H233	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (TAS)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.02	5.7A	 0.134A	 19.5H	 6	 0.57	 0.23	 14.2H	 48.9B
	 22.6E
	0.02 - 0.08	5.5A	 0.122A	 9.8H	 3.8	 0.32	 0.2	 9.5H	 28.8B
	 14.7E
	0.08 - 0.14	5.4A	 0.051A
	0.14 - 0.23	5.8A	 0.033A	 2.3H	 2.3	 0.13	 0.09	 2.5H	 8.6B
	 3.8E
	0.2 - 0.28	5.5A	 0.045A
	0.28 - 0.41	5.3A	 0.042A
	0.41 - 0.56	4.9A	 0.092A	 6.1H	 17.2	 0.11	 1.3	 9.3H	 38.6B
	 13.9E
	0.56 - 0.71	5A	 0.152A
	0.71 - 0.81	5A	 0.223A	 9.9H	 22.8	 0.17	 2.3	 7.1H	 46.7B
	 11.5E
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.02	 10.1D	 0.015D	 0.447A	 20	 3B	 39	 29	 13
	0.02 - 0.08	 4.82D	 0.006D	 0.192A	 8	 3B	 45	 29	 11
	0.08 - 0.14	 2.1D	 0.077A
	0.14 - 0.23	 0.74D	 0.04A	 13	 5D	 49	 36	 8
	0.2 - 0.28
	0.28 - 0.41
	0.41 - 0.56	 8	 3D	 21	 16	 58
	0.56 - 0.71
	0.71 - 0.81	 11	 27D	 25	 12	 33
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.02
	0.02 - 0.08
	0.08 - 0.14
	0.14 - 0.23
	0.2 - 0.28
	0.28 - 0.41
	0.41 - 0.56
	0.56 - 0.71
	0.71 - 0.81

	Project Name:	DER
	Project Code:	DER	Site ID:	H233	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (TAS)
	Laboratory Analyses Completed for this profile
	15E1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) by compulsive exchange, no pretreatment for soluble 
	15E1_K	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MG	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_NA	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15G_C_H1	Exchangeable hydrogen - meq per 100g of soil - Hydrogen By back titration of A or B
	15G1_H	Hydrogen Cation - meq per 100g of soil - 1M KCl Exch. Acidity By titration to pH 8.0
	15J_H	Sum of Ex. cations + Ex. acidity - Sum of basic exch. cations and exch. (Hydrogen)
	2_LOI	Loss on Ignition (%)
	2A1	Air-dry moisture content
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	5A2	Chloride - 1:5 soil/water extract, automated colour
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	7A2	Total nitrogen - semimicro Kjeldahl , automated colour
	9A_HCL	Total element - P(%) - By boiling HCl
	P10_GRAV	Gravel (%)
	P10_PB_C	Clay (%) - Plummet balance
	P10_PB_CS	Coarse sand (%) - Plummet balance
	P10_PB_FS	Fine sand (%) - Plummet balance
	P10_PB_Z	Silt (%) - Plummet balance
	P10A1_C	Clay (%) - Pipette
	P10A1_CS	Coarse sand (%) - Pipette
	P10A1_FS	Fine sand (%) - Pipette
	P10A1_Z	Silt (%) - Pipette