Project Name:	FLI
	Project Code:	FLI	Site ID:	H106	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (TAS)
	Site Information
	Desc. By:	G.M. Dimmock	Locality:	Near site 279:2CH west of Lady Barron-Sumer Camp 
	Track:2.75ML south west of Memanah:
	Date Desc.:	27/03/54	Elevation:	 82 metres
	Map Ref.:	Sheet No. : 8517   1:100000	Rainfall:	740
	Northing/Long.:	148.133333333333	Runoff:	Moderately rapid
	Easting/Lat.:	-40.0333333333333	Drainage:	No Data
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Granite 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	Hills
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Bench	Slope Category:	No Data
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Bleached-Mottled Dystrophic Grey Kurosol     	Principal Profile Form:	Dy5.41
	ASC Confidence:	Great Soil Group:	Yellow podzolic soil
	All necessary analytical data are available.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:
	Mid Strata - Heath shrub, 0.51-1m, . *Species includes - None recorded
	Tall Strata - Malle shrub, 1.01-3m, . *Species includes - None Recorded
	Surface Coarse Fragments:	10-20%, fine gravelly, 2-6mm, angular, Quartz
	Profile Morphology
	A1	0 - 0.05 m	Grey (10YR5/1-Moist); ; Loamy coarse sand; Single grain grade of structure; Moist; Firm 
	consistence; 2-10%, angular, Quartz, coarse fragments; Field pH 5 (pH meter); ManySharp, 
	Irregular change to - 
	A2	0.08 - 0.14 m	Light brownish grey (10YR6/2-Moist); ; Sand; Single grain grade of structure; Moderately moist; 
	Firm consistence; 20-50%, medium gravelly, 6-20mm, angular, Quartz, coarse fragments; 
	Irregular change to - 
	A2	0.14 - 0.2 m	Light brownish grey (10YR6/2-Moist); ; Sand; Single grain grade of structure; Moderately moist; 
	Very firm consistence; 20-50%, angular, Quartz, coarse fragments; Field pH 4.5 (pH meter); 
	B	0.23 - 0.33 m	Light brownish grey (10YR6/2-Moist); , 10YR52; , 10YR56; Light clay; Moderate grade of 
	structure, 50-100 mm, Prismatic; Moderately moist; Very firm consistence; 20-50%, coarse 
	gravelly, 20-60mm, angular, Quartz, coarse fragments; 
	B	0.33 - 0.48 m	Yellowish brown (10YR5/6-Moist); , 10YR62; , 10YR52; Light clay; Moderate grade of structure, 
	50-100 mm, Prismatic; Moderately moist; Firm consistence; 2-10%, angular, Quartz, coarse 
	fragments; Diffuse change to - 
	B	0.48 - 0.61 m	Yellowish brown (10YR5/6-Moist); , 10YR82; , 10YR62; Light clay; Weak grade of structure, 50-
	100 mm, Prismatic; Moderately moist; Very weak consistence; 10-20%, angular, Quartz, coarse 
	fragments; 
	B	0.61 - 0.74 m	Yellowish brown (10YR5/6-Moist); , 10YR82; , 10YR62; Light clay; Weak grade of structure, 50-
	100 mm, Prismatic; Moderately moist; Very weak consistence; 10-20%, angular, Quartz, coarse 
	fragments; 
	0.74 - 0.89 m	Brownish yellow (10YR6/6-Moist); , 10YR82; Light clay; Weak grade of structure, 50-100 mm, 
	Prismatic; Very weak consistence; 10-20%, angular, Quartz, coarse fragments; 
	1.52 - 1.6 m	White (10YR8/1-Moist); , 10YR72; , 10YR66; Light clay; Weak consistence; 20-50%, angular, 
	Quartz, coarse fragments; 
	Morphological Notes
	Observation Notes

	Project Name:	FLI
	Project Code:	FLI	Site ID:	H106	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (TAS)
	DISTRIBUTION OF GRAVEL THROUGHOUT CLAY HORIZON IS UNEVEN:                                                               
	Site Notes
	LACKRANA

	Project Name:	FLI
	Project Code:	FLI	Site ID:	H106	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (TAS)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.05	5A	 4.6H	 3	 0.25	 0.45	 17.4H	 32.6B
	 24.3E
	0.08 - 0.14	4.9A	 4.5C
	0.14 - 0.2	4.6A	 2.5C
	0.23 - 0.33	4.4A	 0.52H	 1	 0.14	 0.19	 10.6H	 17.7B
	 15.8E
	0.33 - 0.48	4.9A
	0.48 - 0.61	4.7A
	0.61 - 0.74	4.9A	 0.47H	 0.05	 0.1	 0.13	 11.3H	 22.8B
	 22E
	0.74 - 0.89	4.8A
	1.52 - 1.6	4.8A	 0.33H	 0.18	 0.06	 0.15	 4.4H	 7.9B
	 7.2E
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.05	 6.1D	 0.006D	 0.24A	 8	 34B	 37	 11	 8
	0.08 - 0.14	 1.5D	 0.061A
	0.14 - 0.2	 0.8D
	0.23 - 0.33	 1D	 30	 29D	 9	 10	 53
	0.33 - 0.48
	0.48 - 0.61
	0.61 - 0.74	 13	 13D	 5	 6	 71
	0.74 - 0.89
	1.52 - 1.6	 24	 29D	 10	 14	 46
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.05
	0.08 - 0.14
	0.14 - 0.2
	0.23 - 0.33
	0.33 - 0.48
	0.48 - 0.61
	0.61 - 0.74
	0.74 - 0.89
	1.52 - 1.6

	Project Name:	FLI
	Project Code:	FLI	Site ID:	H106	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (TAS)
	Laboratory Analyses Completed for this profile
	15D1_CEC	CEC - 1M ammonium acetate at pH 7.0, pretreatment for soluble salts; manual leach
	15E1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) by compulsive exchange, no pretreatment for soluble 
	15E1_K	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MG	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_NA	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15G_C_H1	Exchangeable hydrogen - meq per 100g of soil - Hydrogen By back titration of A or B
	15G1_H	Hydrogen Cation - meq per 100g of soil - 1M KCl Exch. Acidity By titration to pH 8.0
	15J_H	Sum of Ex. cations + Ex. acidity - Sum of basic exch. cations and exch. (Hydrogen)
	2_LOI	Loss on Ignition (%)
	2A1	Air-dry moisture content
	4A1	pH of 1:5 soil/water suspension
	5A2	Chloride - 1:5 soil/water extract, automated colour
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	7A2	Total nitrogen - semimicro Kjeldahl , automated colour
	9A_HCL	Total element - P(%) - By boiling HCl
	P10_GRAV	Gravel (%)
	P10_PB_C	Clay (%) - Plummet balance
	P10_PB_CS	Coarse sand (%) - Plummet balance
	P10_PB_FS	Fine sand (%) - Plummet balance
	P10_PB_Z	Silt (%) - Plummet balance
	P10A1_C	Clay (%) - Pipette
	P10A1_CS	Coarse sand (%) - Pipette
	P10A1_FS	Fine sand (%) - Pipette
	P10A1_Z	Silt (%) - Pipette