Project Name:	FLI
	Project Code:	FLI	Site ID:	H47	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (TAS)
	Site Information
	Desc. By:	G.M. Dimmock	Locality:	.4km NW of Loccota:
	Date Desc.:	11/12/52	Elevation:	 12 metres
	Map Ref.:	Sheet No. : 8517   1:100000	Rainfall:	760
	Northing/Long.:	148.05	Runoff:	Rapid
	Easting/Lat.:	-40.2	Drainage:	Rapidly drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Calcareous sand 
	Land Form
	Rel/Slope Class: 	Undulating plains <9m 3-10%	Pattern Type:	Dunefield
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	Dune	Slope Category:	No Data
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	No Available Class No Available Class Shelly Rudosol     	Principal Profile Form:	Uc1.11
	ASC Confidence:	Great Soil Group:	Calcareous sand
	All necessary analytical data are available.
	Site Disturbance:	Complete clearing. Pasture, native or improved, but never cultivated
	Vegetation:	Low Strata - Tussock grass, 0.26-0.5m, Mid-dense. *Species includes - None recorded
	Tall Strata - Shrub, 3.01-6m, Mid-dense. *Species includes - None Recorded
	Surface Coarse Fragments:
	Profile Morphology
	A	0 - 0.08 m	Very dark greyish brown (10YR3/2-Moist); ; Sand (Fibric); Single grain grade of structure; Dry; 
	Very weak consistence; Abundant, fine (1-2mm) roots; Diffuse change to - 
	A	0.08 - 0.15 m	Dark greyish brown (10YR4/2-Moist); ; Sand; Single grain grade of structure; Dry; Loose 
	consistence; CommonDiffuse change to - 
	AC	0.15 - 0.25 m	Greyish brown (10YR5/2-Moist); ; Sand; Single grain grade of structure; Dry; Loose consistence;
	 2-10%, fine gravelly, 2-6mm, Shells, coarse fragments; Diffuse change to - 
	C	0.25 - 0.36 m	Light brown (7.5YR6/4-Moist); ; Sand; Single grain grade of structure; Dry; Loose consistence; 
	2-10%, fine gravelly, 2-6mm, Shells, coarse fragments; Diffuse change to - 
	C	0.38 - 0.51 m	Light yellowish brown (10YR6/4-Moist); ; Sand; Single grain grade of structure; Moderately 
	moist; Loose consistence; 2-10%, fine gravelly, 2-6mm, Shells, coarse fragments; 
	CommonDiffuse change to - 
	C	0.61 - 0.76 m	Light yellowish brown (10YR6/4-Moist); ; Sand; Single grain grade of structure; Moist; Loose 
	consistence; 10-20%, fine gravelly, 2-6mm, Shells, coarse fragments; Diffuse change to - 
	C	1.04 - 1.19 m	Light yellowish brown (10YR6/4-Moist); ; Sand; Single grain grade of structure; Moist; Loose 
	consistence; 10-20%, fine gravelly, 2-6mm, Shells, coarse fragments; Diffuse change to - 
	1.47 - 1.57 m	Dark greyish brown (10YR4/2-Moist); ; Sand; Single grain grade of structure; Very weak 
	consistence; 2-10%, fine gravelly, 2-6mm, Shells, coarse fragments; Diffuse change to - 
	2.54 - 2.72 m	Light brownish grey (10YR6/2-Moist); , 10YR64; Sand; Single grain grade of structure; Loose 
	consistence; 10-20%, fine gravelly, 2-6mm, Shells, coarse fragments; 
	3.05 - 3.2 m	Light brown (7.5YR6/4-Moist); ; Sand; Single grain grade of structure; Loose consistence; 20-
	50%, fine gravelly, 2-6mm, Shells, coarse fragments; 
	Morphological Notes
	Observation Notes
	LUGHRATA SERIES:                                                                                                        
	Site Notes

	Project Name:	FLI
	Project Code:	FLI	Site ID:	H47	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (TAS)

	Project Name:	FLI
	Project Code:	FLI	Site ID:	H47	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (TAS)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.08	8.3A
	0.08 - 0.15	8.6A
	0.15 - 0.25	8.2A
	0.25 - 0.36	9A
	0.38 - 0.51	9A
	0.61 - 0.76	8.5A
	1.04 - 1.19	9.3A
	1.47 - 1.57	9.1A
	2.54 - 2.72	9A
	3.05 - 3.2	9.3A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.08	 57.6A	 4.59D	 0.02D	 0.408A	 0	 34B	 15	 2	 6
	0.08 - 0.15	 60A	 2.72D	 0.017D	 0.216A
	0.15 - 0.25	 65.6A	 0.97D	 0.077A
	0.25 - 0.36	 68.9A	 0.44D	 0.036A
	0.38 - 0.51	 72.5A	 0	 26B	 11	<1	 1
	0.61 - 0.76	 67.8A
	1.04 - 1.19	 68.8A
	1.47 - 1.57	 52.2A	 0	 19B	 29	<1	 2
	2.54 - 2.72	 59.8A
	3.05 - 3.2	 60.8A
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.08
	0.08 - 0.15
	0.15 - 0.25
	0.25 - 0.36
	0.38 - 0.51
	0.61 - 0.76
	1.04 - 1.19
	1.47 - 1.57
	2.54 - 2.72
	3.05 - 3.2

	Project Name:	FLI
	Project Code:	FLI	Site ID:	H47	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (TAS)
	Laboratory Analyses Completed for this profile
	19A1	Carbonates - rapid titration
	2_LOI	Loss on Ignition (%)
	2A1	Air-dry moisture content
	4A1	pH of 1:5 soil/water suspension
	5A2	Chloride - 1:5 soil/water extract, automated colour
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	7A2	Total nitrogen - semimicro Kjeldahl , automated colour
	9A_HCL	Total element - P(%) - By boiling HCl
	P10_GRAV	Gravel (%)
	P10A1_C	Clay (%) - Pipette
	P10A1_CS	Coarse sand (%) - Pipette
	P10A1_FS	Fine sand (%) - Pipette
	P10A1_Z	Silt (%) - Pipette