Project Name:	FLI
	Project Code:	FLI	Site ID:	H98	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (TAS)
	Site Information
	Desc. By:	G.M. Dimmock	Locality:	Approx 1.3km S along coast from Middle Inlet
	Date Desc.:	16/08/54	Elevation:	 8 metres
	Map Ref.:	Sheet No. : 8518   1:100000	Rainfall:	730
	Northing/Long.:	148.166666666667	Runoff:	Rapid
	Easting/Lat.:	-39.9333333333333	Drainage:	Rapidly drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Sand 
	Land Form
	Rel/Slope Class: 	Gently undulating plains <9m  	Pattern Type:	Dunefield
	1-3%
	Morph. Type:	Open depression (vale)	Relief:	No Data
	Elem. Type:	Swale	Slope Category:	Gently inclined
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:	Moderate (wind); 
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Parapanic Humic Semiaquic Podosol     	Principal Profile Form:	Uc4.33
	ASC Confidence:	Great Soil Group:	Podzol
	Analytical data are incomplete but reasonable confidence.
	Site Disturbance:	No effective disturbance. Natural
	Vegetation:	Low Strata - , , . *Species includes - None recorded
	Tall Strata - Tree, 3.01-6m, Mid-dense. *Species includes - None Recorded
	Surface Coarse Fragments:
	Profile Morphology
	A1	0 - 0.08 m	Dark greyish brown (10YR4/2-Moist); ; Sand (Fibric); Single grain grade of structure; Moderately 
	moist; Very weak consistence; AbundantDiffuse change to - 
	A1	0.08 - 0.2 m	Light brownish grey (10YR6/2-Moist); ; Sand (Fibric); Single grain grade of structure; Dry; Very 
	weak consistence; CommonDiffuse change to - 
	A2	0.2 - 0.33 m	Light brownish grey (10YR6/2-Moist); ; Sand; Single grain grade of structure; Dry; Loose 
	consistence; Sharp, Tongued change to - 
	BA2C	0.48 - 0.66 m	; Sand (Fibric); Organic pan, Weakly cemented, Continuous; 
	C	1.04 - 1.24 m	Very pale brown (10YR7/3-Moist); ; Sand; Single grain grade of structure; Moderately moist; 
	Loose consistence; 2-10%, fine gravelly, 2-6mm, Shells, coarse fragments; 
	C	1.24 - 1.47 m	Very pale brown (10YR7/3-Moist); ; Sand; Single grain grade of structure; Moist; Loose 
	consistence; 2-10%, fine gravelly, 2-6mm, Shells, coarse fragments; 
	C	3.45 - 3.61 m	Very pale brown (10YR7/3-Moist); ; Sand; Single grain grade of structure; Moist; Loose 
	consistence; 2-10%, medium gravelly, 6-20mm, Shells, coarse fragments; 
	Morphological Notes
	Observation Notes
	48-66CM MIXTURE OF CONVULUTING 4CM THICK WEAKLY CEMENTED COFFEE PAN(B)+LGB CALCAREOUS SAND(C) 
	AND VLbG SAND(A2):        LACKRANA SERIES:
	Site Notes
	MEMANA

	Project Name:	FLI
	Project Code:	FLI	Site ID:	H98	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (TAS)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.08	5.7A	 10.2H	 2.9	 0.12	 0.28	 8.6H	 24.9B
	 11.4E
	0.08 - 0.2	4.8A	 4C
	0.2 - 0.33	5.6A
	0.48 - 0.66	6.9A
	1.04 - 1.24	8.1A	 0.57H	 0.23	 0.13	 0.73	 1.66B
	1.24 - 1.47	8.5A
	3.45 - 3.61	8.5A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.08	 3.3D	 0.005D	 0.238A	 0	 69D	 32	 0	 1
	0.08 - 0.2	 0.9D	 0.07A
	0.2 - 0.33	 0.3D
	0.48 - 0.66
	1.04 - 1.24	 3.3A	 0	 58B	 36	 8	 0
	1.24 - 1.47	 3.3A
	3.45 - 3.61	 4.4A
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.08
	0.08 - 0.2
	0.2 - 0.33
	0.48 - 0.66
	1.04 - 1.24
	1.24 - 1.47
	3.45 - 3.61

	Project Name:	FLI
	Project Code:	FLI	Site ID:	H98	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (TAS)
	Laboratory Analyses Completed for this profile
	15D1_CEC	CEC - 1M ammonium acetate at pH 7.0, pretreatment for soluble salts; manual leach
	15E1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) by compulsive exchange, no pretreatment for soluble 
	15E1_K	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MG	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_NA	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15G_C_H1	Exchangeable hydrogen - meq per 100g of soil - Hydrogen By back titration of A or B
	15G1_H	Hydrogen Cation - meq per 100g of soil - 1M KCl Exch. Acidity By titration to pH 8.0
	15J_H	Sum of Ex. cations + Ex. acidity - Sum of basic exch. cations and exch. (Hydrogen)
	19A1	Carbonates - rapid titration
	2_LOI	Loss on Ignition (%)
	2A1	Air-dry moisture content
	4A1	pH of 1:5 soil/water suspension
	5A2	Chloride - 1:5 soil/water extract, automated colour
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	7A2	Total nitrogen - semimicro Kjeldahl , automated colour
	9A_HCL	Total element - P(%) - By boiling HCl
	P10_GRAV	Gravel (%)
	P10_PB_C	Clay (%) - Plummet balance
	P10_PB_CS	Coarse sand (%) - Plummet balance
	P10_PB_FS	Fine sand (%) - Plummet balance
	P10_PB_Z	Silt (%) - Plummet balance
	P10A1_C	Clay (%) - Pipette
	P10A1_CS	Coarse sand (%) - Pipette
	P10A1_FS	Fine sand (%) - Pipette
	P10A1_Z	Silt (%) - Pipette