Project Name:	HEL
	Project Code:	HEL	Site ID:	H116	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (TAS)
	Site Information
	Desc. By:	J. Loveday	Locality:	On 12% slope below top of narrow ridge 1.6KM south 
	west of Elliott:
	Date Desc.:	17/05/55	Elevation:	 250 metres
	Map Ref.:	Sheet No. : 8015   1:100000	Rainfall:	1140
	Northing/Long.:	145.763888888889	Runoff:	Very rapid
	Easting/Lat.:	-41.1083333333333	Drainage:	Well drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Basalt 
	Land Form
	Rel/Slope Class: 	Rolling low hills 30-90m 10-	Pattern Type:	Plateau
	Morph. Type:	Ridge	Relief:	76 metres
	Elem. Type:	Hillcrest	Slope Category:	Moderately inclined
	Slope:	12.3 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Acidic Mesotrophic Red Ferrosol     	Principal Profile Form:	Gn3.11
	ASC Confidence:	Great Soil Group:	Krasnozem
	All necessary analytical data are available.
	Site Disturbance:	Complete clearing. Pasture, native or improved, cultivated at some stage
	Vegetation:
	Surface Coarse Fragments:
	Profile Morphology
	0 - 0.08 m	Dark reddish brown (5YR3/3-Moist); ; Clay loam; Moderate grade of structure, 2-5 mm, 
	Subangular blocky; Weak consistence; 0-2%, Charcoal, coarse fragments; 
	0.08 - 0.15 m	Dark reddish brown (5YR3/3-Moist); ; Clay loam; Moderate grade of structure, 2-5 mm, 
	Subangular blocky; Weak consistence; 0-2%, Charcoal, coarse fragments; 
	0.15 - 0.23 m	Dark reddish brown (5YR3/3-Moist); ; Light clay; Moderate grade of structure, 5-10 mm, 
	Subangular blocky; Weak consistence; 0-2%, Charcoal, coarse fragments; 
	0.23 - 0.38 m	Reddish brown (5YR4/3-Moist); ; Heavy clay; Strong grade of structure, 10-20 mm, Angular 
	blocky; Strong grade of structure, <2 mm, Angular blocky; Weak consistence; Few (2 - 10 %), 
	Ferruginous, Fine (0 - 2 mm), Concretions; 
	0.38 - 0.53 m	Reddish brown (2.5YR4/4-Moist); ; Heavy clay; Strong grade of structure, 10-20 mm, Angular 
	blocky; Strong grade of structure, <2 mm, Angular blocky; Weak consistence; 
	0.53 - 0.69 m	Red (2.5YR4/6-Moist); ; Heavy clay; Strong grade of structure, 10-20 mm, Angular blocky; Strong 
	grade of structure, <2 mm, Angular blocky; Weak consistence; 
	0.69 - 0.84 m	Red (2.5YR4/6-Moist); ; Heavy clay; Moderate grade of structure, 2-5 mm, Subangular blocky; 
	Moderate grade of structure, <2 mm, Subangular blocky; Weak consistence; 
	0.84 - 0.99 m	Red (2.5YR4/6-Moist); ; Heavy clay; Moderate grade of structure, 2-5 mm, Subangular blocky; 
	Moderate grade of structure, <2 mm, Subangular blocky; Weak consistence; 
	0.99 - 1.22 m	Red (2.5YR4/6-Moist); ; Heavy clay; Moderate grade of structure, 2-5 mm, Subangular blocky; 
	Moderate grade of structure, <2 mm, Subangular blocky; Weak consistence; 
	1.52 - 1.78 m	Red (2.5YR4/8-Moist); ; Light clay (Light); Weak consistence; 
	2.24 - 2.54 m	Red (2.5YR5/8-Moist); ; Silty medium clay; Weak consistence; 
	3.51 - 3.76 m	Red (2.5YR5/8-Moist); ; Silty medium clay; 
	4.47 - 4.67 m	Red (2.5YR5/8-Moist); ; Silty medium clay; , Other, Coarse (6 - 20 mm), ; 
	Morphological Notes
	Observation Notes

	Project Name:	HEL
	Project Code:	HEL	Site ID:	H116	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (TAS)
	0-61CM WORMS ACTIVE:224-467CM BLACK INCLUSIONS INCREASING WITH DEPTH AND SIZE:WHITE FLECKING 
	OCCURRING:                 
	Site Notes
	WELLINGTON

	Project Name:	HEL
	Project Code:	HEL	Site ID:	H116	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (TAS)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.08	5.7A	 31.7C
	0.08 - 0.15	5.8A	 9.9H	 2.3	 0.32	 0.25	 15.7H	 47B
	 35E
	0.15 - 0.23	6A	 29.3C
	0.23 - 0.38	5.9A	 8H	 3	 0.19	 0.31	 9H	 34.8B
	 23.3E
	0.38 - 0.53	6A	 31.1C
	0.53 - 0.69	5.4A	 2.2H	 3.4	 0.5	 0.23	 13.9H	 31.9B
	 25.6E
	0.69 - 0.84	5.3A	 0.46H	 1.7	 1.2	 0.21	 27.1E	 30.7B
	0.84 - 0.99	5.3A
	0.99 - 1.22	5.3A
	1.52 - 1.78	4.8A	 0.16H	 1.8	 0.2	 0.24	 26.3E	 28.7B
	2.24 - 2.54	4.9A
	3.51 - 3.76	4.9A
	4.47 - 4.67	4.9A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.08	 6.4D	 0.134D	 0.499A
	0.08 - 0.15	 5D	 0.101D	 0.39A	 0	 2A	 6	 15	 67
	0.15 - 0.23	 3.4D	 0.263A
	0.23 - 0.38	 2.4D	 0.07D	 0.187A	 0	 1A	 6	 14	 76
	0.38 - 0.53	 1.8D
	0.53 - 0.69	 1D	 0.069D	 0.067A	 1	<1D	 4	 14	 79
	0.69 - 0.84
	0.84 - 0.99
	0.99 - 1.22
	1.52 - 1.78
	2.24 - 2.54
	3.51 - 3.76
	4.47 - 4.67
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.08
	0.08 - 0.15
	0.15 - 0.23
	0.23 - 0.38
	0.38 - 0.53
	0.53 - 0.69
	0.69 - 0.84
	0.84 - 0.99
	0.99 - 1.22
	1.52 - 1.78
	2.24 - 2.54
	3.51 - 3.76
	4.47 - 4.67

	Project Name:	HEL
	Project Code:	HEL	Site ID:	H116	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (TAS)

	Project Name:	HEL
	Project Code:	HEL	Site ID:	H116	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (TAS)
	Laboratory Analyses Completed for this profile
	12_HCL_FE	Total element - Fe(%) - Total acid(HCl) extractable Fe
	13C1_FE	Citrate/dithionite-extractable iron, aluminium, Manganese and Silicon
	15D1_CEC	CEC - 1M ammonium acetate at pH 7.0, pretreatment for soluble salts; manual leach
	15E1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) by compulsive exchange, no pretreatment for soluble 
	15E1_K	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MG	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_NA	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15G_C_H1	Exchangeable hydrogen - meq per 100g of soil - Hydrogen By back titration of A or B
	15G1_H	Hydrogen Cation - meq per 100g of soil - 1M KCl Exch. Acidity By titration to pH 8.0
	15J_H	Sum of Ex. cations + Ex. acidity - Sum of basic exch. cations and exch. (Hydrogen)
	2_LOI	Loss on Ignition (%)
	2A1	Air-dry moisture content
	4A1	pH of 1:5 soil/water suspension
	5A2	Chloride - 1:5 soil/water extract, automated colour
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	7A2	Total nitrogen - semimicro Kjeldahl , automated colour
	9A_HCL	Total element - P(%) - By boiling HCl
	P10_CF_C	Clay (%) - Coventry and Fett pipette method
	P10_CF_CS	Coarse sand (%) - Coventry and Fett pipette method
	P10_CF_FS	Fine sand (%) - Coventry and Fett pipette method
	P10_CF_Z	Silt (%) - Coventry and Fett pipette method
	P10_GRAV	Gravel (%)
	P10_PB_C	Clay (%) - Plummet balance
	P10_PB_CS	Coarse sand (%) - Plummet balance
	P10_PB_FS	Fine sand (%) - Plummet balance
	P10_PB_Z	Silt (%) - Plummet balance