Project Name:	HEL
	Project Code:	HEL	Site ID:	H141	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (TAS)
	Site Information
	Desc. By:	J. Loveday	Locality:	2KM north of Preolenna:
	Date Desc.:	22/03/56	Elevation:	 213 metres
	Map Ref.:	Sheet No. : 8015   1:100000	Rainfall:	1640
	Northing/Long.:	145.555555555556	Runoff:	Moderately rapid
	Easting/Lat.:	-41.0666666666667	Drainage:	Moderately well drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Soil pit, 1.1 m deep,Schist 
	Land Form
	Rel/Slope Class: 	Steep low hills 30-90m 32-56%	Pattern Type:	Low hills
	Morph. Type:	Upper-slope	Relief:	61 metres
	Elem. Type:	Hillslope	Slope Category:	Steep
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Self-mulching
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Acidic Mesotrophic Brown Kandosol     	Principal Profile Form:	Gn3.54
	ASC Confidence:	Great Soil Group:	Yellow podzolic soil
	All necessary analytical data are available.
	Site Disturbance:	Limited clearing, for example selective logging
	Vegetation:	Low Strata - Fern, 0.51-1m, Mid-dense. *Species includes - None recorded
	Tall Strata - Tree, , . *Species includes - Eucalyptus obliqua
	Surface Coarse Fragments:
	Profile Morphology
	O1	0.05 - 0.02 m	Organic Layer; ; ManyDiffuse change to - 
	O2	0.02 - 0 m	Organic Layer; Very dark greyish brown (10YR3/2-Moist); ; CommonDiffuse change to - 
	A1	0 - 0.05 m	Dark brown (7.5YR3/2-Moist); ; Fine sandy loam; Weak grade of structure, 5-10 mm, Subangular 
	blocky; Moist; Weak consistence; 10-20%, angular, Quartz, coarse fragments; CommonDiffuse 
	change to - 
	A2	0.05 - 0.1 m	Dark grey (10YR4/1-Moist); ; Fine sandy loam; Moist; Weak consistence; 10-20%, angular, 
	Quartz, coarse fragments; CommonDiffuse change to - 
	B1	0.18 - 0.25 m	Dark yellowish brown (10YR4/6-Moist); ; Sandy clay loam (Light); Weak grade of structure, 5-10 
	mm, Subangular blocky; Moist; Weak consistence; 10-20%, angular, Quartz, coarse fragments; 
	CommonDiffuse change to - 
	0.25 - 0.41 m	Dark yellowish brown (10YR4/6-Moist); ; Sandy clay loam (Light); Weak grade of structure, 5-10 
	mm, Subangular blocky; Weak consistence; 10-20%, angular, Quartz, coarse fragments; 
	FewDiffuse change to - 
	0.41 - 0.56 m	Yellowish brown (10YR5/7-Moist); ; Fine sandy medium clay; Massive grade of structure; Weak 
	consistence; 10-20%, angular, Quartz, coarse fragments; Diffuse change to - 
	0.64 - 0.76 m	Yellowish brown (10YR5/7-Moist); ; Silty medium clay; Massive grade of structure; Weak 
	consistence; Slightly plastic; Normal plasticity; 10-20%, angular, Quartz, coarse fragments; 
	BC	0.76 - 0.89 m	Yellowish brown (10YR5/7-Moist); ; Heavy clay; Moderately moist; Very firm consistence; 10-
	20%, angular, Quartz, coarse fragments; Sharp change to - 
	C	0.89 - 1.07 m	Yellowish brown (10YR5/6-Moist); , 2.5YR35; Moderately moist; Very strong consistence; 
	1.07 - 1.17 m	; 
	Morphological Notes
	On parent material (schists):
	Observation Notes
	0-46CM WORM ACTIVITY:94-112CM COMPACT DECOMPOSED SCHIST:23-94CM DECOMPOSED SCHIST FRACTION 

	Project Name:	HEL
	Project Code:	HEL	Site ID:	H141	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (TAS)
	Site Notes
	BURNIE

	Project Name:	HEL
	Project Code:	HEL	Site ID:	H141	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (TAS)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.05	4A
	0.05 - 0.1	4.3A	 1.3H	 0.58	 0.22	 0.14	 17.9H	 24.5E
	 22.3E
	0.1 - 0.15	4.3A
	0.23 - 0.3	4.5A	 0.1H	 0.65	 0.09	 0.11	 8.3H	 11.8E
	0.3 - 0.46	4.6A
	0.46 - 0.61	4.9A
	0.61 - 0.81	4.6A
	0.81 - 0.94	5A
	0.94 - 1.12	5A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.05	 0.02D
	0.05 - 0.1	 2.9D	 0.008D	 0.162A	 5	 8D	 62	 15	 12
	0.1 - 0.15	 1.5D	 0.08A
	0.23 - 0.3	 0.8D	 0.051A	 6	 10D	 61	 16	 15
	0.3 - 0.46
	0.46 - 0.61
	0.61 - 0.81
	0.81 - 0.94
	0.94 - 1.12
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.05
	0.05 - 0.1
	0.1 - 0.15
	0.23 - 0.3
	0.3 - 0.46
	0.46 - 0.61
	0.61 - 0.81
	0.81 - 0.94
	0.94 - 1.12

	Project Name:	HEL
	Project Code:	HEL	Site ID:	H141	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (TAS)
	Laboratory Analyses Completed for this profile
	15_NR	Sum of Ex. cations + Ex. acidity - Not recorded
	15E1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) by compulsive exchange, no pretreatment for soluble 
	15E1_K	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MG	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_NA	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15G_C_H1	Exchangeable hydrogen - meq per 100g of soil - Hydrogen By back titration of A or B
	15G1_H	Hydrogen Cation - meq per 100g of soil - 1M KCl Exch. Acidity By titration to pH 8.0
	2_LOI	Loss on Ignition (%)
	2A1	Air-dry moisture content
	4A1	pH of 1:5 soil/water suspension
	5A2	Chloride - 1:5 soil/water extract, automated colour
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	7A2	Total nitrogen - semimicro Kjeldahl , automated colour
	9A_HCL	Total element - P(%) - By boiling HCl
	P10_GRAV	Gravel (%)
	P10_PB_C	Clay (%) - Plummet balance
	P10_PB_CS	Coarse sand (%) - Plummet balance
	P10_PB_FS	Fine sand (%) - Plummet balance
	P10_PB_Z	Silt (%) - Plummet balance
	XRD_C_Hm	Hematite - X-Ray Diffraction
	XRD_C_Il	Illite - X-Ray Diffraction
	XRD_C_Ka	Kaolin - X-Ray Diffraction
	XRD_C_Qz	Quartz - X-Ray Diffraction
	XRD_C_Vm	Vermiculte - X-Ray Diffraction