Project Name:	HEL
	Project Code:	HEL	Site ID:	H144	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (TAS)
	Site Information
	Desc. By:	J. Loveday	Locality:	West Ridgley
	Date Desc.:	24/03/56	Elevation:	 244 metres
	Map Ref.:	Sheet No. : 8015   1:100000	Rainfall:	1140
	Northing/Long.:	145.775	Runoff:	Rapid
	Easting/Lat.:	-41.15	Drainage:	Moderately well drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Basalt 
	Land Form
	Rel/Slope Class: 	Undulating hills 90-300m 3-	Pattern Type:	Plateau
	Morph. Type:	No Data	Relief:	152 metres
	Elem. Type:	Hillslope	Slope Category:	Moderately inclined
	Slope:	15.8 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Melanic Eutrophic Brown Ferrosol     	Principal Profile Form:	Gn3.21
	ASC Confidence:	Great Soil Group:	Prairie soil
	All necessary analytical data are available.
	Site Disturbance:	Complete clearing. Pasture, native or improved, cultivated at some stage
	Vegetation:
	Surface Coarse Fragments:
	Profile Morphology
	A	0 - 0.08 m	Very dark brown (10YR2/2-Moist); ; Clay loam (Heavy); Strong grade of structure, <2 mm, 
	Subangular blocky; Moist; Weak consistence; Diffuse change to - 
	A	0.08 - 0.18 m	Very dark brown (10YR2/2-Moist); ; Clay loam (Heavy); Strong grade of structure, <2 mm, 
	Subangular blocky; Moist; Weak consistence; Clear change to - 
	B	0.22 - 0.33 m	Very dark greyish brown (2.5Y3/2-Moist); ; Medium clay; Strong grade of structure, 5-10 mm, 
	Subangular blocky; Moist; Weak consistence; 0-2%, fine gravelly, 2-6mm, angular, Quartz, 
	coarse fragments; Diffuse change to - 
	B	0.33 - 0.46 m	Dark greyish brown (2.5Y4/3-Moist); ; Medium clay; Moderate grade of structure, 5-10 mm, 
	Subangular blocky; Moist; Weak consistence; Diffuse change to - 
	B	0.46 - 0.61 m	Dark greyish brown (2.5Y4/3-Moist); ; Medium clay; Moderate grade of structure, 5-10 mm, 
	Subangular blocky; Moist; Weak consistence; Common (10 - 20 %), Unidentified, Medium (2 -6 
	mm), Soft segregations; Diffuse change to - 
	B	0.61 - 0.81 m	Dark greyish brown (2.5Y4/3-Moist); ; Medium clay; Moderate grade of structure, 5-10 mm, 
	Angular blocky; Moist; Weak consistence; 0-2%, stony, 200-600mm, Basalt, coarse fragments; 
	Common (10 - 20 %), Unidentified, Medium (2 -6 mm), Soft segregations; Diffuse change to - 
	B	0.81 - 0.99 m	Dark greyish brown (2.5Y4/3-Moist); ; Medium clay; Weak grade of structure, 5-10 mm, Angular 
	blocky; Moist; Weak consistence; Common (10 - 20 %), Unidentified, Medium (2 -6 mm), Soft 
	segregations; Diffuse change to - 
	C	1.04 - 1.24 m	Greyish brown (2.5Y5/3-Moist); , 10YR56; Moist; Weak consistence; 2-10%, Basalt, coarse 
	fragments; 
	1.68 - 1.83 m	Yellowish brown (10YR5/6-Moist); , 10YR76; Weak consistence; 
	Morphological Notes
	Observation Notes
	104-124CM AND 168-183CM ARE MEALY DECOMPOSED BA WITH A FEW POCKETS OF DYG CLAY:33-99CM BL STAINING
	 ON GV:               
	Site Notes
	BURNIE

	Project Name:	HEL
	Project Code:	HEL	Site ID:	H144	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (TAS)

	Project Name:	HEL
	Project Code:	HEL	Site ID:	H144	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (TAS)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.08	5.8A	 10.8H	 4	 1.3	 0.18	 10.5H	 39.5B
	 23.2E
	0.08 - 0.18	5.6A
	0.22 - 0.33	5.3A	 5.05H	 4.8	 0.82	 0.15	 8.6H	 30.4B
	 19.6E
	0.33 - 0.46	5A
	0.46 - 0.61	4.8A
	0.61 - 0.81	4.7A
	0.81 - 0.99	4.9A	 2.6H	 4.9	 0.1	 0.16	 13.4H	 28.8B
	 21E
	1.04 - 1.24	4.8A
	1.68 - 1.83	4.7A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.08	 3.4D	 0.08D	 0.314A	 2D	 16	 31	 37
	0.08 - 0.18	 2.7D	 0.062D	 0.228A
	0.22 - 0.33	 1.3D	 0.024D	 0.124A	 1D	 11	 32	 48
	0.33 - 0.46
	0.46 - 0.61	 0.6D
	0.61 - 0.81
	0.81 - 0.99	 0.016D	 5B	 11	 25	 58
	1.04 - 1.24
	1.68 - 1.83
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.08
	0.08 - 0.18
	0.22 - 0.33
	0.33 - 0.46
	0.46 - 0.61
	0.61 - 0.81
	0.81 - 0.99
	1.04 - 1.24
	1.68 - 1.83

	Project Name:	HEL
	Project Code:	HEL	Site ID:	H144	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (TAS)
	Laboratory Analyses Completed for this profile
	12_HCL_FE	Total element - Fe(%) - Total acid(HCl) extractable Fe
	13C1_FE	Citrate/dithionite-extractable iron, aluminium, Manganese and Silicon
	15E1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) by compulsive exchange, no pretreatment for soluble 
	15E1_K	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MG	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_NA	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15G_C_H1	Exchangeable hydrogen - meq per 100g of soil - Hydrogen By back titration of A or B
	15G1_H	Hydrogen Cation - meq per 100g of soil - 1M KCl Exch. Acidity By titration to pH 8.0
	15J_H	Sum of Ex. cations + Ex. acidity - Sum of basic exch. cations and exch. (Hydrogen)
	2_LOI	Loss on Ignition (%)
	2A1	Air-dry moisture content
	4A1	pH of 1:5 soil/water suspension
	5A2	Chloride - 1:5 soil/water extract, automated colour
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	7A2	Total nitrogen - semimicro Kjeldahl , automated colour
	9A_HCL	Total element - P(%) - By boiling HCl
	P10_PB_C	Clay (%) - Plummet balance
	P10_PB_CS	Coarse sand (%) - Plummet balance
	P10_PB_FS	Fine sand (%) - Plummet balance
	P10_PB_Z	Silt (%) - Plummet balance
	P10A1_C	Clay (%) - Pipette
	P10A1_CS	Coarse sand (%) - Pipette
	P10A1_FS	Fine sand (%) - Pipette
	P10A1_Z	Silt (%) - Pipette
	XRD_C_Ch2	Chloritized 2:1 minerals - X-Ray Diffraction
	XRD_C_Gt	Geothite - X-Ray Diffraction
	XRD_C_Ka	Kaolin - X-Ray Diffraction
	XRD_C_Qz	Quartz - X-Ray Diffraction