Project Name:	HEL
	Project Code:	HEL	Site ID:	H145	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (TAS)
	Site Information
	Desc. By:	J. Loveday	Locality:	2.4KM north west of Highclere:
	Date Desc.:	24/03/56	Elevation:	 274 metres
	Map Ref.:	Sheet No. : 8015   1:100000	Rainfall:	1550
	Northing/Long.:	145.775	Runoff:	Rapid
	Easting/Lat.:	-41.1847222222222	Drainage:	Well drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Auger boring, 1.9 m deep,Basalt 
	Land Form
	Rel/Slope Class: 	Undulating hills 90-300m 3-	Pattern Type:	Plateau
	Morph. Type:	Ridge	Relief:	152 metres
	Elem. Type:	Hillcrest	Slope Category:	Gently inclined
	Slope:	14 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Eutrophic Red Ferrosol     	Principal Profile Form:	Gn4.11
	ASC Confidence:	Great Soil Group:	Krasnozem
	All necessary analytical data are available.
	Site Disturbance:	Complete clearing. Pasture, native or improved, cultivated at some stage
	Vegetation:
	Surface Coarse Fragments:
	Profile Morphology
	A	0 - 0.06 m	Dark brown (7.5YR3/4-Moist); ; Clay loam; Strong grade of structure, <2 mm, Subangular blocky; 
	Moist; Weak consistence; 0-2%, coarse gravelly, 20-60mm, Basalt, coarse fragments; Diffuse 
	change to - 
	A	0.06 - 0.13 m	Dark brown (7.5YR3/4-Moist); ; Clay loam; Strong grade of structure, <2 mm, Subangular blocky; 
	Moist; Weak consistence; 0-2%, coarse gravelly, 20-60mm, Basalt, coarse fragments; Clear 
	change to - 
	B	0.14 - 0.23 m	Reddish brown (5YR4/4-Moist); ; Medium clay; Strong grade of structure, 2-5 mm, Subangular 
	blocky; Moist; Weak consistence; Diffuse change to - 
	B	0.23 - 0.33 m	Reddish brown (5YR4/4-Moist); ; Medium clay; Strong grade of structure, 10-20 mm, Subangular 
	blocky; Moist; Weak consistence; Diffuse change to - 
	B	0.33 - 0.46 m	Reddish brown (5YR4/4-Moist); ; Medium clay; Weak grade of structure, 20-50 mm, Subangular 
	blocky; Moist; Weak consistence; , Unidentified, Fine (0 - 2 mm), Concretions; Diffuse change 
	to - 
	B	0.46 - 0.61 m	Reddish brown (5YR4/4-Moist); ; Medium clay; Massive grade of structure; Moist; Weak 
	consistence; 0-2%, Gravel, coarse fragments; Diffuse change to - 
	B	0.61 - 0.76 m	Yellowish red (5YR4/6-Moist); ; Medium clay; Massive grade of structure; Moist; Weak 
	consistence; Diffuse change to - 
	BC	0.76 - 0.97 m	Yellowish red (5YR4/6-Moist); ; Medium clay; Massive grade of structure; Moist; Weak 
	consistence; Diffuse change to - 
	BC	0.97 - 1.17 m	Yellowish red (5YR4/6-Moist); ; Light clay; Moist; Weak consistence; 
	C	1.75 - 1.83 m	Reddish brown (5YR4/4-Moist); ; Light clay; 
	Morphological Notes
	Observation Notes
	76-117CM BL STAINS IN POCKETS OF DECOMPOSED BA (INCREASING DOWN):175-183CM W`D BA WITH BL STAINS 
	AND W INCLUSIONS:      
	Site Notes
	BURNIE

	Project Name:	HEL
	Project Code:	HEL	Site ID:	H145	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (TAS)

	Project Name:	HEL
	Project Code:	HEL	Site ID:	H145	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (TAS)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.06	5.1A	 9H	 2.1	 0.35	 0.14	 21H	 55.5B
	 43.9E
	0.06 - 0.13	5.2A
	0.14 - 0.23	5.6A	 7.1H	 4.15	 0.14	 0.14	 14H	 43.2B
	 31.7E
	0.23 - 0.33	5.5A
	0.33 - 0.46	5.2A
	0.46 - 0.61	4.9A
	0.61 - 0.76	4.8A	 1.9H	 2.5	 0.27	 0.22	 16.9H	 31.8B
	 26.9E
	0.76 - 0.97	4.5A
	0.97 - 1.17	4.8A	 1.4H	 1	 0.07	 0.49	 15H	 26B
	 23E
	1.75 - 1.83	4.6A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.06	 5.7D	 0.194D	 0.43A	 3D	 12	 34	 32
	0.06 - 0.13	 5.3D	 0.163D	 0.423A
	0.14 - 0.23	 3.4D	 0.105D	 0.281A	 1	 2D	 8	 15	 71
	0.23 - 0.33
	0.33 - 0.46	 1.7D
	0.46 - 0.61
	0.61 - 0.76	 0.11D	 1D	 10	 19	 67
	0.76 - 0.97
	0.97 - 1.17	 0.173D	 1B	 24	 28	 41
	1.75 - 1.83
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.06
	0.06 - 0.13
	0.14 - 0.23
	0.23 - 0.33
	0.33 - 0.46
	0.46 - 0.61
	0.61 - 0.76
	0.76 - 0.97
	0.97 - 1.17
	1.75 - 1.83

	Project Name:	HEL
	Project Code:	HEL	Site ID:	H145	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (TAS)
	Laboratory Analyses Completed for this profile
	12_HCL_FE	Total element - Fe(%) - Total acid(HCl) extractable Fe
	13C1_FE	Citrate/dithionite-extractable iron, aluminium, Manganese and Silicon
	15E1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) by compulsive exchange, no pretreatment for soluble 
	15E1_K	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MG	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_NA	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15G_C_H1	Exchangeable hydrogen - meq per 100g of soil - Hydrogen By back titration of A or B
	15G1_H	Hydrogen Cation - meq per 100g of soil - 1M KCl Exch. Acidity By titration to pH 8.0
	15J_H	Sum of Ex. cations + Ex. acidity - Sum of basic exch. cations and exch. (Hydrogen)
	2_LOI	Loss on Ignition (%)
	2A1	Air-dry moisture content
	4A1	pH of 1:5 soil/water suspension
	5A2	Chloride - 1:5 soil/water extract, automated colour
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	7A2	Total nitrogen - semimicro Kjeldahl , automated colour
	9A_HCL	Total element - P(%) - By boiling HCl
	P10_GRAV	Gravel (%)
	P10_PB_C	Clay (%) - Plummet balance
	P10_PB_CS	Coarse sand (%) - Plummet balance
	P10_PB_FS	Fine sand (%) - Plummet balance
	P10_PB_Z	Silt (%) - Plummet balance
	P10A1_C	Clay (%) - Pipette
	P10A1_CS	Coarse sand (%) - Pipette
	P10A1_FS	Fine sand (%) - Pipette
	P10A1_Z	Silt (%) - Pipette