Project Name:	HEL
	Project Code:	HEL	Site ID:	H147	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (TAS)
	Site Information
	Desc. By:	J. Loveday	Locality:	2KM south of Heybridge 4.8KM north of Cuprona:
	Date Desc.:	24/03/56	Elevation:	 152 metres
	Map Ref.:	Sheet No. : 8015   1:100000	Rainfall:	990
	Northing/Long.:	145.980555555556	Runoff:	Rapid
	Easting/Lat.:	-41.1	Drainage:	Well drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Basalt 
	Land Form
	Rel/Slope Class: 	Gently undulating rises 9-30m  	Pattern Type:	Plateau
	1-3%
	Morph. Type:	Simple-slope	Relief:	15 metres
	Elem. Type:	Hillslope	Slope Category:	Gently inclined
	Slope:	5.2 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Eutrophic Red Ferrosol     	Principal Profile Form:	Gn4.11
	ASC Confidence:	Great Soil Group:	Krasnozem
	All necessary analytical data are available.
	Site Disturbance:	Complete clearing. Pasture, native or improved, cultivated at some stage
	Vegetation:
	Surface Coarse Fragments:
	Profile Morphology
	A	0 - 0.08 m	Dark reddish brown (5YR3/4-Moist); ; Clay loam; Strong grade of structure, 2-5 mm, Subangular 
	blocky; Moist; Weak consistence; Diffuse change to - 
	A	0.08 - 0.18 m	Dark reddish brown (5YR3/4-Moist); ; Clay loam; Strong grade of structure, 2-5 mm, Subangular 
	blocky; Moist; Weak consistence; 0-2%, medium gravelly, 6-20mm, Basalt, coarse fragments; 
	Very few (0 - 2 %), Ferruginous, Medium (2 -6 mm), Concretions; Clear change to - 
	B	0.2 - 0.28 m	Yellowish red (5YR3/5-Moist); ; Medium clay; Strong grade of structure, 5-10 mm, Subangular 
	blocky; Moist; Weak consistence; 0-2%, medium gravelly, 6-20mm, Basalt, coarse fragments; 
	Very few (0 - 2 %), Ferruginous, Medium (2 -6 mm), Concretions; Diffuse change to - 
	B	0.28 - 0.36 m	Yellowish red (5YR3/5-Moist); ; Medium clay; Strong grade of structure, 5-10 mm, Subangular 
	blocky; Moist; Weak consistence; 0-2%, medium gravelly, 6-20mm, Basalt, coarse fragments; 
	Very few (0 - 2 %), Ferruginous, Medium (2 -6 mm), Concretions; Diffuse change to - 
	B	0.36 - 0.48 m	Dark red (2.5YR3/5-Moist); ; Medium clay; Moderate grade of structure, 10-20 mm, Subangular 
	blocky; Moist; Weak consistence; 0-2%, Basalt, coarse fragments; , Unidentified, Fine (0 - 2 
	mm), Concretions; Diffuse change to - 
	B	0.48 - 0.61 m	Dark red (2.5YR3/5-Moist); ; Medium clay; Moderate grade of structure, 10-20 mm, Subangular 
	blocky; Moist; Weak consistence; 2-10%, fine gravelly, 2-6mm, Basalt, coarse fragments; , 
	Unidentified, Fine (0 - 2 mm), Concretions; Diffuse change to - 
	B	0.61 - 0.76 m	Dark red (2.5YR3/6-Moist); ; Medium clay; Massive grade of structure; Moist; Weak consistence; 
	2-10%, fine gravelly, 2-6mm, Basalt, coarse fragments; Diffuse change to - 
	0.76 - 0.91 m	Dark red (2.5YR3/6-Moist); ; Medium clay; Massive grade of structure; Weak consistence; 2-10%,
	 fine gravelly, 2-6mm, Basalt, coarse fragments; Diffuse change to - 
	0.91 - 1.19 m	Dark red (2.5YR3/6-Moist); ; Medium clay; Massive grade of structure; Weak consistence; 2-10%,
	 fine gravelly, 2-6mm, Basalt, coarse fragments; 
	1.57 - 1.68 m	Yellowish red (5YR4/6-Moist); ; Light clay; 50-90%, Basalt, coarse fragments; 
	2.44 - 2.54 m	Yellowish brown (10YR5/6-Moist); , 5YR54; Very strong consistence; 50-90%, Basalt, coarse 
	fragments; 
	Morphological Notes

	Project Name:	HEL
	Project Code:	HEL	Site ID:	H147	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (TAS)
	Observation Notes
	244-254CM COMPACT DECOMPOSED BA WITH SOME CLAY:36-254CM BL STAINING ON BA GRAVELS:                                
	      
	Site Notes
	BURNIE

	Project Name:	HEL
	Project Code:	HEL	Site ID:	H147	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (TAS)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.08	5.5A	 10.9H	 1.4	 0.63	 0.21	 16.3H	 47.5B
	 34.4E
	0.08 - 0.18	5.6A
	0.2 - 0.28	5.9A	 9.35H	 1.2	 0.55	 0.13	 9.9H	 33.9B
	 22.7E
	0.28 - 0.36	6A
	0.36 - 0.48	6.1A
	0.48 - 0.61	6A
	0.61 - 0.76	6.1A	 5.2H	 1.6	 0.28	 0.13	 7.1H	 22.3B
	 15.1E
	0.76 - 0.91	6.3A
	0.91 - 1.19	6.4A
	1.57 - 1.68	5.2A
	2.44 - 1.54	4.8A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.08	 4.7D	 0.14D	 0.46A	 2B	 9	 14	 61
	0.08 - 0.18	 3.8D	 0.11D	 0.381A
	0.2 - 0.28	 2.6D	 0.08D	 0.244A	 1	 2B	 11	 14	 67
	0.28 - 0.36
	0.36 - 0.48	 1.8D	 0.189A
	0.48 - 0.61
	0.61 - 0.76	 0.6D	 0.056D	 1	 3D	 9	 13	 69
	0.76 - 0.91
	0.91 - 1.19
	1.57 - 1.68
	2.44 - 1.54
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.08
	0.08 - 0.18
	0.2 - 0.28
	0.28 - 0.36
	0.36 - 0.48
	0.48 - 0.61
	0.61 - 0.76
	0.76 - 0.91
	0.91 - 1.19
	1.57 - 1.68
	2.44 - 1.54

	Project Name:	HEL
	Project Code:	HEL	Site ID:	H147	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (TAS)
	Laboratory Analyses Completed for this profile
	12_HCL_FE	Total element - Fe(%) - Total acid(HCl) extractable Fe
	13C1_FE	Citrate/dithionite-extractable iron, aluminium, Manganese and Silicon
	15E1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) by compulsive exchange, no pretreatment for soluble 
	15E1_K	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MG	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_NA	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15G_C_H1	Exchangeable hydrogen - meq per 100g of soil - Hydrogen By back titration of A or B
	15G1_H	Hydrogen Cation - meq per 100g of soil - 1M KCl Exch. Acidity By titration to pH 8.0
	15J_H	Sum of Ex. cations + Ex. acidity - Sum of basic exch. cations and exch. (Hydrogen)
	2_LOI	Loss on Ignition (%)
	2A1	Air-dry moisture content
	4A1	pH of 1:5 soil/water suspension
	5A2	Chloride - 1:5 soil/water extract, automated colour
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	7A2	Total nitrogen - semimicro Kjeldahl , automated colour
	9A_HCL	Total element - P(%) - By boiling HCl
	P10_GRAV	Gravel (%)
	P10_PB_C	Clay (%) - Plummet balance
	P10_PB_CS	Coarse sand (%) - Plummet balance
	P10_PB_FS	Fine sand (%) - Plummet balance
	P10_PB_Z	Silt (%) - Plummet balance
	P10A1_C	Clay (%) - Pipette
	P10A1_CS	Coarse sand (%) - Pipette
	P10A1_FS	Fine sand (%) - Pipette
	P10A1_Z	Silt (%) - Pipette