Project Name:	LAR
	Project Code:	LAR	Site ID:	H18	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (TAS)
	Site Information
	Desc. By:	K.D. Nicholls	Locality:	Valleyfield:
	Date Desc.:	07/12/51	Elevation:	 168 metres
	Map Ref.:	Sheet No. : 8314   1:100000	Rainfall:	490
	Northing/Long.:	147.316666666667	Runoff:	Rapid
	Easting/Lat.:	-41.8166666666667	Drainage:	Well drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Sand 
	Land Form
	Rel/Slope Class: 	Undulating rises 9-30m 3-10%	Pattern Type:	Dunefield
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	Dune	Slope Category:	No Data
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:	Minor or present (wind); 
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Regolithic Bleached-Leptic Tenosol     	Principal Profile Form:	Uc4.31
	ASC Confidence:	Great Soil Group:	Siliceous sand
	All necessary analytical data are available.
	Site Disturbance:	Limited clearing, for example selective logging
	Vegetation:	Low Strata - , , . *Species includes - Lomandra longifolia
	Tall Strata - Tree, 3.01-6m, Mid-dense. *Species includes - Banksia marginata, Bursaria spinosa
	Surface Coarse Fragments:
	Profile Morphology
	A1	0 - 0.05 m	Greyish brown (10YR5/2-Moist); ; Sand; Massive grade of structure; Very weak consistence; 
	Diffuse change to - 
	0.05 - 0.13 m	Greyish brown (10YR5/2-Moist); ; Sand; Massive grade of structure; Loose consistence; Diffuse 
	change to - 
	0.13 - 0.43 m	Brownish yellow (10YR6/5-Moist); ; Sand; Massive grade of structure; Loose consistence; 
	Diffuse change to - 
	0.43 - 0.71 m	Light yellowish brown (10YR6/4-Moist); ; Sand; Massive grade of structure; Loose consistence; 
	Diffuse change to - 
	0.71 - 1.09 m	Light yellowish brown (10YR6/4-Moist); ; Sand; Massive grade of structure; Loose consistence; 
	Diffuse change to - 
	1.19 - 1.4 m	Pale brown (10YR6/3-Moist); ; Sand; Firm consistence; 
	1.73 - 1.85 m	Olive grey (5Y5/2-Moist); , 5Y71; , 10YR56; Heavy clay; Strong consistence; 
	2.92 - 3.05 m	Olive grey (5Y5/2-Moist); , 5Y62; Sandy medium clay; Few (2 - 10 %), Ferruginous, , ; 
	Morphological Notes
	Observation Notes
	109-119CM SLIGHT IRREGULAR FE DEPOSITIONAL LAYER:PONSHANGER SERIES.                                                     
	Site Notes
	SOMERSET

	Project Name:	LAR
	Project Code:	LAR	Site ID:	H18	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (TAS)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.05	6A	 2H	 0.39	 0.08	 0.05	 2.1H	 5.2B
	 2.7E
	0.05 - 0.13	5.4A	 0.7H	 0.2	 0.05	 0.05	 0.6H	 2B
	 1E
	0.13 - 0.43	5.5A
	0.43 - 0.71	5.7A
	0.71 - 1.09	6A
	1.19 - 1.4	6.1A
	1.73 - 1.85	5.6A	 0.42H	 8.4	 0.17	 2.3	 7.6H	 22B
	 10.8E
	2.92 - 3.05	5.6A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.05	 0.8D	 0.006D	 0.07A	 0	 32D	 63	 4	 5
	0.05 - 0.13	 0.3D	 0.003D	 0.04A	 0	 24B	 73	 1	 2
	0.13 - 0.43	 0.1D	 0.013A
	0.43 - 0.71
	0.71 - 1.09
	1.19 - 1.4	 0	 17B	 77	 3	 2
	1.73 - 1.85	 0.002D	 0	 14B	 44	 3	 39
	2.92 - 3.05
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.05
	0.05 - 0.13
	0.13 - 0.43
	0.43 - 0.71
	0.71 - 1.09
	1.19 - 1.4
	1.73 - 1.85
	2.92 - 3.05

	Project Name:	LAR
	Project Code:	LAR	Site ID:	H18	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (TAS)
	Laboratory Analyses Completed for this profile
	12_HCL_FE	Total element - Fe(%) - Total acid(HCl) extractable Fe
	13C1_FE	Citrate/dithionite-extractable iron, aluminium, Manganese and Silicon
	15E1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) by compulsive exchange, no pretreatment for soluble 
	15E1_K	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MG	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_NA	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15G_C_H1	Exchangeable hydrogen - meq per 100g of soil - Hydrogen By back titration of A or B
	15G1_H	Hydrogen Cation - meq per 100g of soil - 1M KCl Exch. Acidity By titration to pH 8.0
	15J_H	Sum of Ex. cations + Ex. acidity - Sum of basic exch. cations and exch. (Hydrogen)
	2_LOI	Loss on Ignition (%)
	2A1	Air-dry moisture content
	4A1	pH of 1:5 soil/water suspension
	5A2	Chloride - 1:5 soil/water extract, automated colour
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	7A2	Total nitrogen - semimicro Kjeldahl , automated colour
	9A_HCL	Total element - P(%) - By boiling HCl
	P10_GRAV	Gravel (%)
	P10_PB_C	Clay (%) - Plummet balance
	P10_PB_CS	Coarse sand (%) - Plummet balance
	P10_PB_FS	Fine sand (%) - Plummet balance
	P10_PB_Z	Silt (%) - Plummet balance
	P10A1_C	Clay (%) - Pipette
	P10A1_CS	Coarse sand (%) - Pipette
	P10A1_FS	Fine sand (%) - Pipette
	P10A1_Z	Silt (%) - Pipette