Project Name:	LON
	Project Code:	LON	Site ID:	H17	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (TAS)
	Site Information
	Desc. By:	K.D. Nicholls	Locality:	8.1km NW of Longford:
	Date Desc.:	06/12/51	Elevation:	 158 metres
	Map Ref.:	Sheet No. : 8314   1:100000	Rainfall:	700
	Northing/Long.:	147.066666666667	Runoff:	Slow
	Easting/Lat.:	-41.5333333333333	Drainage:	Imperfectly drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Unconsolidated material (unidentified) 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	No Data
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	No Data	Slope Category:	No Data
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Mesotrophic Mottled-Subnatric Yellow Sodosol     	Principal Profile Form:	Dy5.41
	ASC Confidence:	Great Soil Group:	Lateritic podzolic 
	All necessary analytical data are available.	soil
	Site Disturbance:	No effective disturbance. Natural
	Vegetation:	Low Strata - Fern, 0.26-0.5m, Closed or dense. *Species includes - Pteridium esculentum, Lomandra longifolia
	Tall Strata - Tree, 20.01-35m, Mid-dense. *Species includes - None Recorded
	Surface Coarse Fragments:
	Profile Morphology
	A1	0 - 0.05 m	Light grey (10YR7/1-Dry); ; Loamy sand; Massive grade of structure; Weak consistence; 0-2%, 
	Gravel, coarse fragments; Sharp, Irregular change to - 
	A1A2	0.05 - 0.1 m	Light grey (10YR7/2-Moist); ; Sand; Massive grade of structure; Weak consistence; 0-2%, Gravel,
	 coarse fragments; 
	A2	0.1 - 0.2 m	Very pale brown (10YR7/3-Moist); ; Sand; Massive grade of structure; Firm consistence; 0-2%, 
	Gravel, coarse fragments; Sharp change to - 
	A2	0.2 - 0.36 m	Light grey (10YR7/2-Dry); ; Sand; Massive grade of structure; Weak consistence; 10-20%, 
	coarse gravelly, 20-60mm, rounded, Quartz, coarse fragments; Sharp, Irregular change to - 
	B1	0.36 - 0.51 m	Brownish yellow (10YR6/6-Moist); , 7.5YR58; Heavy clay; , Columnar; Weak consistence; 
	Diffuse change to - 
	B	0.51 - 0.76 m	Brownish yellow (10YR6/6-Moist); , 7.5YR58; , 5YR44; Heavy clay; , Columnar; Weak 
	consistence; Few (2 - 10 %), Ferruginous, , Soft segregations; 
	B	0.76 - 0.99 m	Brownish yellow (10YR6/6-Moist); , 7.5YR58; , 5YR44; Heavy clay; Weak consistence; Few (2 - 
	10 %), Ferruginous, , Soft segregations; 
	C	1.52 - 1.68 m	Yellowish brown (10YR5/6-Moist); , 10YR71; , 2.5YR48; Sandy medium clay; Weak 
	C	2.79 - 2.9 m	Yellowish brown (10YR5/6-Moist); , 2.5YR48; , 10YR81; Sandy medium clay; Weak 
	consistence; 2-10%, coarse gravelly, 20-60mm, rounded, Quartz, coarse fragments; 
	Morphological Notes
	Observation Notes
	>290CM ON QZ GRAVEL:152-168CM SC WITH POCKETS OF CLAY:20-36CM <10%BLACKSPECKS:BRICKENDON SERIES.  
	                      
	Site Notes
	WESTMORLAND

	Project Name:	LON
	Project Code:	LON	Site ID:	H17	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (TAS)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.05	5.6A	 2.8H	 0.54	 0.13	 0.14	 4.1H	 10.1B
	 6.5E
	0.05 - 0.1	5.6A
	0.1 - 0.2	5.7A
	0.2 - 0.36	5.6A
	0.36 - 0.51	5.9A	 2H	 5.1	 0.18	 0.61	 3.6H	 16.4B
	 8.3E
	0.51 - 0.76	6.1A
	0.76 - 0.99	5.7A
	1.52 - 1.68	4.9A	 0.3H	 0.71	 0.04	 0.29	 3.9H	 6.7B
	 5.4E
	2.79 - 2.9	4A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.05	 1.3D	 0.004D	 0.07A	 1	 36B	 48	 8	 3
	0.05 - 0.1	 0.4D	 0.02A
	0.1 - 0.2	 0.1D	 0.002D	 0.014A
	0.2 - 0.36
	0.36 - 0.51	 0.005D	 11D	 10	 4	 73
	0.51 - 0.76
	0.76 - 0.99
	1.52 - 1.68	 0.002D	 42D	 15	 9	 37
	2.79 - 2.9
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.05
	0.05 - 0.1
	0.1 - 0.2
	0.2 - 0.36
	0.36 - 0.51
	0.51 - 0.76
	0.76 - 0.99
	1.52 - 1.68
	2.79 - 2.9

	Project Name:	LON
	Project Code:	LON	Site ID:	H17	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (TAS)
	Laboratory Analyses Completed for this profile
	15E1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) by compulsive exchange, no pretreatment for soluble 
	15E1_K	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MG	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_NA	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15G_C_H1	Exchangeable hydrogen - meq per 100g of soil - Hydrogen By back titration of A or B
	15G1_H	Hydrogen Cation - meq per 100g of soil - 1M KCl Exch. Acidity By titration to pH 8.0
	15J_H	Sum of Ex. cations + Ex. acidity - Sum of basic exch. cations and exch. (Hydrogen)
	2_LOI	Loss on Ignition (%)
	2A1	Air-dry moisture content
	4A1	pH of 1:5 soil/water suspension
	5A2	Chloride - 1:5 soil/water extract, automated colour
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	7A2	Total nitrogen - semimicro Kjeldahl , automated colour
	9A_HCL	Total element - P(%) - By boiling HCl
	P10_GRAV	Gravel (%)
	P10_PB_C	Clay (%) - Plummet balance
	P10_PB_CS	Coarse sand (%) - Plummet balance
	P10_PB_FS	Fine sand (%) - Plummet balance
	P10_PB_Z	Silt (%) - Plummet balance
	P10A1_C	Clay (%) - Pipette
	P10A1_CS	Coarse sand (%) - Pipette
	P10A1_FS	Fine sand (%) - Pipette
	P10A1_Z	Silt (%) - Pipette
	XRD_C_Ch2	Chloritized 2:1 minerals - X-Ray Diffraction
	XRD_C_Ka	Kaolin - X-Ray Diffraction
	XRD_C_Qz	Quartz - X-Ray Diffraction