Project Name:	LON
	Project Code:	LON	Site ID:	H24	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (TAS)
	Site Information
	Desc. By:	J.K. Taylor	Locality:	3.2km S of Carrick:
	Date Desc.:	21/01/52	Elevation:	 171 metres
	Map Ref.:	Sheet No. : 8313   1:100000	Rainfall:	700
	Northing/Long.:	147	Runoff:	Moderately rapid
	Easting/Lat.:	-41.5666666666667	Drainage:	Imperfectly drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Dolerite 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	No Data
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	No Data	Slope Category:	No Data
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Ferric Eutrophic Black Chromosol     	Principal Profile Form:	Db1.22
	ASC Confidence:	Great Soil Group:	Grey-brown 
	All necessary analytical data are available.	podzolic soil
	Site Disturbance:	Limited clearing, for example selective logging
	Vegetation:	Low Strata - Tussock grass, , . *Species includes - Danthonia species
	Tall Strata - Tree, 6.01-12m, Very sparse. *Species includes - Eucalyptus pauciflora, Eucalyptus ovata
	Surface Coarse Fragments:	2-10%, , , Dolerite
	Profile Morphology
	A1	0 - 0.08 m	Greyish brown (10YR5/2-Dry); ; Fine sandy loam; Moist; 0-2%, Gravel, coarse fragments; Diffuse 
	change to - 
	A1A2	0.08 - 0.18 m	Grey (10YR5/1-Moist); ; Fine sandy loam; 0-2%, Dolerite, coarse fragments; Very few (0 - 2 %), 
	Ferruginous, , ; Diffuse change to - 
	A2	0.18 - 0.25 m	Light brownish grey (10YR6/2-Moist); ; Fine sandy loam; 20-50%, Gravel, coarse fragments; 
	Diffuse change to - 
	A2B	0.25 - 0.36 m	Grey (10YR5/1-Moist); , 10YR52; Fine sandy loam (Heavy); 2-10%, medium gravelly, 6-20mm, 
	Dolerite, coarse fragments; Many (20 - 50 %), Ferruginous, Fine (0 - 2 mm), ; Sharp change to - 
	B	0.36 - 0.41 m	Dark olive grey (5Y3/2-Moist); , 10YR52; , 2.5YR48; Light clay; Massive grade of structure; 2-
	10%, Gravel, coarse fragments; Common (10 - 20 %), Ferruginous, , ; Sharp change to - 
	0.41 - 0.71 m	Dark olive grey (5Y3/2-Moist); , 2.5YR48; Heavy clay; Very firm consistence; 2-10%, Dolerite, 
	coarse fragments; Very few (0 - 2 %), Ferruginous, , ; Diffuse change to - 
	0.74 - 0.81 m	Dark olive grey (5Y3/2-Moist); , 10YR56; Heavy clay; 0-2%, Dolerite, coarse fragments; Common
	Morphological Notes
	Observation Notes
	SAMPLE 7 TAKEN FROM BETWEEN BOULDERS:>81CM ON A DOLERITE BOULDER:EASTFIELD SERIES:                           
	           
	Site Notes
	WESTMORLAND

	Project Name:	LON
	Project Code:	LON	Site ID:	H24	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (TAS)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.08	6.1A	 7.6H	 2.5	 0.49	 0.19	 7H	 23.6B
	 12.8E
	0.08 - 0.18	6.7A
	0.18 - 0.25	7.1A	 3.7H	 1.5	 0.1	 0.19	 4.3E	 9.8B
	0.25 - 0.36	7.1A
	0.36 - 0.41	7A	 8.6H	 7.9	 0.17	 0.48	 6.7E	 23.9B
	0.41 - 0.71	7.2A	 11.3H	 13	 0.17	 0.76	 7.9E	 32.8B
	0.74 - 0.81	7.1A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.08	 3.4D	 0.013D	 0.304A	 1	 10B	 41	 28	 16
	0.08 - 0.18	 1.01D	 0.007D	 0.1A
	0.18 - 0.25	 0.61D	 0.063A	 30	 13B	 43	 26	 16
	0.25 - 0.36	 0.61D	 0.065A
	0.36 - 0.41	 0.6D	 0.074A	 26	 8D	 23	 17	 49
	0.41 - 0.71	 0.84D	 0.008D	 0.068A	 12	 7B	 14	 9	 69
	0.74 - 0.81
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.08
	0.08 - 0.18
	0.18 - 0.25
	0.25 - 0.36
	0.36 - 0.41
	0.41 - 0.71
	0.74 - 0.81

	Project Name:	LON
	Project Code:	LON	Site ID:	H24	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (TAS)
	Laboratory Analyses Completed for this profile
	15E1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) by compulsive exchange, no pretreatment for soluble 
	15E1_K	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MG	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_NA	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15G_C_H1	Exchangeable hydrogen - meq per 100g of soil - Hydrogen By back titration of A or B
	15G1_H	Hydrogen Cation - meq per 100g of soil - 1M KCl Exch. Acidity By titration to pH 8.0
	15J_H	Sum of Ex. cations + Ex. acidity - Sum of basic exch. cations and exch. (Hydrogen)
	2_LOI	Loss on Ignition (%)
	2A1	Air-dry moisture content
	4A1	pH of 1:5 soil/water suspension
	5A2	Chloride - 1:5 soil/water extract, automated colour
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	7A2	Total nitrogen - semimicro Kjeldahl , automated colour
	9A_HCL	Total element - P(%) - By boiling HCl
	P10_GRAV	Gravel (%)
	P10_PB_C	Clay (%) - Plummet balance
	P10_PB_CS	Coarse sand (%) - Plummet balance
	P10_PB_FS	Fine sand (%) - Plummet balance
	P10_PB_Z	Silt (%) - Plummet balance
	P10A1_C	Clay (%) - Pipette
	P10A1_CS	Coarse sand (%) - Pipette
	P10A1_FS	Fine sand (%) - Pipette
	P10A1_Z	Silt (%) - Pipette
	XRD_C_Ch2	Chloritized 2:1 minerals - X-Ray Diffraction
	XRD_C_Hm	Hematite - X-Ray Diffraction
	XRD_C_Ka	Kaolin - X-Ray Diffraction
	XRD_C_Qz	Quartz - X-Ray Diffraction
	XRD_C_St	Smectite - X-Ray Diffraction