Project Name:	MEA
	Project Code:	MEA	Site ID:	H110	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (TAS)
	Site Information
	Desc. By:	K.D. Nicholls	Locality:	100m from north end of Pine Lake:
	Date Desc.:	26/11/54	Elevation:	 1189 metres
	Map Ref.:	Rainfall:	813
	Northing/Long.:	146.7	Runoff:	No runoff
	Easting/Lat.:	-42.7575	Drainage:	Very poorly drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Soil pit, 0.4 m deep,Dolerite 
	Land Form
	Rel/Slope Class: 	Level plain <9m <1%	Pattern Type:	Plateau
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Cliff-foot slope	Slope Category:	Very gently sloped
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	No Available Class Acidic Fibric Organosol     	Principal Profile Form:	O
	ASC Confidence:	Great Soil Group:	Acid peat
	All necessary analytical data are available.
	Site Disturbance:	No effective disturbance. Natural
	Vegetation:
	Surface Coarse Fragments:
	Profile Morphology
	0 - 0.1 m	Very dark brown (10YR2/2-Moist); ; Massive grade of structure; AbundantDiffuse change to - 
	0.1 - 0.25 m	Black (10YR2/1-Moist); ; Massive grade of structure; 
	0.25 - 0.36 m	Black (10YR2/1-Moist); ; Loam (Fibric); Massive grade of structure; 
	Morphological Notes
	Observation Notes
	AT 36CM FLOOR OF DOLERITE BOULDERS:                                                                                     
	Site Notes
	QUAMBY

	Project Name:	MEA
	Project Code:	MEA	Site ID:	H110	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (TAS)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	4.5A	 71C
	0.1 - 0.25	4.7A	 0.4H	 2.7	 0.41	 0.18	 129H
	0.25 - 0.36	5A	 56C
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1	 35.9D
	0.1 - 0.25	 29.7D	 0.076D	 1.42A	<1B	 6	 21	 30
	0.25 - 0.36	 16.8D
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.1
	0.1 - 0.25
	0.25 - 0.36

	Project Name:	MEA
	Project Code:	MEA	Site ID:	H110	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (TAS)
	Laboratory Analyses Completed for this profile
	15D1_CEC	CEC - 1M ammonium acetate at pH 7.0, pretreatment for soluble salts; manual leach
	15E1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) by compulsive exchange, no pretreatment for soluble 
	15E1_K	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MG	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_NA	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15G_C_H1	Exchangeable hydrogen - meq per 100g of soil - Hydrogen By back titration of A or B
	2_LOI	Loss on Ignition (%)
	2A1	Air-dry moisture content
	4A1	pH of 1:5 soil/water suspension
	5A2	Chloride - 1:5 soil/water extract, automated colour
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	7A2	Total nitrogen - semimicro Kjeldahl , automated colour
	9A_HCL	Total element - P(%) - By boiling HCl
	P10A1_C	Clay (%) - Pipette
	P10A1_CS	Coarse sand (%) - Pipette
	P10A1_FS	Fine sand (%) - Pipette
	P10A1_Z	Silt (%) - Pipette