Project Name:	PAT
	Project Code:	PAT	Site ID:	H248	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (TAS)
	Site Information
	Desc. By:	G.M. Dimmock	Locality:	.8KM NNE of Legana:
	Date Desc.:	23/04/63	Elevation:	 38 metres
	Map Ref.:	Rainfall:	780
	Northing/Long.:	147.381944444444	Runoff:	Moderately rapid
	Easting/Lat.:	-41.3638888888889	Drainage:	Poorly drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Auger boring, 2.3 m deep,Unconsolidated 
	material (unidentified) 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	Terrace (alluvial)
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	No Data	Slope Category:	Gently inclined
	Slope:	3.5 % 	Aspect:	45 degrees
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Ferric Mesotrophic Brown Chromosol     	Principal Profile Form:	Dy5.61
	ASC Confidence:	Great Soil Group:	Lateritic podzolic 
	All necessary analytical data are available.	soil
	Site Disturbance:	Limited clearing, for example selective logging
	Vegetation:	Low Strata - Fern, , . *Species includes - None recorded
	Tall Strata - Tree, , . *Species includes - None Recorded
	Surface Coarse Fragments:
	Profile Morphology
	A	0 - 0.025 m	Very dark grey (10YR3/1-Moist); ; Loamy sand; Massive grade of structure; Dry; Very weak 
	consistence; 0-2%, fine gravelly, 2-6mm, subangular, Quartz, coarse fragments; Common (10 - 
	20 %), Ferruginous, Coarse (6 - 20 mm), Nodules; Many, coarse (>5mm) roots; Clear, Irregular 
	change to - 
	A1A2	0.025 - 0.09 m	Very dark grey (10YR3/1-Moist); ; Loamy sand; Massive grade of structure; Dry; Very weak 
	consistence; 2-10%, medium gravelly, 6-20mm, rounded, Quartz, coarse fragments; Common 
	(10 - 20 %), Ferruginous, Very coarse (20 - 60 mm), Nodules; Many, coarse (>5mm) roots; 
	Diffuse change to - 
	A21	0.09 - 0.18 m	Brown (10YR5/3-Moist); ; Loamy sand; Massive grade of structure; Dry; Loose consistence; 2-
	10%, medium gravelly, 6-20mm, rounded, Quartz, coarse fragments; Very many (50 - 100 %), 
	Ferruginous, Very coarse (20 - 60 mm), Nodules; Many, coarse (>5mm) roots; Diffuse change to 
	- 
	A22	0.23 - 0.36 m	Brown (10YR5/3-Moist); ; Loamy sand (Heavy); Massive grade of structure; Moderately moist; 
	Weak consistence; 2-10%, medium gravelly, 6-20mm, rounded, Quartz, coarse fragments; Very 
	many (50 - 100 %), Ferruginous, Very coarse (20 - 60 mm), Nodules; Abundant, coarse (>5mm) 
	roots; Abrupt, Wavy change to - 
	B21	0.42 - 0.56 m	Yellowish brown (10YR5/6-Moist); , 2.5YR48; Heavy clay; Weak grade of structure, 20-50 mm, 
	Angular blocky; Moderately moist; Strong consistence; Very few (0 - 2 %), Ferruginous, 
	Extremely coarse (> 60 mm), Nodules; 
	B22	0.56 - 0.71 m	Yellowish brown (10YR5/4-Moist); , 2.5YR48; , 2.5Y71; Heavy clay; Massive grade of structure; 
	Moderately moist; Weak consistence; Very few (0 - 2 %), Ferruginous, Very coarse (20 - 60 mm), 
	Nodules; 
	B2	0.71 - 0.86 m	Yellowish brown (10YR5/4-Moist); , 2.5Y54; , 7.5YR56; Heavy clay; Massive grade of structure; 
	Moderately moist; Weak consistence; Very few (0 - 2 %), Ferruginous, Very coarse (20 - 60 mm), 
	Nodules; 
	B24	0.86 - 1.07 m	Yellowish brown (10YR5/4-Moist); , 2.5Y62; , 2.5YR48; Heavy clay; Massive grade of structure; 
	Moderately moist; Weak consistence; Very few (0 - 2 %), Ferruginous, Very coarse (20 - 60 mm), 
	Nodules; Few

	Project Name:	PAT
	Project Code:	PAT	Site ID:	H248	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (TAS)
	C	1.52 - 1.68 m	Light grey (2.5Y7/1-Moist); , 10YR54; , 2.5YR36; Heavy clay; Moderately moist; Weak 
	consistence; Very few (0 - 2 %), Ferruginous, , Nodules; Few
	2.13 - 2.26 m	Light grey (2.5Y7/1-Moist); , 2.5YR36; , 10YR54; Heavy clay; Weak consistence; 
	Morphological Notes
	Observation Notes
	ODD LARGE LUMPS OF CONCRETIONARY LATERITE <150MM IN CLAY HORIZON:WORMS ACTIVE:>226CM ON LATERITE
	 BOULDERS:              
	Site Notes
	LAUNCESTON

	Project Name:	PAT
	Project Code:	PAT	Site ID:	H248	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (TAS)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.025	6.1A	 0.048A	 8.1H	 2.3	 0.28	 0.16	 12.5E	 23.3B
	0.025 - 0.09	5.7A	 0.027A	 1.9H	 0.62	 0.1	 0.08	 7.5E	 10.2B
	0.09 - 0.18	5.4A	 0.024A	 0.29H	 0.24	 0.06	 0.08	 6.3E	 7B
	0.23 - 0.36	5.8A	 0.018A	 0.23H	 0.29	 0.05	 0.08	 4.8E	 5.5B
	0.42 - 0.56	6.1A	 0.039A	 3.2H	 6	 0.13	 0.77	 10.4E	 20.5B
	0.56 - 0.71	6.2A	 0.039A	 3.6H	 7.3	 0.18	 0.4	 9.6E	 21.4B
	0.71 - 0.86	6.1A	 0.045A
	0.86 - 1.07	6A	 0.048A
	1.52 - 1.68	5.3A	 0.071A
	2.13 - 2.26	4.9A	 0.11A	 0.48H	 3.1	 0.08	 0.8	 15.6E	 20.1B
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.025	 4.35D	 0.008D	 0.227A	 22	 13B	 60	 15	 5
	0.025 - 	 1.74D	 0.003D	 0.089A	 31	 15B	 63	 15	 5
	0.09
	0.09 - 0.18	 1.13D	 0.049A	 42	 15B	 63	 14	 5
	0.23 - 0.36	 0.72D	 0.037A	 61	 19D	 59	 14	 7
	0.42 - 0.56	 0.8D	 0.09A	 1	 3D	 15	 7	 73
	0.56 - 0.71	 0	 1D	 10	 5	 81
	0.71 - 0.86
	0.86 - 1.07
	1.52 - 1.68
	2.13 - 2.26	 0	 2D	 12	 10	 73
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.025
	0.025 - 0.09
	0.09 - 0.18
	0.23 - 0.36
	0.42 - 0.56
	0.56 - 0.71
	0.71 - 0.86
	0.86 - 1.07
	1.52 - 1.68
	2.13 - 2.26

	Project Name:	PAT
	Project Code:	PAT	Site ID:	H248	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (TAS)
	Laboratory Analyses Completed for this profile
	12_HCL_FE	Total element - Fe(%) - Total acid(HCl) extractable Fe
	15E1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) by compulsive exchange, no pretreatment for soluble 
	15E1_K	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MG	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_NA	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15G1_H	Hydrogen Cation - meq per 100g of soil - 1M KCl Exch. Acidity By titration to pH 8.0
	15J_H	Sum of Ex. cations + Ex. acidity - Sum of basic exch. cations and exch. (Hydrogen)
	2_LOI	Loss on Ignition (%)
	2A1	Air-dry moisture content
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	5A2	Chloride - 1:5 soil/water extract, automated colour
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	7A2	Total nitrogen - semimicro Kjeldahl , automated colour
	9A_HCL	Total element - P(%) - By boiling HCl
	P10_GRAV	Gravel (%)
	P10_PB_C	Clay (%) - Plummet balance
	P10_PB_CS	Coarse sand (%) - Plummet balance
	P10_PB_FS	Fine sand (%) - Plummet balance
	P10_PB_Z	Silt (%) - Plummet balance
	P10A1_C	Clay (%) - Pipette
	P10A1_CS	Coarse sand (%) - Pipette
	P10A1_FS	Fine sand (%) - Pipette
	P10A1_Z	Silt (%) - Pipette