Project Name:	PAU
	Project Code:	PAU	Site ID:	H232	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (TAS)
	Site Information
	Desc. By:	K.D. Nicholls	Locality:	6.5KM SE of Mathinna in forestry commission pine 
	plantation:1CH SW of 60CH peg on survey line No.10:
	Date Desc.:	10/11/61	Elevation:	 442 metres
	Map Ref.:	Sheet No. : 4794   	Rainfall:	0
	Northing/Long.:	147.944444444444	Runoff:	Rapid
	Easting/Lat.:	-41.5027777777778	Drainage:	Well drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Soil pit, 1.1 m deep,Quartzite 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	Escarpment
	Morph. Type:	Ridge	Relief:	No Data
	Elem. Type:	Hillslope	Slope Category:	Steep
	Slope:	48.8 % 	Aspect:	0 degrees
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Magnesic Brown Kandosol     	Principal Profile Form:	Gn3.74
	ASC Confidence:	Great Soil Group:	Yellow podzolic soil
	All necessary analytical data are available.
	Site Disturbance:	Limited clearing, for example selective logging
	Vegetation:	Low Strata - Tussock grass, , Very sparse. *Species includes - None recorded
	Tall Strata - Tree, , Very sparse. *Species includes - None Recorded
	Surface Coarse Fragments:	20-50%, , , Quartzite
	Profile Morphology
	O1	0 - 0.01 m	Organic Layer; Very dark grey (10YR3/1-Moist); ; Loam (Sapric); Moderate grade of structure, <2 
	mm, Granular; Moderately moist; Loose consistence; 20-50%, Charcoal, coarse fragments; 
	Clear change to - 
	A2	0.01 - 0.04 m	Very dark greyish brown (10YR3/2-Moist); Brown (10YR5/3-Dry); ; Loam; Moderate grade of 
	structure, <2 mm, Granular; Moderately moist; Loose consistence; 50-90%, subangular platy, 
	Gravel, coarse fragments; Diffuse change to - 
	A2	0.04 - 0.08 m	Very dark greyish brown (10YR3/2-Moist); Pale brown (10YR6/3-Dry); ; Loam (Heavy); Moderate 
	grade of structure, <2 mm, Granular; Moderately moist; Loose consistence; 50-90%, subangular 
	platy, Gravel, coarse fragments; Diffuse change to - 
	B1	0.08 - 0.18 m	Brownish yellow (10YR6/5-Moist); ; Clay loam (Heavy); Moderate grade of structure, <2 mm, 
	Granular; 20-50%, subangular platy, Gravel, coarse fragments; Clear change to - 
	B1	0.18 - 0.25 m	Brownish yellow (10YR6/5-Moist); ; Clay loam (Heavy); Weak grade of structure; Moist; Weak 
	consistence; 20-50%, subangular platy, Gravel, coarse fragments; Clear change to - 
	B1B2	0.25 - 0.43 m	Brownish yellow (10YR6/6-Moist); ; Light clay; Weak grade of structure; Moist; Weak 
	consistence; 20-50%, subangular platy, Gravel, coarse fragments; Diffuse change to - 
	B2	0.43 - 0.61 m	Reddish yellow (7.5YR6/6-Moist); ; Medium clay; Weak grade of structure; Moist; Weak 
	consistence; 20-50%, subangular platy, Gravel, coarse fragments; Diffuse change to - 
	B2	0.61 - 0.76 m	Strong brown (7.5YR5/6-Moist); ; Medium clay; Massive grade of structure; Moist; Weak 
	consistence; 20-50%, subangular platy, Gravel, coarse fragments; Diffuse change to - 
	B2	0.76 - 0.96 m	Strong brown (7.5YR5/8-Moist); ; Medium clay; Massive grade of structure; Moist; Weak 
	consistence; 2-10%, subangular platy, Gravel, coarse fragments; Clear change to - 
	Morphological Notes
	Observation Notes
	96-109CM MOSTLY ROCK FRAGMENTS WITH CLAY COATINGS:GROUND COVER OF PLATYQU AND SL:                              
	         
	Site Notes

	Project Name:	PAU
	Project Code:	PAU	Site ID:	H232	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (TAS)
	BEN LOMOND

	Project Name:	PAU
	Project Code:	PAU	Site ID:	H232	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (TAS)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.01	5.3A	 0.027A	 2.6H	 1.7	 0.66	 0.45
	0.01 - 0.04	5.2A	 0.057A	 0.87H	 1.7	 0.72	 0.72
	0.04 - 0.08	5.2A	 0.039A	 0.15H	 1.2	 0.49	 0.64
	0.08 - 0.18	5.4A	 0.018A
	0.18 - 0.25	5.5A	 0.018A
	0.25 - 0.43	5.6A	 0.021A
	0.43 - 0.61	5.6A	 0.018A	<0.05H	 0.84	 0.42	 0.23
	0.61 - 0.76	5.2A	 0.051A
	0.76 - 0.96	5.5A	 0.018A	<0.05H	 0.74	 0.32	 0.18
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.01	 14.7D	 0.013D	 0.196A	 68	 24B	 25	 22	 11
	0.01 - 0.04	 11.3D	 0.009D	 0.138A	 64	 10B	 34	 27	 12
	0.04 - 0.08	 7.36D	 0.008D	 0.103A	 53	 16B	 28	 32	 14
	0.08 - 0.18	 1.35D	 0.043A
	0.18 - 0.25
	0.25 - 0.43
	0.43 - 0.61	 23	 10D	 15	 30	 47
	0.61 - 0.76
	0.76 - 0.96	 10	 7D	 25	 22	 47
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.01
	0.01 - 0.04
	0.04 - 0.08
	0.08 - 0.18
	0.18 - 0.25
	0.25 - 0.43
	0.43 - 0.61
	0.61 - 0.76
	0.76 - 0.96

	Project Name:	PAU
	Project Code:	PAU	Site ID:	H232	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (TAS)
	Laboratory Analyses Completed for this profile
	15E1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) by compulsive exchange, no pretreatment for soluble 
	15E1_K	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MG	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_NA	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	2_LOI	Loss on Ignition (%)
	2A1	Air-dry moisture content
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	5A2	Chloride - 1:5 soil/water extract, automated colour
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	7A2	Total nitrogen - semimicro Kjeldahl , automated colour
	9A_HCL	Total element - P(%) - By boiling HCl
	P10_GRAV	Gravel (%)
	P10_PB_C	Clay (%) - Plummet balance
	P10_PB_CS	Coarse sand (%) - Plummet balance
	P10_PB_FS	Fine sand (%) - Plummet balance
	P10_PB_Z	Silt (%) - Plummet balance
	P10A1_C	Clay (%) - Pipette
	P10A1_CS	Coarse sand (%) - Pipette
	P10A1_FS	Fine sand (%) - Pipette
	P10A1_Z	Silt (%) - Pipette