Project Name:	POR
	Project Code:	POR	Site ID:	H111	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (TAS)
	Site Information
	Desc. By:	G.M. Dimmock	Locality:	Near site of old yacca plots (Dept of Agric.)
	Date Desc.:	14/12/54	Elevation:	 12 metres
	Map Ref.:	Rainfall:	530
	Northing/Long.:	147.6916667	Runoff:	Slow
	Easting/Lat.:	-40.86666667	Drainage:	Poorly drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Unconsolidated material (unidentified) 
	Land Form
	Rel/Slope Class: 	Gently undulating plains <9m  	Pattern Type:	Plain
	1-3%
	Morph. Type:	Simple-slope	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	Gently inclined
	Slope:	0 % 	Aspect:	0 degrees
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Melacic-Parapanic Humic/Humosequic Semiaquic Podosol   	Principal Profile Form:	Uc4.33
	ASC Confidence:	Great Soil Group:	Humus podzol
	Analytical data are incomplete but reasonable confidence.
	Site Disturbance:	No effective disturbance. Natural
	Vegetation:
	Tall Strata - Tree, , . *Species includes - Banksia marginata
	Surface Coarse Fragments:
	Profile Morphology
	A1	0 - 0.15 m	Black (10YR2/1-Moist); Grey (10YR5/1-Dry); ; Sand; Single grain grade of structure; Moist; 
	ManyDiffuse change to - 
	A12	0.15 - 0.28 m	Black (10YR2/1-Moist); ; Sand; Single grain grade of structure; Moist; CommonDiffuse change 
	to - 
	A2	0.28 - 0.53 m	Dark grey (10YR4/1-Moist); Grey (10YR5/1-Dry); , 10YR62; Sand; Single grain grade of structure; 
	Wet; Diffuse change to - 
	B	0.63 - 0.74 m	Very dark brown (10YR2/2-Moist); ; Sandy loam; Wet; Sharp, Irregular change to - 
	B	0.74 - 0.86 m	Very dark brown (10YR2/2-Moist); , 10YR33; , 7.5YR34; Massive grade of structure; Wet; Other 
	pans, Strongly cemented, Massive; Diffuse change to - 
	B	0.86 - 1.04 m	Dark brown (10YR3/3-Moist); , 10YR54; Sand; Single grain grade of structure; Wet; 
	Morphological Notes
	Observation Notes
	86-104CM SOME LUMPS OF STRONGLY CEMENTED MATERIAL:                                                                      
	Site Notes
	DORSET

	Project Name:	POR
	Project Code:	POR	Site ID:	H111	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (TAS)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.15	5.9A	 1.9H	 0.82	 0.09	 0.26	 3.4H	 7.5B
	 4.4E
	0.15 - 0.28	4.9A	 3C
	0.28 - 0.53	4.6A	 1C
	0.63 - 0.74	5.5A	 6C
	0.74 - 0.86	5.7A	 0.04	 10C
	0.86 - 1.04	5.3A	 4C
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.15	 1.6D	 0.002D	 0.072A	 20D	 70	 6	 2
	0.15 - 0.28
	0.28 - 0.53	 0.3D	 0.021A
	0.63 - 0.74	 1.2D	 0.058A
	0.74 - 0.86	 1.5D	 0.059A
	0.86 - 1.04
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.15
	0.15 - 0.28
	0.28 - 0.53
	0.63 - 0.74
	0.74 - 0.86
	0.86 - 1.04

	Project Name:	POR
	Project Code:	POR	Site ID:	H111	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (TAS)
	Laboratory Analyses Completed for this profile
	12_HCL_FE	Total element - Fe(%) - Total acid(HCl) extractable Fe
	15D1_CEC	CEC - 1M ammonium acetate at pH 7.0, pretreatment for soluble salts; manual leach
	15E1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) by compulsive exchange, no pretreatment for soluble 
	15E1_K	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MG	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_NA	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15G_C_H1	Exchangeable hydrogen - meq per 100g of soil - Hydrogen By back titration of A or B
	15G1_H	Hydrogen Cation - meq per 100g of soil - 1M KCl Exch. Acidity By titration to pH 8.0
	15J_H	Sum of Ex. cations + Ex. acidity - Sum of basic exch. cations and exch. (Hydrogen)
	2_LOI	Loss on Ignition (%)
	2A1	Air-dry moisture content
	4A1	pH of 1:5 soil/water suspension
	5A2	Chloride - 1:5 soil/water extract, automated colour
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	7A2	Total nitrogen - semimicro Kjeldahl , automated colour
	9A_HCL	Total element - P(%) - By boiling HCl
	P10_PB_C	Clay (%) - Plummet balance
	P10_PB_CS	Coarse sand (%) - Plummet balance
	P10_PB_FS	Fine sand (%) - Plummet balance
	P10_PB_Z	Silt (%) - Plummet balance