Project Name:	SAN
	Project Code:	SAN	Site ID:	H172	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (TAS)
	Site Information
	Desc. By:	K.D. Nicholls	Locality:	Approx 4.6M below crest of Long Dune Ridge on 
	leeward side:
	Date Desc.:	16/01/58	Elevation:	 43 metres
	Map Ref.:	Rainfall:	No Data
	Northing/Long.:	144.6666667	Runoff:	No Data
	Easting/Lat.:	-41.0416667	Drainage:	No Data
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Calcareous sand 
	Land Form
	Rel/Slope Class: 	Undulating rises 9-30m 3-10%	Pattern Type:	Dunefield
	Morph. Type:	Upper-slope	Relief:	No Data
	Elem. Type:	Dune	Slope Category:	Gently inclined
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Fragic Humosequic Aeric Podosol     	Principal Profile Form:	N/A
	ASC Confidence:	Great Soil Group:	N/A
	All necessary analytical data are available.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Fern, 0.51-1m, Mid-dense. *Species includes - None recorded
	Mid Strata - Shrub, , . *Species includes - Banksia marginata
	Tall Strata - Tree, 3.01-6m, . *Species includes - Eucalyptus similis
	Surface Coarse Fragments:
	Profile Morphology
	A1	0 - 0.04 m	Dark grey (10YR4/1-Moist); ; Sand; Single grain grade of structure; Dry; Very weak consistence; 
	AbundantDiffuse change to - 
	A2	0.04 - 0.1 m	Grey (10YR6/1-Moist); ; Sand; Single grain grade of structure; Dry; Loose consistence; Common
	A2	0.1 - 0.2 m	Grey (10YR6/1-Moist); ; Sand; Single grain grade of structure; Moderately moist; Loose 
	consistence; Common
	A2	0.2 - 0.32 m	Grey (10YR6/1-Moist); ; Sand; Single grain grade of structure; Moderately moist; Loose 
	consistence; CommonDiffuse change to - 
	0.32 - 0.4 m	White (10YR8/1-Moist); , 10YR64; , 10YR62; Sand; Single grain grade of structure; Loose 
	consistence; CommonDiffuse, Tongued change to - 
	0.41 - 0.69 m	White (10YR8/2-Moist); , 7.5YR56; , 7.5YR54; Sand; Single grain grade of structure; Loose 
	consistence; Diffuse change to - 
	0.69 - 0.79 m	Strong brown (7.5YR5/6-Moist); , 7.5YR54; Sand; Single grain grade of structure; Loose 
	consistence; CommonDiffuse change to - 
	0.86 - 0.97 m	Strong brown (7.5YR5/6-Moist); , 7.5YR54; , 7.5YR34; Sand; Single grain grade of structure; 
	Loose consistence; 
	B	0.97 - 0.99 m	Dark brown (7.5YR3/4-Moist); ; Massive grade of structure; 50-90%, Shells, coarse fragments; 
	Other pans, Weakly cemented, Massive; 
	C	1.02 - 1.22 m	Light yellowish brown (10YR6/4-Moist); ; Sand; Single grain grade of structure; Moderately 
	moist; Loose consistence; 50-90%, Shells, coarse fragments; 
	C	1.22 - 1.57 m	Light yellowish brown (10YR6/4-Moist); ; Sand; Single grain grade of structure; Moderately 
	moist; Loose consistence; 50-90%, Shells, coarse fragments; 
	C	2.54 - 3.81 m	Light yellowish brown (10YR6/4-Moist); ; Sand; Single grain grade of structure; Moderately 
	moist; Loose consistence; 50-90%, Shells, coarse fragments; 

	Project Name:	SAN
	Project Code:	SAN	Site ID:	H172	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (TAS)
	C	3.81 - 3.96 m	Light yellowish brown (10YR6/4-Moist); ; Sand; Single grain grade of structure; Moderately 
	moist; Loose consistence; 
	Morphological Notes
	Observation Notes
	86-97CM SAND WITH WEAKLY CEMENTED ORGANIC SAND AND CALC. SAND:97-99CM ORGANIC PAN:>97CM IS 
	CALCAREOUS SAND:             
	Site Notes

	Project Name:	SAN
	Project Code:	SAN	Site ID:	H172	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (TAS)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.04	5.2A	 0.016A	 4.6H	 1.2	 0.13	 0.37	 7.8H	 17.9B
	 11.6E
	0.04 - 0.1	5A	 0.018A	 0.6H	 0.19	 0.04	 0.12	 2.1H	 3.8B
	 2.8E
	0.1 - 0.2	5A	 0.012A
	0.2 - 0.32	4.8A	 0.015A
	0.32 - 0.4	5A	 0.012A
	0.41 - 0.69	5.5A	 0.024A
	0.69 - 0.79	6.6A	 0.057A
	0.86 - 0.97	8.6A	 0.092A
	0.97 - 0.99	6.7A	 0.065A
	1.02 - 1.22	9.2A	 0.054A
	1.22 - 1.57	9.3A	 0.057A
	2.54 - 3.81	9.4A	 0.057A
	3.81 - 3.96	9.5A	 0.057A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.04	 3D	 0.005D	 0.138A	 0	 27B	 64	 1	 1
	0.04 - 0.1	 0.87D	 0.001D	 0.033A	 0	 23D	 74	 3	 0
	0.1 - 0.2
	0.2 - 0.32
	0.32 - 0.4
	0.41 - 0.69
	0.69 - 0.79
	0.86 - 0.97	 24A
	0.97 - 0.99	 1.2D	 0.053B
	1.02 - 1.22	 29A
	1.22 - 1.57	 35A
	2.54 - 3.81	 25A
	3.81 - 3.96	 28A
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.04
	0.04 - 0.1
	0.1 - 0.2
	0.2 - 0.32
	0.32 - 0.4
	0.41 - 0.69
	0.69 - 0.79
	0.86 - 0.97
	0.97 - 0.99
	1.02 - 1.22
	1.22 - 1.57
	2.54 - 3.81
	3.81 - 3.96

	Project Name:	SAN
	Project Code:	SAN	Site ID:	H172	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (TAS)

	Project Name:	SAN
	Project Code:	SAN	Site ID:	H172	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (TAS)
	Laboratory Analyses Completed for this profile
	15E1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) by compulsive exchange, no pretreatment for soluble 
	15E1_K	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MG	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_NA	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15G_C_H1	Exchangeable hydrogen - meq per 100g of soil - Hydrogen By back titration of A or B
	15G1_H	Hydrogen Cation - meq per 100g of soil - 1M KCl Exch. Acidity By titration to pH 8.0
	15J_H	Sum of Ex. cations + Ex. acidity - Sum of basic exch. cations and exch. (Hydrogen)
	19A1	Carbonates - rapid titration
	2_LOI	Loss on Ignition (%)
	2A1	Air-dry moisture content
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	5A2	Chloride - 1:5 soil/water extract, automated colour
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	7_NR	Total nitrogen (%) - Not recorded
	7A2	Total nitrogen - semimicro Kjeldahl , automated colour
	9A_HCL	Total element - P(%) - By boiling HCl
	P10_GRAV	Gravel (%)
	P10_PB_C	Clay (%) - Plummet balance
	P10_PB_CS	Coarse sand (%) - Plummet balance
	P10_PB_FS	Fine sand (%) - Plummet balance
	P10_PB_Z	Silt (%) - Plummet balance
	P10A1_C	Clay (%) - Pipette
	P10A1_CS	Coarse sand (%) - Pipette
	P10A1_FS	Fine sand (%) - Pipette
	P10A1_Z	Silt (%) - Pipette