Project Name:	SOR
	Project Code:	SOR	Site ID:	H211	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (TAS)
	Site Information
	Desc. By:	K.D. Nicholls	Locality:	Property "Lowes Park":4.2KM E of Midlands H`way on 
	Glen Morey Rd:~2M from H210 (same pit):
	Date Desc.:	29/03/61	Elevation:	 216 metres
	Map Ref.:	Rainfall:	480
	Northing/Long.:	147.434722222222	Runoff:	Slow
	Easting/Lat.:	-42.1819444444445	Drainage:	Poorly drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Unconsolidated material (unidentified) 
	Land Form
	Rel/Slope Class: 	Gently undulating plains <9m  	Pattern Type:	Alluvial plain
	1-3%
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Pediment	Slope Category:	Gently inclined
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Eutrophic Mottled-Mesonatric Grey Sodosol     	Principal Profile Form:	Dd2.33
	ASC Confidence:	Great Soil Group:	Solodized solonetz
	All necessary analytical data are available.
	Site Disturbance:	Complete clearing. Pasture, native or improved, but never cultivated
	Vegetation:	Low Strata - Tussock grass, 0.51-1m, Mid-dense. *Species includes - None recorded
	Tall Strata - Tree, , . *Species includes - Eucalyptus ovata
	Surface Coarse Fragments:
	Profile Morphology
	A1	0 - 0.02 m	Dark brown (7.5YR3/2-Moist); Brown (7.5YR4/3-Dry); ; Sandy loam; Weak grade of structure, <2 
	mm, Subangular blocky; Dry; Very weak consistence; Diffuse change to - 
	A1	0.02 - 0.11 m	Dark brown (7.5YR3/3-Moist); Brown (7.5YR5/3-Dry); ; Sandy loam; Weak grade of structure, 10-
	20 mm, Angular blocky; Dry; Very weak consistence; 2-10%, Gravel, coarse fragments; Diffuse 
	change to - 
	A1A2cb	0.11 - 0.27 m	Brown (10YR4/3-Moist); Brown (10YR5/3-Dry); , 10YR52; Sand (Heavy); Single grain grade of 
	structure; Common (1-5 per 100mm2) Fine (1-2mm) macropores, Dry; Weak consistence; 2-10%,
	 Gravel, coarse fragments; Clear change to - 
	A2	0.27 - 0.51 m	; 2-10%, Gravel, coarse fragments; 
	B	0.56 - 0.69 m	Very dark grey (10YR3/1-Moist); , 5YR34; , 10YR43; Heavy clay; Weak grade of structure, 10-20 
	mm, Angular blocky; Moderately moist; Very firm consistence; 2-10%, Gravel, coarse fragments; 
	Few cutans, <10% of ped faces or walls coated; Diffuse change to - 
	B	0.74 - 0.86 m	Brown (10YR4/3-Moist); , 10YR54; Medium clay; Massive grade of structure; Moist; Very firm 
	consistence; 10-20%, stony, 200-600mm, rounded, Dolerite, coarse fragments; Few (2 - 10 %), 
	Unidentified, Fine (0 - 2 mm), Concretions; Diffuse change to - 
	Morphological Notes
	Observation Notes
	MICRORELIEF - OCCASIONAL DEPRESSIONS:27-51CM SCRAPED FROM A STEEPLY DIPPING SIDE OF A CLAY DOME:     
	                   
	Site Notes
	INTERLARKEN

	Project Name:	SOR
	Project Code:	SOR	Site ID:	H211	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (TAS)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.02	6.2A	 0.804A	 7.7H	 4	 1.1	 0.27	 4.3H	 17.4B
	0.02 - 0.11	6.5A	 0.063A	 6.8H	 2.8	 0.74	 0.47	 2.3H	 13.1B
	0.11 - 0.27	7.1A	 0.039A
	0.27 - 0.51	7.8A	 0.071A	 2.1H	 2.1	 0.36	 1.3	 4.9B
	0.56 - 0.69	8.4A	 0.247A	 6.2H	 6.2	 0.72	 4.4	 24.3B
	0.74 - 0.86	9.4A	 0.661A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.02	 3.3D	 0.019D	 0.247A	 0	 13B	 54	 11	 17
	0.02 - 0.11	 1.63D	 0.014D	 0.139A	 7	 13D	 55	 11	 18
	0.11 - 0.27	 0.59D	 0.05A
	0.27 - 0.51	 0.29D	 0.027A	 5	 16D	 64	 10	 8
	0.56 - 0.69	 0.76D	 0.078A	 5	 6B	 31	 7	 55
	0.74 - 0.86
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.02
	0.02 - 0.11
	0.11 - 0.27
	0.27 - 0.51
	0.56 - 0.69
	0.74 - 0.86

	Project Name:	SOR
	Project Code:	SOR	Site ID:	H211	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (TAS)
	Laboratory Analyses Completed for this profile
	15E1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) by compulsive exchange, no pretreatment for soluble 
	15E1_K	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MG	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_NA	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15G_C_H1	Exchangeable hydrogen - meq per 100g of soil - Hydrogen By back titration of A or B
	15J_H	Sum of Ex. cations + Ex. acidity - Sum of basic exch. cations and exch. (Hydrogen)
	2_LOI	Loss on Ignition (%)
	2A1	Air-dry moisture content
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	5A2	Chloride - 1:5 soil/water extract, automated colour
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	7A2	Total nitrogen - semimicro Kjeldahl , automated colour
	9A_HCL	Total element - P(%) - By boiling HCl
	P10_GRAV	Gravel (%)
	P10_PB_C	Clay (%) - Plummet balance
	P10_PB_CS	Coarse sand (%) - Plummet balance
	P10_PB_FS	Fine sand (%) - Plummet balance
	P10_PB_Z	Silt (%) - Plummet balance
	P10A1_C	Clay (%) - Pipette
	P10A1_CS	Coarse sand (%) - Pipette
	P10A1_FS	Fine sand (%) - Pipette
	P10A1_Z	Silt (%) - Pipette