Project Name:	STM
	Project Code:	STM	Site ID:	H48	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (TAS)
	Site Information
	Desc. By:	C.G. Stephens	Locality:
	Date Desc.:	21/01/53	Elevation:	 247 metres
	Map Ref.:	Sheet No. : 8514   1:100000	Rainfall:	790
	Northing/Long.:	148.033333333333	Runoff:	Slow
	Easting/Lat.:	-41.5666666666667	Drainage:	Moderately well drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Unconsolidated material (unidentified) 
	Land Form
	Rel/Slope Class: 	Undulating rises 9-30m 3-10%	Pattern Type:	Terrace (alluvial)
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	Valley flat	Slope Category:	Gently inclined
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Bleached-Mottled Mesotrophic Grey Kandosol     	Principal Profile Form:	Gn2.95
	ASC Confidence:	Great Soil Group:	Yellow podzolic soil
	All necessary analytical data are available.
	Site Disturbance:	Complete clearing. Pasture, native or improved, cultivated at some stage
	Vegetation:	Low Strata - Sod grass, <0.25m, Closed or dense. *Species includes - None recorded
	Tall Strata - Tree, 12.01-20m, Isolated plants. *Species includes - Eucalyptus pauciflora
	Surface Coarse Fragments:
	Profile Morphology
	A1p	0 - 0.11 m	Very dark greyish brown (10YR3/2-Moist); ; Loamy sand; Single grain grade of structure; Moist; 
	Weak consistence; Sharp change to - 
	A2	0.14 - 0.24 m	Brown (10YR4/3-Moist); ; Sand; Single grain grade of structure; Moist; Weak consistence; 
	Diffuse change to - 
	A2	0.27 - 0.36 m	Yellowish brown (10YR5/4-Moist); ; Sand; Single grain grade of structure; Moist; Weak 
	consistence; 0-2%, Gravel, coarse fragments; Diffuse change to - 
	A2B1	0.38 - 0.51 m	Light olive grey (5Y6/2-Moist); , 2.5Y54, 0-2% ; , 0-2% ; Sand; Single grain grade of structure; 
	Firm consistence; Diffuse change to - 
	A2B1	0.51 - 0.66 m	Light olive grey (5Y6/2-Moist); , 2.5Y54, 2-10% ; , 2-10% ; Sand; Single grain grade of structure; 
	Firm consistence; Diffuse change to - 
	B2	0.69 - 0.84 m	Light olive grey (5Y6/2-Moist); , 2.5Y54, 2-10% , Distinct; , 2-10% , Distinct; Clayey sand; Single 
	grain grade of structure; Common (1-5 per 100mm2) Very fine (0.075-1mm) macropores, Firm 
	consistence; Few (2 - 10 %), Ferruginous, Very coarse (20 - 60 mm), Concretions; Diffuse 
	change to - 
	Bg	0.86 - 1.09 m	Light grey (5Y7/1-Moist); , 5Y62; , 10YR56; Sandy clay loam; Massive grade of structure; Fine, (0
	 - 5) mm crack; Firm consistence; Diffuse change to - 
	Bg	1.12 - 1.32 m	Light grey (5Y7/1-Moist); , 10YR56; , 10YR53; Sandy medium clay; Massive grade of structure; 
	Fine, (0 - 5) mm crack; Firm consistence; Sharp change to - 
	1.32 - 1.55 m	Light grey (5Y7/1-Moist); , 10YR56; , 10YR53; Sandy medium clay; 2-10%, rounded, Sandstone, 
	coarse fragments; Diffuse change to - 
	1.55 - 1.73 m	Light grey (5Y7/1-Moist); , 10YR56; , 2.5YR48; Heavy clay; 2-10%, rounded, Gravel, coarse 
	fragments; 
	Morphological Notes
	Observation Notes
	>173CM ON WATER WORN DOLERITE STONES:86-132CM WEAKLY DEVELOPED VERTICALCLEAVAGE FACES:              

	Project Name:	STM
	Project Code:	STM	Site ID:	H48	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (TAS)
	Site Notes
	CORNWALL

	Project Name:	STM
	Project Code:	STM	Site ID:	H48	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (TAS)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.11	4.5A	 4.7H	 1	 0.33	 0.08	 4.5H	 14B
	 7.9E
	0.14 - 0.24	4.4A
	0.27 - 0.36	4.3A
	0.38 - 0.51	4.1A
	0.51 - 0.66	5.3A
	0.69 - 0.84	6.9A
	0.86 - 1.09	7.3A
	1.12 - 1.32	7.1A
	1.32 - 1.55	7.2A
	1.55 - 1.73	6.6A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.11	 2.04D	 0.01D	 0.226A	 0	 50B	 29	 8	 7
	0.14 - 0.24	 0.44D	 0.058A
	0.27 - 0.36	 0.16D	 0.004D	 1	 54B	 32	 7	 6
	0.38 - 0.51
	0.51 - 0.66
	0.69 - 0.84	 0	 29B	 47	 11	 12
	0.86 - 1.09
	1.12 - 1.32	 0.003D	 0	 43B	 24	 8	 24
	1.32 - 1.55
	1.55 - 1.73
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.11
	0.14 - 0.24
	0.27 - 0.36
	0.38 - 0.51
	0.51 - 0.66
	0.69 - 0.84
	0.86 - 1.09
	1.12 - 1.32
	1.32 - 1.55
	1.55 - 1.73

	Project Name:	STM
	Project Code:	STM	Site ID:	H48	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (TAS)
	Laboratory Analyses Completed for this profile
	15E1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) by compulsive exchange, no pretreatment for soluble 
	15E1_K	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MG	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_NA	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15G_C_H1	Exchangeable hydrogen - meq per 100g of soil - Hydrogen By back titration of A or B
	15G1_H	Hydrogen Cation - meq per 100g of soil - 1M KCl Exch. Acidity By titration to pH 8.0
	15J_H	Sum of Ex. cations + Ex. acidity - Sum of basic exch. cations and exch. (Hydrogen)
	2_LOI	Loss on Ignition (%)
	2A1	Air-dry moisture content
	4A1	pH of 1:5 soil/water suspension
	5A2	Chloride - 1:5 soil/water extract, automated colour
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	7A2	Total nitrogen - semimicro Kjeldahl , automated colour
	9A_HCL	Total element - P(%) - By boiling HCl
	P10_GRAV	Gravel (%)
	P10A1_C	Clay (%) - Pipette
	P10A1_CS	Coarse sand (%) - Pipette
	P10A1_FS	Fine sand (%) - Pipette
	P10A1_Z	Silt (%) - Pipette