Project Name:	Soils of the Swiftsynd Pasture Trial Sites
	Project Code:	SWIFS	Site ID:	21	Observation ID:	1
	Agency Name:	NT Natural Resources, Environment and the Arts
	Site Information
	Desc. By:	Locality:
	Date Desc.:	18/02/09	Elevation:	No Data
	Map Ref.:	Rainfall:	No Data
	Northing/Long.:	133.535334	Runoff:	Rapid
	Easting/Lat.:	-23.875262  Datum: GDA94	Drainage:	No Data
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Landform
	Rel/Slope Class: 	No Data	Pattern Type:	Plain
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	No Data
	Slope:	0.2 % 	Aspect:	No Data
	Surface Soil Condition 
	Erosion
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Hyperbasic Paralithic Supracalcic Calcarosol Thin Non-gravelly 	Principal Profile Form:	N/A
	Loamy  Very deep
	ASC Confidence:	Great Soil Group:	N/A
	Analytical data are incomplete but reasonable confidence.
	Site Disturbance
	Vegetation
	Surface Coarse Fragments
	Profile Morphology
	A12	0.03 - 0.09 m	Reddish brown (5YR5/3-Moist); ; Sandy loam; Massive grade of structure; Earthy fabric; Field pH 8.6 
	(pH meter); 
	B1k	0.09 - 0.2 m	Reddish brown (5YR4/3-Moist); ; Sandy clay loam; Massive grade of structure; Earthy fabric; Field pH 
	8.5 (pH meter); 
	B21k	0.2 - 0.3 m	Reddish brown (5YR4/4-Moist); ; Sandy clay loam; Massive grade of structure; Earthy fabric; Field pH 
	8.5 (pH meter); 
	B22k	0.3 - 0.6 m	Yellowish red (5YR4/6-Moist); ; Sandy clay loam; Massive grade of structure; Earthy fabric; Field pH 8.5 
	(pH meter); 
	B32	0.8 - 1.8 m	Reddish brown (5YR4/4-Moist); ; Sandy clay loam; Massive grade of structure; Earthy fabric; Field pH 
	9.1 (pH meter); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Soils of the Swiftsynd Pasture Trial Sites
	Project Code:	SWIFS	Site ID:	21	Observation 	1
	Agency Name:	NT Natural Resources, Environment and the Arts
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	8.4C	0.074A	10.44H	1.01	0.53	0.01	0J
	8.6A
	0.1 - 0.2	8.4C	0.078A	11.89H	1.07	0.55	0.03	0J
	8.5A
	0.2 - 0.3	8.4C	0.074A	12.11H	1.06	0.47	0.02	0J
	8.5A
	0.5 - 0.6	8.4C	0.089A	14.16H	1.42	0.15	0.03	0J
	8.5A
	0.8 - 0.9	8.4C	0.059A	12.36H	1.81	0.14	0.05	0J
	9.1A
	1.1 - 1.2	8.6C	0.055A	11.45H	2.22	0.15	0.12	0J
	9.1A
	1.4 - 1.5	8.6C	0.07A	10.13H	3.98	0.15	0.35	0J
	9.1A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1	0.43A	12J	0.02D	3	42.17A	33.46	10.74	13.63
	75.63G
	0.1 - 0.2	0.28A	5J	0.03D	2	40.42A	25.71	12.97	20.9
	66.13G
	0.2 - 0.3	0.24A	5J	0.03D	7	37.5A	28.52	11.01	22.97
	66.02G
	0.5 - 0.6	0.08A	3J	0.02D	8	38.19A	33.29	10.83	17.68
	71.48G
	0.8 - 0.9	0.1A	3J	0.04D	4	44.94A	28.54	8.86	17.66
	73.48G
	1.1 - 1.2	0.15A	2J	0.04D	4	50.71A	26.86	7.82	14.61
	77.57G
	1.4 - 1.5	0.09A	2J	0.03D	2	39A	38.66	9.74	12.61
	77.65G
	Laboratory Analyses Completed for this profile
	10D1	Potassium chloride - 40 sulfur (KCl-40)-S
	12A1_CU	DTPA - extractable copper, zinc, manganese and iron
	12A1_FE	DTPA - extractable copper, zinc, manganese and iron
	12A1_MN	DTPA - extractable copper, zinc, manganese and iron
	12A1_ZN	DTPA - extractable copper, zinc, manganese and iron
	15E1_AL	Exchangeable Al - by compulsive exchange, no pretreatment for soluble salts
	15E1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) by compulsive exchange, no pretreatment for soluble salts
	15E1_K	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MG	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_NA	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts

	Project Name:	Soils of the Swiftsynd Pasture Trial Sites
	Project Code:	SWIFS	Site ID:	21	Observation 	1
	Agency Name:	NT Natural Resources, Environment and the Arts
	18A1	Bicarbonate-extractable potassium
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	4B2	pH of 1:5 soil/0.01M calcium chloride extract - following Method 4A1
	5A2	Chloride - 1:5 soil/water extract, automated colour
	6A1	Organic carbon - Walkley and Black
	7A5	Total nitrogen - high frequency induction furnace, thermal conductivity
	9B1	Bicarbonate-extractable phosphorus - manual colour
	P10_CF_C	Clay (%) - Coventry and Fett pipette method
	P10_CF_CS	Coarse sand (%) - Coventry and Fett pipette method
	P10_CF_FS	Fine sand (%) - Coventry and Fett pipette method
	P10_CF_S	Sand (%) - Coventry and Fett pipette method
	P10_CF_Z	Silt (%) - Coventry and Fett pipette method
	P10_GRAV	Gravel (%)