Project Name:	Soils of the Swiftsynd Pasture Trial Sites
	Project Code:	SWIFS	Site ID:	27	Observation ID:	1
	Agency Name:	NT Natural Resources, Environment and the Arts
	Site Information
	Desc. By:	Locality:
	Date Desc.:	19/05/09	Elevation:	No Data
	Map Ref.:	Rainfall:	No Data
	Northing/Long.:	134.082789	Runoff:	No runoff
	Easting/Lat.:	-17.099049  Datum: GDA94	Drainage:	No Data
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Landform
	Rel/Slope Class: 	No Data	Pattern Type:	Plain
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	No Data
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition 
	Erosion
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Mottled Epipedal Brown Vertosol Non-gravelly Fine Fine  	Principal Profile Form:	N/A
	ASC Confidence:	Great Soil Group:	N/A
	No analytical data are available but confidence is fair.
	Site Disturbance
	Vegetation
	Surface Coarse Fragments
	Profile Morphology
	A1	0 - 0.2 m	Brown (10YR5/3-Moist); ; Light clay; Strong grade of structure; Smooth-ped fabric; Field pH 6.9 (pH 
	meter); 
	B21	0.2 - 0.32 m	Brown (10YR5/3-Moist); ; Light clay; Strong grade of structure; Smooth-ped fabric; Field pH 6.9 (pH 
	meter); 
	B23	0.5 - 0.95 m	Reddish brown (2.5YR5/3-Moist); ; Light medium clay; Strong grade of structure; Smooth-ped fabric; 
	Field pH 7.8 (pH meter); 
	B24	0.95 - 1.4 m	Light olive brown (2.5Y5/4-Moist); ; Light clay; Strong grade of structure; Smooth-ped fabric; Field pH 
	7.4 (pH meter); 
	B25	1.4 - 2 m	Light olive brown (2.5Y5/4-Moist); ; Light medium clay; Strong grade of structure; Smooth-ped fabric; 
	Field pH 7.4 (pH meter); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Soils of the Swiftsynd Pasture Trial Sites
	Project Code:	SWIFS	Site ID:	27	Observation 	1
	Agency Name:	NT Natural Resources, Environment and the Arts
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	6.6C	0.017A	8.51H	5.06	0.12	0.07	0J
	6.9A
	0.1 - 0.2	6.6C	0.02A	10.48H	4.46	0.04	0.1	0J
	6.9A
	0.2 - 0.6	6.8C	0.027A	10.95H	4.17	0.03	0.13	0J
	6.9A
	0.5 - 0.6	7C	0.024A	10.28H	4.15	0.02	0.61	0J
	7.8A
	0.8 - 0.9	7.3C	0.056A	10.64H	4.35	0.02	0.88	0J
	7.8A
	1.1 - 1.2	7.4C	0.732A	12.17H	5.1	0.04	1.5	0J
	7.4A
	1.4 - 1.5	7.3C	0.601A	10.16H	6.73	0.04	2.36	0J
	7.4A
	1.7 - 1.8	7.4C	1.244A	10.2H	7.6	0.06	2.77	0J
	7.4A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1	0.38A	3J	0.03D	0	14.75A	20.42	13.76	51.07
	35.17G
	0.1 - 0.2	0.23A	2J	0.02D	0	15.5A	18.02	17.14	49.34
	33.52G
	0.2 - 0.6	0.21A	4J	0.01D	0	14.75A	20.28	16	48.96
	35.03G
	0.5 - 0.6	0.16A	2J	0.02D	1	19.03A	16.43	13.12	51.43
	35.45G
	0.8 - 0.9	0.12A	2J	0.01D	1	16.74A	19.02	13.85	50.4
	35.76G
	1.1 - 1.2	0.14A	2J	0.01D	0	13.1A	24.38	25.23	37.29
	37.47G
	1.4 - 1.5	0.13A	2J	0.01D	1	14.37A	21.02	22.58	42.03
	35.39G
	1.7 - 1.8	0.1A	2J	0.01D	0	9.97A	23.92	25.45	40.66
	33.89G
	Laboratory Analyses Completed for this profile
	10D1	Potassium chloride - 40 sulfur (KCl-40)-S
	12A1_CU	DTPA - extractable copper, zinc, manganese and iron
	12A1_FE	DTPA - extractable copper, zinc, manganese and iron
	12A1_MN	DTPA - extractable copper, zinc, manganese and iron
	12A1_ZN	DTPA - extractable copper, zinc, manganese and iron

	Project Name:	Soils of the Swiftsynd Pasture Trial Sites
	Project Code:	SWIFS	Site ID:	27	Observation 	1
	Agency Name:	NT Natural Resources, Environment and the Arts
	15E1_AL	Exchangeable Al - by compulsive exchange, no pretreatment for soluble salts
	15E1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) by compulsive exchange, no pretreatment for soluble salts
	15E1_K	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MG	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_NA	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	18A1	Bicarbonate-extractable potassium
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	4B2	pH of 1:5 soil/0.01M calcium chloride extract - following Method 4A1
	5A2	Chloride - 1:5 soil/water extract, automated colour
	6A1	Organic carbon - Walkley and Black
	7A5	Total nitrogen - high frequency induction furnace, thermal conductivity
	9B1	Bicarbonate-extractable phosphorus - manual colour
	P10_CF_C	Clay (%) - Coventry and Fett pipette method
	P10_CF_CS	Coarse sand (%) - Coventry and Fett pipette method
	P10_CF_FS	Fine sand (%) - Coventry and Fett pipette method
	P10_CF_S	Sand (%) - Coventry and Fett pipette method
	P10_CF_Z	Silt (%) - Coventry and Fett pipette method
	P10_GRAV	Gravel (%)