Project Name:	YAMBULLA RESEARCH CATCHMENTS            
	Project Code:	1000196	Site ID:	YAM_RC1	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Site Information
	Desc. By:	P. Ryan	Locality:
	Date Desc.:	18/03/86	Elevation:	No Data
	Map Ref.:	Sheet No. : 8823   1:25000	Rainfall:	No Data
	Northing/Long.:	5866025 AMG zone: 55	Runoff:	No Data
	Easting/Lat.:	733875  Datum: AGD66	Drainage:	Well drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	Probable
	Geol. Ref.:	DGL	Substrate Material:	Adamellite 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	No Data
	Morph. Type:	Mid-slope	Relief:	0 metres
	Elem. Type:	Hillslope	Slope Category:	No Data
	Slope:	33 % 	Aspect:	180 degrees
	Surface Soil Condition (dry):	Soft
	Erosion:	Stable, Minor (sheet) No rill erosion (rill) No gully
	 erosion (gully) 
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 N/A    	Principal Profile Form:	Db3.11
	ASC Confidence:	Great Soil Group:	Brown podzolic soil
	Confidence level not specified
	Site Disturbance:
	Vegetation:
	Surface Coarse Fragments:	2-10%, stony, 200-600mm, subrounded, Adamellite
	Profile Morphology
	O1	0 - 0.03 m	Organic Layer; ; Sandy loam (Sapric); Dry; Non-plastic; Non-sticky; Abrupt, Smooth change to - 
	A1	0.03 - 0.07 m	Very dark greyish brown (10YR3/2-Moist); ; Coarse sandy clay loam; Single grain grade of 
	structure; Dry; Loose consistence; Slightly plastic; Slightly sticky; 2-10%, coarse gravelly, 20-
	60mm, subangular, dispersed, Adamellite, coarse fragments; 20-50%, fine gravelly, 2-6mm, 
	subangular, dispersed, Quartz, coarse fragments; Field pH 5.5 (Raupach); ManyGradual, 
	Irregular change to - 
	B21	0.07 - 0.4 m	Dark yellowish brown (10YR4/4-Moist); ; Coarse sandy clay; Moderate grade of structure, 5-10 
	mm, Subangular blocky; 2-5 mm, Polyhedral; Rough-ped fabric; Moderately moist; Firm 
	consistence; 2-10%, coarse gravelly, 20-60mm, subangular, dispersed, Adamellite, coarse 
	fragments; 20-50%, fine gravelly, 2-6mm, subangular, dispersed, Quartz, coarse fragments; Few 
	cutans, <10% of ped faces or walls coated, faint; Field pH 6.5 (Raupach); CommonGradual, 
	Irregular change to - 
	B22	0.4 - 0.68 m	Strong brown (7.5YR5/6-Moist); ; Moderate grade of structure, 5-10 mm, Angular blocky; Smooth-
	ped fabric; Firm consistence; 20-50%, cobbly, 60-200mm, subrounded, undisturbed, 
	Adamellite, coarse fragments; 20-50%, fine gravelly, 2-6mm, subangular, undisturbed, Quartz, 
	coarse fragments; Common cutans, 10-50% of ped faces or walls coated, faint; Field pH 6.5 
	(Raupach); Common
	BC	0.68 - 0.69 m	; 
	Morphological Notes
	Observation Notes
	B21 could possibly be A2 (colluvial)    over in-situ B22.                       A1 is hydrophobic.                                                               
	                                       
	Site Notes
	Catch.3/310-313                       

	Project Name:	YAMBULLA RESEARCH CATCHMENTS            
	Project Code:	1000196	Site ID:	YAM_RC1	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0.03 - 0.07	4.48I	8.96F	3.9	0.86	1.96	0.17G
	4.88H
	0.07 - 0.4	5.03I	3.09F	1.68	0.44	1.02	0.02G
	5.58H
	0.4 - 0.68	4.35I	1.63F	1.83	0.46	0.97	0.32G
	4.89H
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0.03 - 0.07	17.7A	210F	0.4E	28.4
	0.07 - 0.4	1.42A	59F	0.04E	13.3
	0.4 - 0.68	1.23A	76F	0.04E	15.6
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0.03 - 0.07
	0.07 - 0.4
	0.4 - 0.68

	Project Name:	YAMBULLA RESEARCH CATCHMENTS            
	Project Code:	1000196	Site ID:	YAM_RC1	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Analyses Completed for this profile
	15D1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium acetate at pH 7.0, pretreatment for 
	soluble salts; manual leach
	15D1_K	Exchangeable bases and CEC - 1M ammonium acetate at pH 7.0, pretreatment for soluble salts; 
	manual leach
	15D1_MG	Exchangeable bases and CEC - 1M ammonium acetate at pH 7.0, pretreatment for soluble salts; 
	manual leach
	15D1_NA	Exchangeable bases and CEC - 1M ammonium acetate at pH 7.0, pretreatment for soluble salts; 
	manual leach
	15G_C_AL2	Exchangeable aluminium - meq per 100g of soil - Aluminium By KCl extraction and detremination By
	 AAS
	2A1	Air-dry moisture content
	4A_C_1	pH of soil - pH of 1:1 soil/water suspension
	4C_C_1	pH of 1:1 soil/1M potassium chloride suspension
	6A1	Organic carbon - Walkley and Black
	7A1	Total nitrogen - semimicro Kjeldahl, steam distillation
	9A_NR	Total element - P(%) - Not recorded
	P10_GRAV	Gravel (%)