Project Name:	YAMBULLA RESEARCH CATCHMENTS            
	Project Code:	1000196	Site ID:	YAM_RC4	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Site Information
	Desc. By:	P. Ryan	Locality:
	Date Desc.:	19/03/86	Elevation:	No Data
	Map Ref.:	Sheet No. : 8823   1:25000	Rainfall:	No Data
	Northing/Long.:	5865525 AMG zone: 55	Runoff:	No Data
	Easting/Lat.:	733400  Datum: AGD66	Drainage:	Well drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	Probable
	Geol. Ref.:	DGL	Substrate Material:	Adamellite 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	No Data
	Morph. Type:	Mid-slope	Relief:	0 metres
	Elem. Type:	Hillslope	Slope Category:	No Data
	Slope:	18 % 	Aspect:	315 degrees
	Surface Soil Condition (dry):	Soft
	Erosion:	Stable, Minor (sheet) No rill erosion (rill) No gully
	 erosion (gully) 
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 N/A    	Principal Profile Form:	Dy4.81
	ASC Confidence:	Great Soil Group:	Yellow podzolic soil
	Confidence level not specified
	Site Disturbance:
	Vegetation:
	Surface Coarse Fragments:	2-10%, cobbly, 60-200mm, subrounded, Adamellite
	Profile Morphology
	A1	0 - 0.08 m	Dark yellowish brown (10YR4/4-Moist); ; Coarse sandy loam; Weak grade of structure, 5-10 mm, 
	Polyhedral; 2-5 mm, Granular; Rough-ped fabric; Dry; Weak consistence; Non-plastic; Non-
	sticky; 10-20%, coarse gravelly, 20-60mm, subrounded, dispersed, Adamellite, coarse 
	fragments; 10-20%, fine gravelly, 2-6mm, subangular, dispersed, Quartz, coarse fragments; Few 
	(2 - 10 %), Ferruginous, Medium (2 -6 mm), Nodules; Few (2 - 10 %), Ferruginous, Coarse (6 - 20 
	mm), Nodules; Clear, Wavy change to - 
	A2e	0.08 - 0.33 m	Brownish yellow (10YR6/6-Moist); Very pale brown (10YR7/4-Dry); ; Coarse sandy clay loam; 
	Weak grade of structure, 5-10 mm, Subangular blocky; Earthy fabric; Dry; Firm consistence; 
	Slightly plastic; Slightly sticky; 10-20%, coarse gravelly, 20-60mm, subrounded, dispersed, 
	Adamellite, coarse fragments; 10-20%, fine gravelly, 2-6mm, subangular, dispersed, Quartz, 
	coarse fragments; Few (2 - 10 %), Ferruginous, Medium (2 -6 mm), Nodules; Few (2 - 10 %), 
	Ferruginous, Coarse (6 - 20 mm), Nodules; Gradual, Wavy change to - 
	B2	0.33 - 0.64 m	Brownish yellow (10YR6/8-Moist); ; Coarse sandy clay; Weak grade of structure, 5-10 mm, 
	Subangular blocky; Rough-ped fabric; Moderately moist; Firm consistence; Moderately plastic; 
	Moderately sticky; 2-10%, coarse gravelly, 20-60mm, subrounded, dispersed, Adamellite, coarse
	 fragments; 2-10%, fine gravelly, 2-6mm, subangular, dispersed, Quartz, coarse fragments; Few 
	cutans, <10% of ped faces or walls coated, faint; Clear, Smooth change to - 
	BC	0.64 - 0.8 m	Brownish yellow (10YR6/6-Moist); Mottles, 10-20% , Faint; Coarse sandy clay loam; Massive 
	grade of structure; Earthy fabric; Moderately moist; Firm consistence; Moderately plastic; 10-
	20%, coarse gravelly, 20-60mm, subrounded, dispersed, Adamellite, coarse fragments; 10-20%,
	 fine gravelly, 2-6mm, subangular, dispersed, Quartz, coarse fragments; Few cutans, <10% of 
	ped faces or walls coated, faint; 
	Morphological Notes
	Observation Notes
	North-facing slope with tor field       upslope.                                BC hor retains rock fabric.                                                           
	                                  
	Site Notes
	Catch.3/306-309                       

	Project Name:	YAMBULLA RESEARCH CATCHMENTS            
	Project Code:	1000196	Site ID:	YAM_RC4	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.08	4.06I	1.94F	0.95	0.44	0.89	0.8G
	4.82H
	0.08 - 0.33	4.14I	0.58F	0.95	0.42	0.75	0.73G
	4.81H
	0.33 - 0.64	3.82I	0.22F	0.88	0.55	0.92	1.55G
	4.47H
	0.64 - 0.8	3.96I	0.26F	1.05	0.48	1.03	0.81G
	4.55H
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.08	3.2A	26F	0.07E	20.7
	0.08 - 0.33	0.7A	13F	0.02E	15.8
	0.33 - 0.64	0.36A	13F	0.01E	6.4
	0.64 - 0.8	0.3A	15F	0.01E	7.4
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.08
	0.08 - 0.33
	0.33 - 0.64
	0.64 - 0.8

	Project Name:	YAMBULLA RESEARCH CATCHMENTS            
	Project Code:	1000196	Site ID:	YAM_RC4	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Analyses Completed for this profile
	15D1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium acetate at pH 7.0, pretreatment for 
	soluble salts; manual leach
	15D1_K	Exchangeable bases and CEC - 1M ammonium acetate at pH 7.0, pretreatment for soluble salts; 
	manual leach
	15D1_MG	Exchangeable bases and CEC - 1M ammonium acetate at pH 7.0, pretreatment for soluble salts; 
	manual leach
	15D1_NA	Exchangeable bases and CEC - 1M ammonium acetate at pH 7.0, pretreatment for soluble salts; 
	manual leach
	15G_C_AL2	Exchangeable aluminium - meq per 100g of soil - Aluminium By KCl extraction and detremination By
	 AAS
	2A1	Air-dry moisture content
	4A_C_1	pH of soil - pH of 1:1 soil/water suspension
	4C_C_1	pH of 1:1 soil/1M potassium chloride suspension
	6A1	Organic carbon - Walkley and Black
	7A1	Total nitrogen - semimicro Kjeldahl, steam distillation
	9A_NR	Total element - P(%) - Not recorded
	P10_GRAV	Gravel (%)