Project Name:	WAGGA WAGGA SOIL LANDSCAPES             
	Project Code:	1000448	Site ID:	WW114	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Site Information
	Desc. By:	Chen, XY	Locality:
	Date Desc.:	15/07/93	Elevation:	308 metres
	Map Ref.:	Sheet No. : 8327   1:25000	Rainfall:	No Data
	Northing/Long.:	6085150 AMG zone: 55	Runoff:	Slow
	Easting/Lat.:	541475  Datum: AGD66	Drainage:	Moderately well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	Ou	Substrate Material:	Siltstone 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	Hills
	Morph. Type:	Simple-slope	Relief:	No Data
	Elem. Type:	Hillslope	Slope Category:	No Data
	Slope:	27 % 	Aspect:	90 degrees
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 N/A    	Principal Profile Form:	Dr2.21
	ASC Confidence:	Great Soil Group:	Red podzolic soil
	Confidence level not specified
	Site Disturbance:	Complete clearing. Pasture, native or improved, but never cultivated
	Vegetation:
	Surface Coarse Fragments:	0-2%, fine gravelly, 2-6mm, subrounded tabular, Siltstone; No surface coarse fragments
	Profile Morphology
	A1	0 - 0.15 m	Dark reddish brown (5YR3/3-Moist); ; Coarse sandy clay loam; Massive grade of structure; Earthy
	 fabric; Common (1-5 per 100mm2) Fine (1-2mm) macropores, Common (1-5 per 100mm2) Very 
	fine (0.075-1mm) macropores, Moist; Slightly plastic; Moderately sticky; 2-10%, fine gravelly, 2-
	6mm, subrounded tabular, dispersed, Siltstone, coarse fragments; Field pH 5.5 (Raupach); 
	Common, fine (1-2mm) roots; Clear, Smooth change to - 
	A2	0.15 - 0.5 m	Reddish brown (5YR4/4-Moist); Light brown (7.5YR6/4-Dry); ; Coarse sandy clay loam; Massive 
	grade of structure; Earthy fabric; Common (1-5 per 100mm2) Fine (1-2mm) macropores, 
	Common (1-5 per 100mm2) Very fine (0.075-1mm) macropores, Moderately moist; Slightly 
	plastic; Moderately sticky; 20-50%, fine gravelly, 2-6mm, subrounded tabular, dispersed, 
	Siltstone, coarse fragments; Field pH 6 (Raupach); Common, fine (1-2mm) roots; Gradual, 
	Smooth change to - 
	B	0.5 - 0.9 m	Red (2.5YR4/6-Moist); ; Medium heavy clay; Moderate grade of structure, 5-10 mm, Subangular 
	blocky; Smooth-ped fabric; Few (<1 per 100mm2) Fine (1-2mm) macropores, Few (<1 per 
	100mm2) Very fine (0.075-1mm) macropores, Moist; Very plastic; Moderately sticky; 20-50%, fine
	 gravelly, 2-6mm, subrounded tabular, dispersed, Siltstone, coarse fragments; Common cutans,
	 10-50% of ped faces or walls coated, distinct; Field pH 6 (Raupach); Common, fine (1-2mm) 
	roots; 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	WAGGA WAGGA SOIL LANDSCAPES             
	Project Code:	1000448	Site ID:	WW114	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.15	4.8B	0.06A	1J	1.4	0.9	0.5	0L	5.1I	9.80
	0.15 - 0.5	5.6B	0.04A	0.7J	1.8	0.4	0.4	0L	7.1I	5.63
	0.5 - 0.9	5.3B	0.04A	0.7J	7	0.6	0.5	0L	10.8I	4.63
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.15	1.44A	3D	5	17F	48	19	11
	0.15 - 0.5	0.4A	1D	36	21F	25	11	7
	0.5 - 0.9	0.45A	0D	9	9F	16	16	50
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.15	0.49B	0.1B
	0.15 - 0.5	0.29B	0.07B
	0.5 - 0.9	0.52B	0.23B

	Project Name:	WAGGA WAGGA SOIL LANDSCAPES             
	Project Code:	1000448	Site ID:	WW114	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Analyses Completed for this profile
	15F1_CA	Exchangeable bases by 0.01M silver-thiourea (AgTU)+, no pretreatment for soluble salts
	15F1_K	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_MG	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_NA	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F2	Exchangeable aluminium by 0.01m (AgTU)+
	15F3	CEC by 0.01M silver-thiourea (AgTU)+
	3A1	EC of 1:5 soil/water extract
	4B1	pH of 1:5 soil/0.01M calcium chloride extract - direct
	6A1	Organic carbon - Walkley and Black
	9E	Available P (mg/kg) - Bray P
	9J2	Phosphate sorption curve - automated colour
	P10_GRAV	Gravel (%)
	P10_HYD_C	Clay (%) - Hydrometer Method
	P10_HYD_CS	Coarse Sand (%) - Hydrometer Method
	P10_HYD_FS	Fine Sand (%) - Hydrometer Method
	P10_HYD_Z	Silt (%) - Hydrometer Method
	P3B_GV_01	0.1 BAR Moisture g/g - Gravimetric  using suction plate
	P3B_GV_15	15 BAR Moisture g/g - Gravimetric using pressure plate