Project Name:	WAGGA WAGGA SOIL LANDSCAPES             
	Project Code:	1000448	Site ID:	WW162	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Site Information
	Desc. By:	Chen, XY	Locality:
	Date Desc.:	15/07/93	Elevation:	211 metres
	Map Ref.:	Sheet No. : 8327   1:25000	Rainfall:	No Data
	Northing/Long.:	6125550 AMG zone: 55	Runoff:	Slow
	Easting/Lat.:	514875  Datum: AGD66	Drainage:	Moderately well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	Probable
	Geol. Ref.:	Sgc	Substrate Material:	Granite 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	Rises
	Morph. Type:	Upper-slope	Relief:	No Data
	Elem. Type:	Hillslope	Slope Category:	No Data
	Slope:	4 % 	Aspect:	135 degrees
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Red Kandosol Medium Slightly gravelly Loamy  	Principal Profile Form:	Gn2.11
	ASC Confidence:	Great Soil Group:	Red earth
	Confidence level not specified
	Site Disturbance:	Complete clearing. Pasture, native or improved, but never cultivated
	Vegetation:
	Surface Coarse Fragments:	0-2%, fine gravelly, 2-6mm, subrounded, Quartz; No surface coarse fragments
	Profile Morphology
	A	0 - 0.1 m	Dark reddish brown (5YR3/4-Moist); ; Clay loam; Weak grade of structure, <2 mm, Granular; 
	Earthy fabric; Common (1-5 per 100mm2) Very fine (0.075-1mm) macropores, Few (<1 per 
	100mm2) Fine (1-2mm) macropores, Dry; Weak consistence; Slightly plastic; Moderately sticky; 
	0-2%, fine gravelly, 2-6mm, subrounded, dispersed, Quartz, coarse fragments; Field pH 5.5 
	(Raupach); Many, fine (1-2mm) roots; Clear, Smooth change to - 
	B	0.1 - 0.5 m	Yellowish red (5YR3/6-Moist); ; Coarse sandy light clay; Weak grade of structure, 10-20 mm, 
	Polyhedral; Earthy fabric; Few (<1 per 100mm2) Very fine (0.075-1mm) macropores, Few (<1 per 
	100mm2) Fine (1-2mm) macropores, Dry; Firm consistence; Moderately plastic; Very sticky; 10-
	20%, fine gravelly, 2-6mm, subrounded, dispersed, Quartz, coarse fragments; Field pH 6 
	(Raupach); Common, fine (1-2mm) roots; Gradual, Smooth change to - 
	BC	0.5 - 0.7 m	Yellowish red (5YR4/8-Moist); Mottles, 10-20% , Faint; Mottles, 2-10% , Distinct; Coarse sandy 
	light clay; Weak grade of structure, 20-50 mm, Polyhedral; Earthy fabric; Few (<1 per 100mm2) 
	Very fine (0.075-1mm) macropores, Few (<1 per 100mm2) Fine (1-2mm) macropores, Dry; Firm 
	consistence; Moderately plastic; Very sticky; 20-50%, fine gravelly, 2-6mm, subrounded, 
	dispersed, Quartz, coarse fragments; Field pH 6 (Raupach); Few, fine (1-2mm) roots; 
	Morphological Notes
	Observation Notes
	Aust soil class: KAAA--CDBFLS- 2nd apprx                                                                                                                                      
	                          
	Site Notes
	30M M T-JUNCTION, W ROAD              

	Project Name:	WAGGA WAGGA SOIL LANDSCAPES             
	Project Code:	1000448	Site ID:	WW162	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h

	Project Name:	WAGGA WAGGA SOIL LANDSCAPES             
	Project Code:	1000448	Site ID:	WW162	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Analyses Completed for this profile