Project Name:	WAGGA WAGGA SOIL LANDSCAPES             
	Project Code:	1000448	Site ID:	WW181	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Site Information
	Desc. By:	Chen, XY	Locality:
	Date Desc.:	15/07/93	Elevation:	255 metres
	Map Ref.:	Sheet No. : 8327   1:25000	Rainfall:	No Data
	Northing/Long.:	6102550 AMG zone: 55	Runoff:	Slow
	Easting/Lat.:	531775  Datum: AGD66	Drainage:	Moderately well drained
	Geology
	ExposureType:	Existing vertical exposure	Conf. Sub. is Parent. Mat.:	Probable
	Geol. Ref.:	Ou	Substrate Material:	Sand 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	Low hills
	Morph. Type:	Lower-slope	Relief:	No Data
	Elem. Type:	Hillslope	Slope Category:	No Data
	Slope:	6 % 	Aspect:	45 degrees
	Surface Soil Condition (dry):	Hardsetting
	Erosion:	Partial, Minor (sheet) Partial, Minor (gully) 
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 N/A    	Principal Profile Form:	Dy3.8
	ASC Confidence:	Great Soil Group:	Soloth
	Confidence level not specified
	Site Disturbance:
	Vegetation:
	Surface Coarse Fragments:	2-10%, , , Quartz
	Profile Morphology
	A1	0 - 0.15 m	Very dark grey (7.5YR3/1-Moist); ; Loam; Massive grade of structure; Earthy fabric; Common (1-5 
	per 100mm2) Very fine (0.075-1mm) macropores, Few (<1 per 100mm2) Fine (1-2mm) 
	macropores, Dry; Firm consistence; Slightly plastic; Slightly sticky; 2-10%, Quartz, coarse 
	fragments; Field pH 4.5 (Raupach); Common, fine (1-2mm) roots; Gradual, Smooth change to - 
	A2	0.15 - 0.5 m	Light brownish grey (10YR6/2-Moist); Light grey (10YR7/2-Dry); ; Clayey coarse sand; Single 
	grain grade of structure; Sandy (grains prominent) fabric; Common (1-5 per 100mm2) Very fine 
	(0.075-1mm) macropores, Common (1-5 per 100mm2) Fine (1-2mm) macropores, Dry; Very firm 
	consistence; Non-plastic; Slightly sticky; 20-50%, Quartz, coarse fragments; Field pH 6 
	(Raupach); Few, fine (1-2mm) roots; Gradual, Smooth change to - 
	B	0.5 - 1 m	Brown (10YR5/3-Moist); Mottles, 10-20% , Distinct; Coarse sandy light medium clay; Weak 
	grade of structure, 10-20 mm, Subangular blocky; Earthy fabric; Few (<1 per 100mm2) Very fine 
	(0.075-1mm) macropores, Dry; Very firm consistence; Moderately plastic; Very sticky; 10-20%, 
	Quartz, coarse fragments; Field pH 5.5 (Raupach); Few, fine (1-2mm) roots; 
	Morphological Notes
	A1	Water expellent.                                                                                                                    
	                                                                    
	B	More sandy downwards.                                                                                                        
	                                                                           
	Observation Notes
	Sample taken near trees                                                                                                                                                                     
	            
	Site Notes
	GULLY NEAR GATE                       

	Project Name:	WAGGA WAGGA SOIL LANDSCAPES             
	Project Code:	1000448	Site ID:	WW181	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h

	Project Name:	WAGGA WAGGA SOIL LANDSCAPES             
	Project Code:	1000448	Site ID:	WW181	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Analyses Completed for this profile