Project Name:	WAGGA WAGGA SOIL LANDSCAPES             
	Project Code:	1000448	Site ID:	WW182	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Site Information
	Desc. By:	Chen, XY	Locality:
	Date Desc.:	15/07/93	Elevation:	253 metres
	Map Ref.:	Sheet No. : 8327   1:25000	Rainfall:	No Data
	Northing/Long.:	6104325 AMG zone: 55	Runoff:	Slow
	Easting/Lat.:	530075  Datum: AGD66	Drainage:	Imperfectly drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	Probable
	Geol. Ref.:	Ou	Substrate Material:	Sand 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	Low hills
	Morph. Type:	Lower-slope	Relief:	No Data
	Elem. Type:	Hillslope	Slope Category:	No Data
	Slope:	6 % 	Aspect:	45 degrees
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 N/A    	Principal Profile Form:	Dy3.41
	ASC Confidence:	Great Soil Group:	Soloth
	Confidence level not specified
	Site Disturbance:	Complete clearing. Pasture, native or improved, but never cultivated
	Vegetation:
	Surface Coarse Fragments:
	Profile Morphology
	A1	0 - 0.1 m	Dark greyish brown (10YR4/2-Moist); ; Coarse sandy loam; Massive grade of structure; Earthy 
	fabric; Common (1-5 per 100mm2) Very fine (0.075-1mm) macropores, Few (<1 per 100mm2) 
	Fine (1-2mm) macropores, Dry; Firm consistence; Non-plastic; Slightly sticky; 0-2%, fine 
	gravelly, 2-6mm, subrounded, dispersed, Quartz, coarse fragments; Field pH 5.5 (Raupach); 
	Many, fine (1-2mm) roots; Clear, Smooth change to - 
	A2	0.1 - 0.65 m	Light brownish grey (10YR6/2-Moist); White (10YR8/2-Dry); ; Clayey coarse sand; Massive grade 
	of structure; Earthy fabric; Common (1-5 per 100mm2) Very fine (0.075-1mm) macropores, Few 
	(<1 per 100mm2) Fine (1-2mm) macropores, Dry; Very firm consistence; Non-plastic; Slightly 
	sticky; 20-50%, fine gravelly, 2-6mm, subrounded, dispersed, Quartz, coarse fragments; Field pH
	 5.5 (Raupach); Few, fine (1-2mm) roots; Clear, Smooth change to - 
	B	0.65 - 1 m	Yellowish brown (10YR5/4-Moist); Mottles, 10-20% , Distinct; Coarse sandy light medium clay; 
	Moderate grade of structure, 20-50 mm, Subangular blocky; Smooth-ped fabric; Few (<1 per 
	100mm2) Very fine (0.075-1mm) macropores, Dry; Very firm consistence; Moderately plastic; 
	Very sticky; 2-10%, fine gravelly, 2-6mm, subrounded, dispersed, Quartz, coarse fragments; 
	Field pH 6 (Raupach); Few, fine (1-2mm) roots; 
	Morphological Notes
	A2	Compact.                                                                                                                              
	                                                                  
	Observation Notes
	Site Notes
	60M W GATE, S SIDE OF ROAD            

	Project Name:	WAGGA WAGGA SOIL LANDSCAPES             
	Project Code:	1000448	Site ID:	WW182	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	5B	0.05A	1.3J	1.4	0.5	0.7	0L	7.2I	9.72
	0.1 - 0.65	5B	0.1A	0.5J	1.7	0.3	0.8	0L	1.4I	57.14
	0.65 - 1	5B	0.17A	1.6J	4.3	0.3	3.1	0L	9.7I	31.96
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1	1.33A	0D	13	43F	28	10	6
	0.1 - 0.65	0.14A	0D	13	38F	33	8	8
	0.65 - 1	0.09A	0D	4	22F	40	11	23
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.1	0.27B	0.04B
	0.1 - 0.65	0.16B	0.04B
	0.65 - 1	0.34B	0.12B

	Project Name:	WAGGA WAGGA SOIL LANDSCAPES             
	Project Code:	1000448	Site ID:	WW182	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Analyses Completed for this profile
	15F1_CA	Exchangeable bases by 0.01M silver-thiourea (AgTU)+, no pretreatment for soluble salts
	15F1_K	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_MG	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_NA	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F2	Exchangeable aluminium by 0.01m (AgTU)+
	15F3	CEC by 0.01M silver-thiourea (AgTU)+
	3A1	EC of 1:5 soil/water extract
	4B1	pH of 1:5 soil/0.01M calcium chloride extract - direct
	6A1	Organic carbon - Walkley and Black
	9E	Available P (mg/kg) - Bray P
	9J2	Phosphate sorption curve - automated colour
	P10_GRAV	Gravel (%)
	P10_HYD_C	Clay (%) - Hydrometer Method
	P10_HYD_CS	Coarse Sand (%) - Hydrometer Method
	P10_HYD_FS	Fine Sand (%) - Hydrometer Method
	P10_HYD_Z	Silt (%) - Hydrometer Method
	P3B_GV_01	0.1 BAR Moisture g/g - Gravimetric  using suction plate
	P3B_GV_15	15 BAR Moisture g/g - Gravimetric using pressure plate