Project Name:	WAGGA WAGGA SOIL LANDSCAPES             
	Project Code:	1000448	Site ID:	WW184	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Site Information
	Desc. By:	Chen, XY	Locality:
	Date Desc.:	15/07/93	Elevation:	233 metres
	Map Ref.:	Sheet No. : 8327   1:25000	Rainfall:	No Data
	Northing/Long.:	6106975 AMG zone: 55	Runoff:	Slow
	Easting/Lat.:	530000  Datum: AGD66	Drainage:	Moderately well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	Cza	Substrate Material:	Clay 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	Pediment
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	No Data
	Slope:	2 % 	Aspect:	45 degrees
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 N/A    	Principal Profile Form:	Dy3.41
	ASC Confidence:	Great Soil Group:	Soloth
	Confidence level not specified
	Site Disturbance:
	Vegetation:
	Surface Coarse Fragments:
	Profile Morphology
	A1	0 - 0.1 m	Brown (7.5YR4/4-Moist); ; Clay loam; Weak grade of structure, 5-10 mm, Polyhedral; Earthy 
	fabric; Common (1-5 per 100mm2) Very fine (0.075-1mm) macropores, Few (<1 per 100mm2) 
	Fine (1-2mm) macropores, Dry; Weak consistence; Moderately plastic; Moderately sticky; Field 
	pH 5.5 (Raupach); Many, fine (1-2mm) roots; Gradual, Smooth change to - 
	A2	0.1 - 0.35 m	Pinkish grey (7.5YR6/3-Moist); Pinkish white (7.5YR8/3-Dry); ; Sandy loam; Massive grade of 
	structure; Earthy fabric; Common (1-5 per 100mm2) Very fine (0.075-1mm) macropores, Few (<1 
	per 100mm2) Fine (1-2mm) macropores, Dry; Firm consistence; Slightly plastic; Moderately 
	sticky; Very few (0 - 2 %), Ferromanganiferous, Fine (0 - 2 mm), Nodules, strong, 
	segregations;Very few (0 - 2 %), Ferromanganiferous, Medium (2 -6 mm), Nodules, strong, 
	segregations;Field pH 6 (Raupach); Common, fine (1-2mm) roots; Clear, Smooth change to - 
	B2	0.35 - 0.85 m	Yellowish brown (10YR5/4-Moist); Mottles, 20-50% , Faint; Light clay; Moderate grade of 
	structure, 20-50 mm, Subangular blocky; Smooth-ped fabric; Few (<1 per 100mm2) Very fine 
	(0.075-1mm) macropores, Dry; Strong consistence; Moderately plastic; Very sticky; Very few (0 - 
	2 %), Ferromanganiferous, Fine (0 - 2 mm), Nodules, strong, segregations;Very few (0 - 2 %), 
	Ferromanganiferous, Medium (2 -6 mm), Nodules, strong, segregations;Field pH 5.5 (Raupach); 
	Common, fine (1-2mm) roots; Gradual, Smooth change to - 
	B3	0.85 - 1.1 m	Yellowish brown (10YR5/4-Moist); Mottles, 20-50% , Faint; Light medium clay; Moderate grade of
	 structure, 2-5 mm, Polyhedral; 50-100 mm, Subangular blocky; Rough-ped fabric; Few (<1 per 
	100mm2) Very fine (0.075-1mm) macropores, Moderately moist; Very firm consistence; Very 
	plastic; Very sticky; Field pH 5.5 (Raupach); Common, fine (1-2mm) roots; 
	Morphological Notes
	Observation Notes
	Artificial drainage ditch exposure.                                                                                                                                                      
	               
	Site Notes

	Project Name:	WAGGA WAGGA SOIL LANDSCAPES             
	Project Code:	1000448	Site ID:	WW184	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	5.8B	0.04A	0.8J	1	0.5	0.6	0.1L	3.2I	18.75
	0.1 - 0.35	6.4B	0.68A	1.5J	1.7	0.5	0.5	0.1L	1.9I	26.32
	0.35 - 0.85	4.7B	1.52A	3.7J	6.8	0.7	1	0.1L	9.1I	10.99
	0.85 - 1.1	5.2B	0.75A	3.8J	7.8	0.3	1.2	0L	9.2I	13.04
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1	0.76A	1D	14F	57	18	11
	0.1 - 0.35	0.1A	0D	9F	49	26	16
	0.35 - 0.85	0.14A	0D	1	11F	32	14	42
	0.85 - 1.1	0.08A	0D	3	14F	34	14	35
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.1	0.37B	0.07B
	0.1 - 0.35	0.28B	0.07B
	0.35 - 0.85	0.39B	0.18B
	0.85 - 1.1	0.4B	0.17B

	Project Name:	WAGGA WAGGA SOIL LANDSCAPES             
	Project Code:	1000448	Site ID:	WW184	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Analyses Completed for this profile
	15F1_CA	Exchangeable bases by 0.01M silver-thiourea (AgTU)+, no pretreatment for soluble salts
	15F1_K	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_MG	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_NA	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F2	Exchangeable aluminium by 0.01m (AgTU)+
	15F3	CEC by 0.01M silver-thiourea (AgTU)+
	3A1	EC of 1:5 soil/water extract
	4B1	pH of 1:5 soil/0.01M calcium chloride extract - direct
	6A1	Organic carbon - Walkley and Black
	9E	Available P (mg/kg) - Bray P
	9J2	Phosphate sorption curve - automated colour
	P10_GRAV	Gravel (%)
	P10_HYD_C	Clay (%) - Hydrometer Method
	P10_HYD_CS	Coarse Sand (%) - Hydrometer Method
	P10_HYD_FS	Fine Sand (%) - Hydrometer Method
	P10_HYD_Z	Silt (%) - Hydrometer Method
	P3B_GV_01	0.1 BAR Moisture g/g - Gravimetric  using suction plate
	P3B_GV_15	15 BAR Moisture g/g - Gravimetric using pressure plate