Project Name:	WAGGA WAGGA SOIL LANDSCAPES             
	Project Code:	1000448	Site ID:	WW196	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Site Information
	Desc. By:	Chen, XY	Locality:
	Date Desc.:	15/07/93	Elevation:	188 metres
	Map Ref.:	Sheet No. : 8327   1:25000	Rainfall:	No Data
	Northing/Long.:	6110750 AMG zone: 55	Runoff:	Slow
	Easting/Lat.:	535675  Datum: AGD66	Drainage:	Imperfectly drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	Probable
	Geol. Ref.:	Cza	Substrate Material:	Sand 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	Alluvial plain
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	No Data
	Slope:	1 % 	Aspect:	45 degrees
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 N/A    	Principal Profile Form:	Db2.42
	ASC Confidence:	Great Soil Group:	N/A
	Confidence level not specified
	Site Disturbance:	Complete clearing. Pasture, native or improved, but never cultivated
	Vegetation:
	Surface Coarse Fragments:
	Profile Morphology
	A1	0 - 0.1 m	Very dark greyish brown (10YR3/2-Moist); Mottles, 2-10% , Faint; Silty clay loam; Weak grade of 
	structure; Earthy fabric; Common (1-5 per 100mm2) Very fine (0.075-1mm) macropores, Few (<1 
	per 100mm2) Fine (1-2mm) macropores, Dry; Very firm consistence; Moderately plastic; 
	Moderately sticky; Field pH 5.5 (Raupach); Common, fine (1-2mm) roots; Clear, Smooth change 
	to - 
	A2	0.1 - 0.4 m	Greyish brown (10YR5/2-Moist); Light grey (10YR7/2-Dry); Mottles, 2-10% , Faint; Silty clay loam; 
	Massive grade of structure; Earthy fabric; Many (>5 per 100mm2) Very fine (0.075-1mm) 
	macropores, Common (1-5 per 100mm2) Fine (1-2mm) macropores, Dry; Firm consistence; 
	Moderately plastic; Very sticky; Few (2 - 10 %), Ferromanganiferous, Fine (0 - 2 mm), Nodules, 
	strong, segregations;Few (2 - 10 %), Ferromanganiferous, Medium (2 -6 mm), Nodules, strong, 
	segregations;Field pH 6 (Raupach); Few, fine (1-2mm) roots; Gradual, Smooth change to - 
	B2	0.4 - 0.9 m	Brown (10YR4/3-Moist); Mottles, 10-20% , Faint; Medium clay; Moderate grade of structure, 50-
	100 mm, Subangular blocky; Smooth-ped fabric; Few (<1 per 100mm2) Very fine (0.075-1mm) 
	macropores, Few (<1 per 100mm2) Fine (1-2mm) macropores, Dry; Strong consistence; Very 
	plastic; Very sticky; Field pH 6 (Raupach); Few, fine (1-2mm) roots; Diffuse change to - 
	B3	0.9 - 1.2 m	Brown (10YR5/3-Moist); Mottles, 20-50% , Faint; Medium clay; Strong grade of structure, 20-50 
	mm, Polyhedral; Smooth-ped fabric; Few (<1 per 100mm2) Very fine (0.075-1mm) macropores, 
	Few (<1 per 100mm2) Fine (1-2mm) macropores, Dry; Strong consistence; Very plastic; Very 
	sticky; Very few (0 - 2 %), Ferromanganiferous, Fine (0 - 2 mm), Soft segregations, weak, 
	segregations;Very few (0 - 2 %), Ferromanganiferous, Medium (2 -6 mm), Soft segregations, 
	weak, segregations;Field pH 7.5 (Raupach); Few, fine (1-2mm) roots; 
	Morphological Notes
	Observation Notes
	Artificial drainage bank exposure.                                                                                                                                                      
	                
	Site Notes
	50M IN FENCE, W BANK                  

	Project Name:	WAGGA WAGGA SOIL LANDSCAPES             
	Project Code:	1000448	Site ID:	WW196	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	5.2B	0.05A	7J	2.6	0.7	0.2	0L	10.7I	1.87
	0.1 - 0.4	5.8B	0.03A	5.8J	2.2	0.4	0.5	0L	8.2I	6.10
	0.4 - 0.9	5.7B	0.03A	9.6J	7.5	1	1.3	0L	14.5I	8.97
	0.9 - 1.2	6.5B	0.04A	8.7J	7	0.6	0.9	0L	13.3I	6.77
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1	1.05A	1D	6F	45	26	23
	0.1 - 0.4	0.28A	1D	3	6F	38	36	17
	0.4 - 0.9	0.21A	0D	2F	27	24	47
	0.9 - 1.2	0.09A	0D	2F	39	23	36
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.1	0.42B	0.11B
	0.1 - 0.4	0.37B	0.09B
	0.4 - 0.9	0.51B	0.22B
	0.9 - 1.2	0.47B	0.17B

	Project Name:	WAGGA WAGGA SOIL LANDSCAPES             
	Project Code:	1000448	Site ID:	WW196	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Analyses Completed for this profile
	15F1_CA	Exchangeable bases by 0.01M silver-thiourea (AgTU)+, no pretreatment for soluble salts
	15F1_K	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_MG	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_NA	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F2	Exchangeable aluminium by 0.01m (AgTU)+
	15F3	CEC by 0.01M silver-thiourea (AgTU)+
	3A1	EC of 1:5 soil/water extract
	4B1	pH of 1:5 soil/0.01M calcium chloride extract - direct
	6A1	Organic carbon - Walkley and Black
	9E	Available P (mg/kg) - Bray P
	9J2	Phosphate sorption curve - automated colour
	P10_GRAV	Gravel (%)
	P10_HYD_C	Clay (%) - Hydrometer Method
	P10_HYD_CS	Coarse Sand (%) - Hydrometer Method
	P10_HYD_FS	Fine Sand (%) - Hydrometer Method
	P10_HYD_Z	Silt (%) - Hydrometer Method
	P3B_GV_01	0.1 BAR Moisture g/g - Gravimetric  using suction plate
	P3B_GV_15	15 BAR Moisture g/g - Gravimetric using pressure plate