Project Name:	WAGGA WAGGA SOIL LANDSCAPES             
	Project Code:	1000448	Site ID:	WW203	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Site Information
	Desc. By:	Chen, XY	Locality:
	Date Desc.:	15/07/93	Elevation:	411 metres
	Map Ref.:	Sheet No. : 8327   1:25000	Rainfall:	No Data
	Northing/Long.:	6081225 AMG zone: 55	Runoff:	Moderately rapid
	Easting/Lat.:	533075  Datum: AGD66	Drainage:	Well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	Probable
	Geol. Ref.:	Sgr	Substrate Material:	Granite 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	Hills
	Morph. Type:	Mid-slope	Relief:	No Data
	Elem. Type:	Hillslope	Slope Category:	No Data
	Slope:	20 % 	Aspect:	45 degrees
	Surface Soil Condition (dry):	Hardsetting
	Erosion:	Partial, Moderate (sheet) 
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Red Kandosol Medium Gravelly Peaty  	Principal Profile Form:	Gn2.14
	ASC Confidence:	Great Soil Group:	Red earth
	Confidence level not specified
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:
	Surface Coarse Fragments:	0-2%, fine gravelly, 2-6mm, subrounded, Quartz; No surface coarse fragments; No surface coarse fragments
	Profile Morphology
	A1	0 - 0.1 m	Dark reddish brown (5YR3/3-Moist); ; Coarse sandy loam; Weak grade of structure, 5-10 mm, 
	Polyhedral; Earthy fabric; Common (1-5 per 100mm2) Very fine (0.075-1mm) macropores, 
	Common (1-5 per 100mm2) Fine (1-2mm) macropores, Dry; Weak consistence; Slightly plastic; 
	Slightly sticky; 0-2%, fine gravelly, 2-6mm, subrounded, dispersed, Quartz, coarse fragments; 
	Field pH 5.5 (Raupach); Many, fine (1-2mm) roots; Gradual change to - 
	A2	0.1 - 0.2 m	Yellowish red (5YR4/6-Moist); Yellowish red (5YR5/6-Dry); ; Coarse sandy clay loam; Weak 
	grade of structure, 5-10 mm, Polyhedral; Earthy fabric; Common (1-5 per 100mm2) Very fine 
	(0.075-1mm) macropores, Common (1-5 per 100mm2) Fine (1-2mm) macropores, Dry; Firm 
	consistence; Slightly plastic; Moderately sticky; 2-10%, fine gravelly, 2-6mm, subrounded, 
	dispersed, Quartz, coarse fragments; Field pH 5.5 (Raupach); Common, fine (1-2mm) roots; 
	Gradual, Smooth change to - 
	B	0.2 - 0.65 m	Red (2.5YR4/8-Moist); ; Clay loam; Weak grade of structure, 2-5 mm, Polyhedral; Earthy fabric; 
	Common (1-5 per 100mm2) Very fine (0.075-1mm) macropores, Common (1-5 per 100mm2) Fine
	 (1-2mm) macropores, Dry; Very firm consistence; Moderately plastic; Moderately sticky; 2-10%, 
	fine gravelly, 2-6mm, subrounded, dispersed, Quartz, coarse fragments; Field pH 5 (Raupach); 
	Few, fine (1-2mm) roots; 
	Morphological Notes
	A1	A few metasedimentary rock pieces.                                                                                    
	                                                                                  
	Observation Notes
	Site Notes

	Project Name:	WAGGA WAGGA SOIL LANDSCAPES             
	Project Code:	1000448	Site ID:	WW203	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	4.2B	0.05A	1.6J	1.2	0.6	0.3	1.2L	5.8I	5.17
	0.1 - 0.2	3.8B	0.06A	0.4J	0.8	0.4	0.3	1.6L	4.2I	7.14
	0.2 - 0.65	5.1B	0.04A	0.3J	2.1	0.4	0.7	4.8L	11.5I	6.09
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1	3.1A	2D	11	32F	32	12	13
	0.1 - 0.2	1.25A	0D	14	24F	33	15	14
	0.2 - 0.65	0.35A	0D	5	23F	9	8	55
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.1	0.33B	0.1B
	0.1 - 0.2	0.27B	0.09B
	0.2 - 0.65	0.41B	0.21B

	Project Name:	WAGGA WAGGA SOIL LANDSCAPES             
	Project Code:	1000448	Site ID:	WW203	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Analyses Completed for this profile
	15F1_CA	Exchangeable bases by 0.01M silver-thiourea (AgTU)+, no pretreatment for soluble salts
	15F1_K	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_MG	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_NA	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F2	Exchangeable aluminium by 0.01m (AgTU)+
	15F3	CEC by 0.01M silver-thiourea (AgTU)+
	3A1	EC of 1:5 soil/water extract
	4B1	pH of 1:5 soil/0.01M calcium chloride extract - direct
	6A1	Organic carbon - Walkley and Black
	9E	Available P (mg/kg) - Bray P
	9J2	Phosphate sorption curve - automated colour
	P10_GRAV	Gravel (%)
	P10_HYD_C	Clay (%) - Hydrometer Method
	P10_HYD_CS	Coarse Sand (%) - Hydrometer Method
	P10_HYD_FS	Fine Sand (%) - Hydrometer Method
	P10_HYD_Z	Silt (%) - Hydrometer Method
	P3B_GV_01	0.1 BAR Moisture g/g - Gravimetric  using suction plate
	P3B_GV_15	15 BAR Moisture g/g - Gravimetric using pressure plate