Project Name:	WAGGA WAGGA SOIL LANDSCAPES             
	Project Code:	1000448	Site ID:	WW262	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Site Information
	Desc. By:	Chen, XY	Locality:
	Date Desc.:	15/07/93	Elevation:	251 metres
	Map Ref.:	Sheet No. : 8327   1:25000	Rainfall:	No Data
	Northing/Long.:	6094300 AMG zone: 55	Runoff:	Slow
	Easting/Lat.:	506550  Datum: AGD66	Drainage:	No Data
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	Probable
	Geol. Ref.:	Du	Substrate Material:	Gravel 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	Hills
	Morph. Type:	Lower-slope	Relief:	No Data
	Elem. Type:	Hillslope	Slope Category:	No Data
	Slope:	12 % 	Aspect:	270 degrees
	Surface Soil Condition (dry):	Hardsetting
	Erosion:	Stable, Minor (sheet) 
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Orthic Rudosol Thick Moderately gravelly Peaty  Shallow	Principal Profile Form:	Uc4.22
	ASC Confidence:	Great Soil Group:	Lithosol
	Confidence level not specified
	Site Disturbance:	Complete clearing. Pasture, native or improved, but never cultivated
	Vegetation:
	Surface Coarse Fragments:	0-2%, medium gravelly, 6-20mm, subrounded, ; No surface coarse fragments
	Profile Morphology
	A1	0 - 0.15 m	Very dark brown (7.5YR2/2-Moist); ; Fine sandy loam; Massive grade of structure; Earthy fabric; 
	Common (1-5 per 100mm2) Very fine (0.075-1mm) macropores, Common (1-5 per 100mm2) Fine
	 (1-2mm) macropores, Dry; Weak consistence; Non-plastic; Slightly sticky; 2-10%, medium 
	gravelly, 6-20mm, subrounded, dispersed, coarse fragments; Field pH 5 (Raupach); Common, 
	fine (1-2mm) roots; Gradual, Smooth change to - 
	A2	0.15 - 0.5 m	Reddish brown (5YR5/4-Moist); ; Loamy fine sand; Massive grade of structure; Earthy fabric; Few
	 (<1 per 100mm2) Very fine (0.075-1mm) macropores, Dry; Very weak consistence; Non-plastic; 
	Slightly sticky; 50-90%, medium gravelly, 6-20mm, subrounded, dispersed, coarse fragments; 
	Field pH 5.5 (Raupach); Few, fine (1-2mm) roots; Diffuse change to - 
	C	0.5 - 0.75 m	Reddish brown (5YR5/4-Moist); ; Loamy fine sand; Massive grade of structure; Earthy fabric; Few
	 (<1 per 100mm2) Very fine (0.075-1mm) macropores, Dry; Weak consistence; Non-plastic; 
	Slightly sticky; 50-90%, medium gravelly, 6-20mm, subrounded, dispersed, coarse fragments; 
	Field pH 5.5 (Raupach); Few, fine (1-2mm) roots; 
	Morphological Notes
	C	Slightly redder than layer 2.                                                                                                  
	                                                                         
	Observation Notes
	All gravels are lithic sandstone.       Quarry exposure.                                                                                                                       
	                         
	Site Notes
	300M SE OF DAM                        

	Project Name:	WAGGA WAGGA SOIL LANDSCAPES             
	Project Code:	1000448	Site ID:	WW262	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.15	4.4B	0.03A	0.9J	0.4	0.5	0.2	0.2L	2.5I	8.00
	0.15 - 0.5	4.3B	0.02A	0.5J	0.5	0.3	0.2	0.5L	2I	10.00
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.15	1.67A	3D	3	11F	73	8	5
	0.15 - 0.5	0.25A	2D	43	8F	40	5	4
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.15	0.24B	0.05B
	0.15 - 0.5	0.16B	0.03B

	Project Name:	WAGGA WAGGA SOIL LANDSCAPES             
	Project Code:	1000448	Site ID:	WW262	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Analyses Completed for this profile
	15F1_CA	Exchangeable bases by 0.01M silver-thiourea (AgTU)+, no pretreatment for soluble salts
	15F1_K	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_MG	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_NA	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F2	Exchangeable aluminium by 0.01m (AgTU)+
	15F3	CEC by 0.01M silver-thiourea (AgTU)+
	3A1	EC of 1:5 soil/water extract
	4B1	pH of 1:5 soil/0.01M calcium chloride extract - direct
	6A1	Organic carbon - Walkley and Black
	9E	Available P (mg/kg) - Bray P
	9J2	Phosphate sorption curve - automated colour
	P10_GRAV	Gravel (%)
	P10_HYD_C	Clay (%) - Hydrometer Method
	P10_HYD_CS	Coarse Sand (%) - Hydrometer Method
	P10_HYD_FS	Fine Sand (%) - Hydrometer Method
	P10_HYD_Z	Silt (%) - Hydrometer Method
	P3B_GV_01	0.1 BAR Moisture g/g - Gravimetric  using suction plate
	P3B_GV_15	15 BAR Moisture g/g - Gravimetric using pressure plate