Project Name:	WAGGA WAGGA SOIL LANDSCAPES             
	Project Code:	1000448	Site ID:	WW284	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Site Information
	Desc. By:	Chen, XY	Locality:
	Date Desc.:	15/07/93	Elevation:	424 metres
	Map Ref.:	Sheet No. : 8327   1:25000	Rainfall:	No Data
	Northing/Long.:	6096150 AMG zone: 55	Runoff:	Slow
	Easting/Lat.:	534125  Datum: AGD66	Drainage:	Moderately well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	Probable
	Geol. Ref.:	Sgf	Substrate Material:	Adamellite 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	Low hills
	Morph. Type:	Crest	Relief:	No Data
	Elem. Type:	Hillcrest	Slope Category:	No Data
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Red Rudosol Medium Gravelly Loamy  	Principal Profile Form:	Dy2.61
	ASC Confidence:	Great Soil Group:	Yellow podzolic soil
	Confidence level not specified
	Site Disturbance:	Complete clearing. Pasture, native or improved, but never cultivated
	Vegetation:
	Surface Coarse Fragments:	2-10%, fine gravelly, 2-6mm, subangular, Quartz
	Profile Morphology
	A1	0 - 0.08 m	Brown (7.5YR4/3-Moist); ; Coarse sandy clay loam; Massive grade of structure; Earthy fabric; 
	Common (1-5 per 100mm2) Very fine (0.075-1mm) macropores, Common (1-5 per 100mm2) Fine
	 (1-2mm) macropores, Dry; Weak consistence; Slightly plastic; Moderately sticky; 10-20%, fine 
	gravelly, 2-6mm, subangular, dispersed, Quartz, coarse fragments; Field pH 5.5 (Raupach); 
	Common, fine (1-2mm) roots; Clear change to - 
	A2	0.08 - 0.2 m	Strong brown (7.5YR4/6-Moist); Reddish yellow (7.5YR6/6-Dry); ; Clay loam, sandy; Massive 
	grade of structure; Earthy fabric; Common (1-5 per 100mm2) Very fine (0.075-1mm) macropores, 
	Common (1-5 per 100mm2) Fine (1-2mm) macropores, Dry; Firm consistence; Moderately 
	plastic; Moderately sticky; 20-50%, fine gravelly, 2-6mm, subangular, dispersed, Quartz, coarse 
	fragments; Field pH 5.5 (Raupach); Few, fine (1-2mm) roots; Clear change to - 
	B2	0.2 - 0.6 m	Yellowish red (5YR5/8-Moist); ; Coarse sandy light medium clay; Weak grade of structure, 2-5 
	mm, Polyhedral; Earthy fabric; Common (1-5 per 100mm2) Very fine (0.075-1mm) macropores, 
	Few (<1 per 100mm2) Fine (1-2mm) macropores, Dry; Firm consistence; Moderately plastic; Very
	 sticky; 20-50%, fine gravelly, 2-6mm, subangular, dispersed, Adamellite, coarse fragments; 
	Field pH 5 (Raupach); Few, fine (1-2mm) roots; Gradual change to - 
	BC	0.6 - 0.85 m	Light reddish brown (5YR6/4-Moist); Mottles, 10-20% , Distinct; Coarse sandy medium clay; 
	Weak grade of structure, 20-50 mm, Subangular blocky; Earthy fabric; Few (<1 per 100mm2) 
	Very fine (0.075-1mm) macropores, Few (<1 per 100mm2) Fine (1-2mm) macropores, Moderately 
	moist; Firm consistence; Moderately plastic; Very sticky; 20-50%, fine gravelly, 2-6mm, 
	subangular, dispersed, Adamellite, coarse fragments; Few cutans, <10% of ped faces or walls 
	coated, faint; Field pH 5 (Raupach); 
	Morphological Notes
	Observation Notes
	Pit to 30cm, auger to 90cm.                                                                                                                                                               
	              
	Site Notes

	Project Name:	WAGGA WAGGA SOIL LANDSCAPES             
	Project Code:	1000448	Site ID:	WW284	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.08	4.5B	0.04A	1.3J	0.7	0.6	0.6	0.2L	4.3I	13.95
	0.08 - 0.2	4B	0.03A	0.8J	0.7	0.3	0.3	0.5L	5.4I	5.56
	0.2 - 0.6	3.7B	0.03A	0.6J	1.1	0.6	0.3	3.2L	6.4I	4.69
	0.6 - 0.85	3.5B	0.03A	1.3J	3	0.5	1.1	4.7L	9.1I	12.09
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.08	2A	15D	7	37F	33	13	10
	0.08 - 0.2	0.89A	2D	4	28F	34	14	20
	0.2 - 0.6	0.51A	1D	7	23F	13	8	49
	0.6 - 0.85	0.15A	1D	15	19F	14	11	41
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.08	0.28B	0.07B
	0.08 - 0.2	0.27B	0.09B
	0.2 - 0.6	0.46B	0.2B
	0.6 - 0.85	0.42B	0.19B

	Project Name:	WAGGA WAGGA SOIL LANDSCAPES             
	Project Code:	1000448	Site ID:	WW284	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Analyses Completed for this profile
	15F1_CA	Exchangeable bases by 0.01M silver-thiourea (AgTU)+, no pretreatment for soluble salts
	15F1_K	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_MG	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_NA	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F2	Exchangeable aluminium by 0.01m (AgTU)+
	15F3	CEC by 0.01M silver-thiourea (AgTU)+
	3A1	EC of 1:5 soil/water extract
	4B1	pH of 1:5 soil/0.01M calcium chloride extract - direct
	6A1	Organic carbon - Walkley and Black
	9E	Available P (mg/kg) - Bray P
	9J2	Phosphate sorption curve - automated colour
	P10_GRAV	Gravel (%)
	P10_HYD_C	Clay (%) - Hydrometer Method
	P10_HYD_CS	Coarse Sand (%) - Hydrometer Method
	P10_HYD_FS	Fine Sand (%) - Hydrometer Method
	P10_HYD_Z	Silt (%) - Hydrometer Method
	P3B_GV_01	0.1 BAR Moisture g/g - Gravimetric  using suction plate
	P3B_GV_15	15 BAR Moisture g/g - Gravimetric using pressure plate