Project Name:	WAGGA WAGGA SOIL LANDSCAPES             
	Project Code:	1000448	Site ID:	WW295	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Site Information
	Desc. By:	Chen, XY	Locality:
	Date Desc.:	15/07/93	Elevation:	207 metres
	Map Ref.:	Sheet No. : 8327   1:25000	Rainfall:	No Data
	Northing/Long.:	6091250 AMG zone: 55	Runoff:	Slow
	Easting/Lat.:	504125  Datum: AGD66	Drainage:	Imperfectly drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	Cza	Substrate Material:	Sand 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	Pediment
	Morph. Type:	Lower-slope	Relief:	No Data
	Elem. Type:	Footslope	Slope Category:	No Data
	Slope:	4 % 	Aspect:	315 degrees
	Surface Soil Condition (dry):	Hardsetting
	Erosion:	Stable, Minor (gully) 
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 N/A    	Principal Profile Form:	Db1.42
	ASC Confidence:	Great Soil Group:	N/A
	Confidence level not specified
	Site Disturbance:	Complete clearing. Pasture, native or improved, but never cultivated
	Vegetation:
	Surface Coarse Fragments:
	Profile Morphology
	A1	0 - 0.15 m	Dark brown (7.5YR3/4-Moist); ; Fine sandy clay loam; Massive grade of structure; Earthy fabric; 
	Common (1-5 per 100mm2) Very fine (0.075-1mm) macropores, Few (<1 per 100mm2) Fine (1-
	2mm) macropores, Dry; Weak consistence; Slightly plastic; Moderately sticky; Field pH 5.5 
	(Raupach); Common, fine (1-2mm) roots; Gradual change to - 
	A2	0.15 - 0.22 m	Reddish brown (5YR4/4-Moist); Pink (7.5YR7/4-Dry); Mottles, 10-20% , Faint; Fine sandy loam; 
	Massive grade of structure; Earthy fabric; Common (1-5 per 100mm2) Very fine (0.075-1mm) 
	macropores, Few (<1 per 100mm2) Fine (1-2mm) macropores, Dry; Firm consistence; Non-
	plastic; Slightly sticky; Field pH 6 (Raupach); Few, fine (1-2mm) roots; Clear change to - 
	B	0.22 - 0.6 m	Brown (7.5YR4/4-Moist); Mottles, 2-10% , Faint; Light medium clay; Moderate grade of structure, 
	20-50 mm, Angular blocky; Smooth-ped fabric; Fine, (0 - 5) mm crack; Few (<1 per 100mm2) 
	Very fine (0.075-1mm) macropores, Dry; Strong consistence; Moderately plastic; Very sticky; 0-
	2%, fine gravelly, 2-6mm, subangular, dispersed, coarse fragments; Field pH 7 (Raupach); Few, 
	fine (1-2mm) roots; 
	Morphological Notes
	B	A few sandstone pieces.                                                                                                      
	                                                                           
	Observation Notes
	Site Notes

	Project Name:	WAGGA WAGGA SOIL LANDSCAPES             
	Project Code:	1000448	Site ID:	WW295	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.15	4.5B	0.1A	3J	1	0.8	0.4	0.5L	4I	10.00
	0.15 - 0.22	5.2B	0.03A	1.5J	1	0.3	0.4	0L	6.4I	6.25
	0.22 - 0.6	6.1B	0.06A	5.7J	7.1	0.9	1.6	0L	16.8I	9.52
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.15	1.79A	8D	2F	74	15	9
	0.15 - 0.22	0.2A	1D	1	9F	71	9	10
	0.22 - 0.6	0.22A	0D	9	8F	42	8	33
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.15	0.43B	0.07B
	0.15 - 0.22	0.18B	0.03B
	0.22 - 0.6	0.44B	0.18B

	Project Name:	WAGGA WAGGA SOIL LANDSCAPES             
	Project Code:	1000448	Site ID:	WW295	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Analyses Completed for this profile
	15F1_CA	Exchangeable bases by 0.01M silver-thiourea (AgTU)+, no pretreatment for soluble salts
	15F1_K	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_MG	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_NA	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F2	Exchangeable aluminium by 0.01m (AgTU)+
	15F3	CEC by 0.01M silver-thiourea (AgTU)+
	3A1	EC of 1:5 soil/water extract
	4B1	pH of 1:5 soil/0.01M calcium chloride extract - direct
	6A1	Organic carbon - Walkley and Black
	9E	Available P (mg/kg) - Bray P
	9J2	Phosphate sorption curve - automated colour
	P10_GRAV	Gravel (%)
	P10_HYD_C	Clay (%) - Hydrometer Method
	P10_HYD_CS	Coarse Sand (%) - Hydrometer Method
	P10_HYD_FS	Fine Sand (%) - Hydrometer Method
	P10_HYD_Z	Silt (%) - Hydrometer Method
	P3B_GV_01	0.1 BAR Moisture g/g - Gravimetric  using suction plate
	P3B_GV_15	15 BAR Moisture g/g - Gravimetric using pressure plate