Project Name:	WAGGA WAGGA SOIL LANDSCAPES             
	Project Code:	1000448	Site ID:	WW5	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Site Information
	Desc. By:	Chen, XY	Locality:
	Date Desc.:	15/07/93	Elevation:	275 metres
	Map Ref.:	Sheet No. : 8327   1:25000	Rainfall:	No Data
	Northing/Long.:	6124900 AMG zone: 55	Runoff:	Slow
	Easting/Lat.:	538050  Datum: AGD66	Drainage:	Moderately well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	Probable
	Geol. Ref.:	Sgw	Substrate Material:	Granodiorite 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	Low hills
	Morph. Type:	Mid-slope	Relief:	No Data
	Elem. Type:	Hillslope	Slope Category:	No Data
	Slope:	15 % 	Aspect:	270 degrees
	Surface Soil Condition (dry):	Firm
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 N/A    	Principal Profile Form:	Gn2.12
	ASC Confidence:	Great Soil Group:	Red earth
	Confidence level not specified
	Site Disturbance:	Complete clearing. Pasture, native or improved, cultivated at some stage
	Vegetation:
	Surface Coarse Fragments:
	Profile Morphology
	A	0 - 0.2 m	Dark brown (7.5YR3/4-Moist); ; Medium sandy clay loam; Weak grade of structure, 2-5 mm, 
	Granular; Earthy fabric; Moderately moist; Non-plastic; Slightly sticky; 2-10%, fine gravelly, 2-
	6mm, subrounded, dispersed, Quartz, coarse fragments; Field pH 5.5 (Raupach); Many, very fine
	 (0-1mm) roots; Diffuse change to - 
	B	0.2 - 0.6 m	Yellowish red (5YR3/6-Moist); ; Medium clay; Weak grade of structure, 50-100 mm, Prismatic; 
	Earthy fabric; Moderately moist; Very plastic; Slightly sticky; 10-20%, fine gravelly, 2-6mm, 
	subrounded, dispersed, Quartz, coarse fragments; Field pH 6 (Raupach); Common, very fine (0-
	1mm) roots; Gradual change to - 
	BC	0.6 - 0.8 m	Yellowish brown (10YR5/6-Moist); Mottles, 2-10% , Faint; Medium heavy clay; Earthy fabric; 
	Moderately moist; Very plastic; Very sticky; 2-10%, fine gravelly, 2-6mm, subrounded, dispersed,
	 Quartz, coarse fragments; Very few (0 - 2 %), Manganiferous, Medium (2 -6 mm), Soft 
	segregations, weak, segregations;Field pH 6.5 (Raupach); Few, very fine (0-1mm) roots; 
	Morphological Notes
	Observation Notes
	Site Notes
	15M N OF TRACK                        

	Project Name:	WAGGA WAGGA SOIL LANDSCAPES             
	Project Code:	1000448	Site ID:	WW5	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.2	5.4B	0.05A	2.5J	1	0.6	0.3	0L	5.7I	5.26
	0.2 - 0.6	5.5B	0.03A	2.6J	2.1	0.6	0.5	0L	9.5I	5.26
	0.6 - 0.8	5.8B	0.04A	4.7J	6.8	0.7	0.6	0L	10.4I	5.77
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.2	1.35A	1D	2	33F	46	11	8
	0.2 - 0.6	0.38A	0D	3	43F	22	5	27
	0.6 - 0.8	0.25A	0D	3	34F	8	7	48
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.2	0.21B	0.04B
	0.2 - 0.6	0.27B	0.11B
	0.6 - 0.8	0.39B	0.19B

	Project Name:	WAGGA WAGGA SOIL LANDSCAPES             
	Project Code:	1000448	Site ID:	WW5	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Analyses Completed for this profile
	15F1_CA	Exchangeable bases by 0.01M silver-thiourea (AgTU)+, no pretreatment for soluble salts
	15F1_K	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_MG	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_NA	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F2	Exchangeable aluminium by 0.01m (AgTU)+
	15F3	CEC by 0.01M silver-thiourea (AgTU)+
	3A1	EC of 1:5 soil/water extract
	4B1	pH of 1:5 soil/0.01M calcium chloride extract - direct
	6A1	Organic carbon - Walkley and Black
	9E	Available P (mg/kg) - Bray P
	9J2	Phosphate sorption curve - automated colour
	P10_GRAV	Gravel (%)
	P10_HYD_C	Clay (%) - Hydrometer Method
	P10_HYD_CS	Coarse Sand (%) - Hydrometer Method
	P10_HYD_FS	Fine Sand (%) - Hydrometer Method
	P10_HYD_Z	Silt (%) - Hydrometer Method
	P3B_GV_01	0.1 BAR Moisture g/g - Gravimetric  using suction plate
	P3B_GV_15	15 BAR Moisture g/g - Gravimetric using pressure plate