Project Name:	EDEN BURNING STUDY AREA                 
	Project Code:	1000638	Site ID:	EDB_SA28	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Site Information
	Desc. By:	P. Ryan	Locality:
	Date Desc.:	19/07/87	Elevation:	230 metres
	Map Ref.:	Sheet No. : 8823   1:25000	Rainfall:	No Data
	Northing/Long.:	5876670 AMG zone: 55	Runoff:	No Data
	Easting/Lat.:	735120  Datum: AGD66	Drainage:	Imperfectly drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	Probable
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	No Data
	Morph. Type:	Upper-slope	Relief:	0 metres
	Elem. Type:	Hillslope	Slope Category:	No Data
	Slope:	12 % 	Aspect:	0 degrees
	Surface Soil Condition (dry):	Loose
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 N/A    	Principal Profile Form:	Gn1.34
	ASC Confidence:	Great Soil Group:	Yellow podzolic soil
	Confidence level not specified
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:
	Surface Coarse Fragments:	; No surface coarse fragments; 10-20%, fine gravelly, 2-6mm, subangular, Quartz
	Profile Morphology
	O1	0 - 0.01 m	Organic Layer; ; Coarse sandy clay loam; Wet; Clear, Smooth change to - 
	A1	0.01 - 0.09 m	Very dark grey (10YR3/1-Moist); ; Coarse sandy clay loam; Weak grade of structure, 2-5 mm, 
	Granular; Earthy fabric; Wet; Weak consistence; 10-20%, fine gravelly, 2-6mm, subangular, 
	dispersed, Quartz, coarse fragments; Field pH 5.5 (Raupach); Many, medium (2-5mm) roots; 
	Many, coarse (>5mm) roots; Clear, Smooth change to - 
	A2c	0.09 - 0.18 m	Very pale brown (10YR7/3-Moist); ; Coarse sandy clay loam; Weak grade of structure, 10-20 mm,
	 Polyhedral; Earthy fabric; Wet; Weak consistence; 10-20%, fine gravelly, 2-6mm, subangular, 
	dispersed, Quartz, coarse fragments; Field pH 5 (Raupach); Many, medium (2-5mm) roots; Many,
	 coarse (>5mm) roots; Gradual, Wavy change to - 
	B21	0.18 - 0.31 m	Light yellowish brown (10YR6/4-Moist); ; Coarse sandy clay loam; Weak grade of structure, 10-
	20 mm, Polyhedral; Earthy fabric; Wet; Weak consistence; 10-20%, fine gravelly, 2-6mm, 
	subangular, dispersed, Quartz, coarse fragments; Field pH 5.5 (Raupach); Common, coarse 
	(>5mm) roots; Clear, Smooth change to - 
	B22	0.31 - 0.57 m	Brownish yellow (10YR6/6-Moist); , 10-20% , Distinct; , 10-20% , Distinct; Coarse sandy clay; 
	Sandy (grains prominent) fabric; Wet; Firm consistence; 10-20%, fine gravelly, 2-6mm, 
	subangular, dispersed, Quartz, coarse fragments; Field pH 5.5 (Raupach); Few, fine (1-2mm) 
	roots; 
	B3	0.57 - 0.78 m	Brownish yellow (10YR6/6-Moist); ; Firm consistence; 10-20%, fine gravelly, 2-6mm, subangular,
	 reoriented, Quartz, coarse fragments; Field pH 5.5 (Raupach); 
	Morphological Notes
	A2c	Also angular blocky dominant ped shape.                                                                           
	                                                                                      
	B22	B3 horizon is mottled & distinctly      higher in clay.                                                            
	                                                                                     
	Observation Notes
	Upper slope of spur ridge.                                                                                                                                                                  
	            
	Site Notes

	Project Name:	EDEN BURNING STUDY AREA                 
	Project Code:	1000638	Site ID:	EDB_SA28	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	DP8                                   

	Project Name:	EDEN BURNING STUDY AREA                 
	Project Code:	1000638	Site ID:	EDB_SA28	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0.01 - 0.09	3.81I	1.88F	0.94	0.15	0.11	0.37G
	4.86H
	0.09 - 0.18	3.54I	0.43F	0.39	0.12	0.1	0.82G
	4.74H
	0.31 - 0.39	3.95I	0.43F	0.18	0.17	0.13	0.67G
	5.29H
	0.57 - 0.78	3.63I	0.01F	2.3	0.08	0.58	1.63G
	5.14H
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0.01 - 0.09	4.72A	31F	<0.01E	19.8
	0.09 - 0.18	1.74A	17F	<0.01E	15.3
	0.31 - 0.39	0.93A	18F	<0.01E	29.9
	0.57 - 0.78	0.8A	13F	<0.01E	25.8
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0.01 - 0.09
	0.09 - 0.18
	0.31 - 0.39
	0.57 - 0.78

	Project Name:	EDEN BURNING STUDY AREA                 
	Project Code:	1000638	Site ID:	EDB_SA28	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Analyses Completed for this profile
	15D1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium acetate at pH 7.0, pretreatment for 
	soluble salts; manual leach
	15D1_K	Exchangeable bases and CEC - 1M ammonium acetate at pH 7.0, pretreatment for soluble salts; 
	manual leach
	15D1_MG	Exchangeable bases and CEC - 1M ammonium acetate at pH 7.0, pretreatment for soluble salts; 
	manual leach
	15D1_NA	Exchangeable bases and CEC - 1M ammonium acetate at pH 7.0, pretreatment for soluble salts; 
	manual leach
	15G_C_AL2	Exchangeable aluminium - meq per 100g of soil - Aluminium By KCl extraction and detremination By
	 AAS
	2A1	Air-dry moisture content
	4A_C_1	pH of soil - pH of 1:1 soil/water suspension
	4C_C_1	pH of 1:1 soil/1M potassium chloride suspension
	6A1	Organic carbon - Walkley and Black
	7A1	Total nitrogen - semimicro Kjeldahl, steam distillation
	9A_NR	Total element - P(%) - Not recorded
	P10_GRAV	Gravel (%)