Project Name:	EDEN BURNING STUDY AREA                 
	Project Code:	1000638	Site ID:	EDB_SA34	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Site Information
	Desc. By:	P. Ryan	Locality:
	Date Desc.:	01/09/87	Elevation:	340 metres
	Map Ref.:	Sheet No. : 8823   1:25000	Rainfall:	No Data
	Northing/Long.:	5878520 AMG zone: 55	Runoff:	No Data
	Easting/Lat.:	734430  Datum: AGD66	Drainage:	Well drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	Probable
	Geol. Ref.:	Dgwa	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	No Data
	Morph. Type:	Mid-slope	Relief:	0 metres
	Elem. Type:	Hillslope	Slope Category:	No Data
	Slope:	18 % 	Aspect:	45 degrees
	Surface Soil Condition (dry):	Loose
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 N/A    	Principal Profile Form:	Gn2.21
	ASC Confidence:	Great Soil Group:	Brown earth
	Confidence level not specified
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:
	Surface Coarse Fragments:	10-20%, medium gravelly, 6-20mm, subangular, ; No surface coarse fragments
	Profile Morphology
	O1	0 - 0.02 m	Organic Layer; ; Coarse sandy loam; Clear, Wavy change to - 
	A1	0.02 - 0.17 m	Brown (7.5YR4/4-Moist); ; Coarse sandy loam; Weak grade of structure, 5-10 mm, Polyhedral; <2
	 mm, Granular; Earthy fabric; Weak consistence; 20-50%, medium gravelly, 6-20mm, 
	subangular, dispersed, coarse fragments; Field pH 5.5 (Raupach); Many, fine (1-2mm) roots; 
	Many, medium (2-5mm) roots; Many, coarse (>5mm) roots; Gradual, Irregular change to - 
	B21	0.17 - 0.52 m	Strong brown (7.5YR5/8-Moist); ; Coarse sandy clay loam; Weak grade of structure, 5-10 mm, 
	Polyhedral; Earthy fabric; Weak consistence; 20-50%, medium gravelly, 6-20mm, subangular, 
	dispersed, coarse fragments; 20-50%, cobbly, 60-200mm, subangular, dispersed, coarse 
	fragments; Field pH 5.5 (Raupach); Common, fine (1-2mm) roots; Common, medium (2-5mm) 
	roots; Gradual, Irregular change to - 
	B22	0.52 - 0.69 m	Reddish yellow (7.5YR6/8-Moist); ; Weak grade of structure, 2-5 mm, Granular; Earthy fabric; 
	Weak consistence; 20-50%, medium gravelly, 6-20mm, subangular, reoriented, coarse 
	fragments; 20-50%, cobbly, 60-200mm, subangular, reoriented, coarse fragments; Field pH 4.5 
	(Raupach); Few, medium (2-5mm) roots; Few, coarse (>5mm) roots; Abrupt, Smooth change to - 
	Cr	0.69 - 0.78 m	; 20-50%, medium gravelly, 6-20mm, subangular, undisturbed, coarse fragments; 20-50%, 
	cobbly, 60-200mm, subangular, undisturbed, coarse fragments; 
	Morphological Notes
	Observation Notes
	Shallow soil. PM present as surface     sheet. Sarub vegetation reflects this.  Little profile development.             Current surface 
	condition = water       repellent.                              
	Site Notes
	DP91                                  

	Project Name:	EDEN BURNING STUDY AREA                 
	Project Code:	1000638	Site ID:	EDB_SA34	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0.02 - 0.1	4I	0.66F	1.89	0.33	0.08	0.71G
	5.28H
	0.32 - 0.4	4.16I	3.48F	1.36	0.45	0.13	0.27G
	5.44H
	0.52 - 0.69	3.8I	0.52F	1.37	0.59	2.38	3.58G
	4.92H
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0.02 - 0.1	2.03A	26F	<0.01E	26.7
	0.32 - 0.4	6.34A	52F	<0.01E	19.9
	0.52 - 0.69	1.35A	39F	<0.01E	44
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0.02 - 0.1
	0.32 - 0.4
	0.52 - 0.69

	Project Name:	EDEN BURNING STUDY AREA                 
	Project Code:	1000638	Site ID:	EDB_SA34	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Analyses Completed for this profile
	15D1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium acetate at pH 7.0, pretreatment for 
	soluble salts; manual leach
	15D1_K	Exchangeable bases and CEC - 1M ammonium acetate at pH 7.0, pretreatment for soluble salts; 
	manual leach
	15D1_MG	Exchangeable bases and CEC - 1M ammonium acetate at pH 7.0, pretreatment for soluble salts; 
	manual leach
	15D1_NA	Exchangeable bases and CEC - 1M ammonium acetate at pH 7.0, pretreatment for soluble salts; 
	manual leach
	15G_C_AL2	Exchangeable aluminium - meq per 100g of soil - Aluminium By KCl extraction and detremination By
	 AAS
	2A1	Air-dry moisture content
	4A_C_1	pH of soil - pH of 1:1 soil/water suspension
	4C_C_1	pH of 1:1 soil/1M potassium chloride suspension
	6A1	Organic carbon - Walkley and Black
	7A1	Total nitrogen - semimicro Kjeldahl, steam distillation
	9A_NR	Total element - P(%) - Not recorded
	P10_GRAV	Gravel (%)