Project Name:	EDEN BURNING STUDY AREA                 
	Project Code:	1000638	Site ID:	EDB_SA39	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Site Information
	Desc. By:	P. Ryan	Locality:
	Date Desc.:	02/09/87	Elevation:	280 metres
	Map Ref.:	Sheet No. : 8823   1:25000	Rainfall:	No Data
	Northing/Long.:	5877490 AMG zone: 55	Runoff:	No Data
	Easting/Lat.:	733720  Datum: AGD66	Drainage:	Well drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	Dgwa	Substrate Material:	Sand 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	No Data
	Morph. Type:	Mid-slope	Relief:	0 metres
	Elem. Type:	Hillslope	Slope Category:	No Data
	Slope:	36 % 	Aspect:	180 degrees
	Surface Soil Condition (dry):	Loose
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 N/A    	Principal Profile Form:	Gn2.21
	ASC Confidence:	Great Soil Group:	Brown earth
	Confidence level not specified
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:
	Surface Coarse Fragments:	20-50%, fine gravelly, 2-6mm, subangular, Sand; 20-50%, coarse gravelly, 20-60mm, subangular, Sand; No surface 
	coarse fragments
	Profile Morphology
	A1	0 - 0.17 m	Dark greyish brown (10YR4/2-Moist); ; Clay loam; Moderate grade of structure, 5-10 mm, 
	Polyhedral; Rough-ped fabric; Moist; Firm consistence; 20-50%, fine gravelly, 2-6mm, 
	subangular, dispersed, Quartz, coarse fragments; Few (2 - 10 %), Ferruginous, Coarse (6 - 20 
	mm), Nodules, strong, segregations;Field pH 4.5 (Raupach); Many, medium (2-5mm) roots; 
	Many, coarse (>5mm) roots; Gradual, Irregular change to - 
	B1	0.17 - 0.4 m	Yellowish brown (10YR5/4-Moist); ; Coarse sandy clay loam; Weak grade of structure, 10-20 
	mm, Polyhedral; Earthy fabric; Moist; Weak consistence; 20-50%, fine gravelly, 2-6mm, 
	subangular, dispersed, Quartz, coarse fragments; Common (10 - 20 %), Ferruginous, Coarse (6 -
	 20 mm), Nodules, strong, segregations;Field pH 5.5 (Raupach); Common, fine (1-2mm) roots; 
	Common, coarse (>5mm) roots; Diffuse, Irregular change to - 
	B2	0.4 - 0.8 m	Yellowish brown (10YR5/6-Moist); ; Coarse sandy clay loam; Weak grade of structure, 10-20 
	mm, Polyhedral; Earthy fabric; Moist; Weak consistence; 20-50%, fine gravelly, 2-6mm, 
	subangular, dispersed, Quartz, coarse fragments; Few (2 - 10 %), Ferruginous, Coarse (6 - 20 
	mm), Nodules, strong, segregations;Field pH 5.5 (Raupach); Common, medium (2-5mm) roots; 
	Abrupt, Wavy change to - 
	Morphological Notes
	A1	Fine sand fraction.                     Higher faunal activity (casts) & fine   texture like YA37.    
	                                                                                                  
	B2	Dispersive.                                                                                                                            
	                                                                 
	Observation Notes
	Below torfield, tor as substrate. As F  or YA38, Fe nodules in profile. One     contained charcoal.                                                  
	                                                   
	Site Notes
	DP81 - ridgeline.                     

	Project Name:	EDEN BURNING STUDY AREA                 
	Project Code:	1000638	Site ID:	EDB_SA39	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.075	3.63I	1.21F	0.76	0.18	0.13	1.05G
	4.65H
	0.3 - 0.38	3.89I	0.14F	0.19	0.12	0.07	1.07G
	4.92H
	0.4 - 0.8	4.11I	0.2F	0.56	0.23	0.05	0.39G
	5.53H
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.075	3.76A	30F	<0.01E	13.3	57.1F	22.8	16.6	3.5
	0.3 - 0.38	1.13A	21F	<0.01E	21	53.7F	21.2	14.3	10.8
	0.4 - 0.8	0.63A	19F	<0.01E	23.1	53.3F	20.8	15.1	10.8
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.075
	0.3 - 0.38
	0.4 - 0.8

	Project Name:	EDEN BURNING STUDY AREA                 
	Project Code:	1000638	Site ID:	EDB_SA39	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Analyses Completed for this profile
	15D1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium acetate at pH 7.0, pretreatment for 
	soluble salts; manual leach
	15D1_K	Exchangeable bases and CEC - 1M ammonium acetate at pH 7.0, pretreatment for soluble salts; 
	manual leach
	15D1_MG	Exchangeable bases and CEC - 1M ammonium acetate at pH 7.0, pretreatment for soluble salts; 
	manual leach
	15D1_NA	Exchangeable bases and CEC - 1M ammonium acetate at pH 7.0, pretreatment for soluble salts; 
	manual leach
	15G_C_AL2	Exchangeable aluminium - meq per 100g of soil - Aluminium By KCl extraction and detremination By
	 AAS
	4A_C_1	pH of soil - pH of 1:1 soil/water suspension
	4C_C_1	pH of 1:1 soil/1M potassium chloride suspension
	6A1	Organic carbon - Walkley and Black
	7A1	Total nitrogen - semimicro Kjeldahl, steam distillation
	9A_NR	Total element - P(%) - Not recorded
	P10_GRAV	Gravel (%)
	P10_HYD_C	Clay (%) - Hydrometer Method
	P10_HYD_CS	Coarse Sand (%) - Hydrometer Method
	P10_HYD_FS	Fine Sand (%) - Hydrometer Method
	P10_HYD_Z	Silt (%) - Hydrometer Method