Project Name:	EDEN BURNING STUDY AREA                 
	Project Code:	1000638	Site ID:	EDB_SA59	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Site Information
	Desc. By:	P. Ryan	Locality:
	Date Desc.:	01/09/87	Elevation:	280 metres
	Map Ref.:	Sheet No. : 8823   1:25000	Rainfall:	No Data
	Northing/Long.:	5877940 AMG zone: 55	Runoff:	No Data
	Easting/Lat.:	735420  Datum: AGD66	Drainage:	Imperfectly drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Sand 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	No Data
	Morph. Type:	Open depression (vale)	Relief:	0 metres
	Elem. Type:	Drainage depression	Slope Category:	No Data
	Slope:	5 % 	Aspect:	270 degrees
	Surface Soil Condition (dry):	Firm
	Erosion:	Partial, Minor (gully) 
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 N/A    	Principal Profile Form:	Gn1.84
	ASC Confidence:	Great Soil Group:	Humic gley
	Confidence level not specified
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:
	Surface Coarse Fragments:	50-90%, fine gravelly, 2-6mm, subangular, Quartz; No surface coarse fragments
	Profile Morphology
	A11	0 - 0.15 m	; Coarse sandy clay loam; Moderate grade of structure, 10-20 mm, Polyhedral; Rough-ped fabric;
	 Moist; Weak consistence; 50-90%, fine gravelly, 2-6mm, subangular, dispersed, Quartz, coarse 
	fragments; 50-90%, medium gravelly, 6-20mm, subangular, dispersed, Quartz, coarse 
	fragments; 50-90%, fine gravelly, 2-6mm, angular, dispersed, Quartz, coarse fragments; Field pH
	 5.5 (Raupach); Many, coarse (>5mm) roots; Many, medium (2-5mm) roots; Many, fine (1-2mm) 
	roots; Many, very fine (0-1mm) roots; Gradual, Wavy change to - 
	A12	0.15 - 0.4 m	Very dark grey (10YR3/1-Moist); ; Clay loam; Moderate grade of structure, 10-20 mm, Polyhedral; 
	Rough-ped fabric; Moist; Firm consistence; 50-90%, fine gravelly, 2-6mm, subangular, 
	dispersed, Quartz, coarse fragments; 50-90%, medium gravelly, 6-20mm, subangular, 
	dispersed, Quartz, coarse fragments; 50-90%, fine gravelly, 2-6mm, angular, dispersed, Quartz, 
	coarse fragments; Field pH 5.5 (Raupach); Common, very fine (0-1mm) roots; Common, fine (1-
	2mm) roots; Gradual, Irregular change to - 
	A13	0.4 - 0.53 m	Dark greyish brown (10YR4/2-Moist); ; Coarse sandy clay loam; Moderate grade of structure, 20-
	50 mm, Subangular blocky; Rough-ped fabric; Moist; Firm consistence; 50-90%, fine gravelly, 2-
	6mm, subangular, dispersed, Quartz, coarse fragments; 50-90%, medium gravelly, 6-20mm, 
	subangular, dispersed, Quartz, coarse fragments; 50-90%, fine gravelly, 2-6mm, angular, 
	dispersed, Quartz, coarse fragments; Few cutans, <10% of ped faces or walls coated, faint; 
	Field pH 5.5 (Raupach); Common, very fine (0-1mm) roots; Common, fine (1-2mm) roots; Clear, 
	Irregular change to - 
	A2	0.53 - 0.72 m	Greyish brown (10YR5/2-Moist); ; Coarse sandy clay loam; Weak grade of structure, 20-50 mm, 
	Subangular blocky; Earthy fabric; Moist; Firm consistence; 50-90%, fine gravelly, 2-6mm, 
	subangular, dispersed, Quartz, coarse fragments; 50-90%, medium gravelly, 6-20mm, 
	subangular, dispersed, Quartz, coarse fragments; 50-90%, fine gravelly, 2-6mm, angular, 
	dispersed, Quartz, coarse fragments; Few cutans, <10% of ped faces or walls coated, faint; 
	Field pH 5.5 (Raupach); Common, very fine (0-1mm) roots; Common, fine (1-2mm) roots; 
	Gradual, Wavy change to - 
	B2	0.72 - 1.05 m	Light yellowish brown (10YR6/4-Moist); , 20-50% , Distinct; , 10-20% , Faint; Coarse sandy clay 
	loam; Massive grade of structure; Sandy (grains prominent) fabric; Moist; Very firm consistence; 
	50-90%, fine gravelly, 2-6mm, subangular, dispersed, Quartz, coarse fragments; 50-90%, 
	medium gravelly, 6-20mm, subangular, dispersed, Quartz, coarse fragments; 50-90%, fine 
	gravelly, 2-6mm, angular, dispersed, Quartz, coarse fragments; Field pH 5 (Raupach); Few, fine 
	(1-2mm) roots; Clear, Wavy change to - 
	Morphological Notes

	Project Name:	EDEN BURNING STUDY AREA                 
	Project Code:	1000638	Site ID:	EDB_SA59	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	A11	Moist Munsell = 2.5YR 2/0.                                                                                                   
	                                                                           
	A12	Coarse sand fraction.                                                                                                           
	                                                                        
	Observation Notes
	Flat bottom of drainage line. Thick A   horizon (70cm) over pallid yellow B hor-izon. A horizon colours are varigated.  Charcoal 
	occurs in bands, one at 38cm.                                          
	Site Notes
	DP107 - dry drainage line - convex    

	Project Name:	EDEN BURNING STUDY AREA                 
	Project Code:	1000638	Site ID:	EDB_SA59	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.08	4.1I	1.3F	3.23	0.41	0.15	0.74G
	5.25H
	0.3 - 0.38	3.88I	0.61F	2.21	0.26	0.21	1.04G
	5.03H
	0.53 - 0.72	3.87I	0.28F	1.17	0.16	0.13	0.73G
	5.23H
	0.72 - 1.05	3.73I	0.18F	1.15	0.15	0.1	0.58G
	5.41H
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.08	6.21A	69F	<0.01E	27.7
	0.3 - 0.38	2.58A	37.6F	<0.01E	21.9
	0.53 - 0.72	0.17A	19.5F	<0.01E	29.4
	0.72 - 1.05	0.78A	8.7F	<0.01E	12.7
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.08
	0.3 - 0.38
	0.53 - 0.72
	0.72 - 1.05

	Project Name:	EDEN BURNING STUDY AREA                 
	Project Code:	1000638	Site ID:	EDB_SA59	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Analyses Completed for this profile
	15D1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium acetate at pH 7.0, pretreatment for 
	soluble salts; manual leach
	15D1_K	Exchangeable bases and CEC - 1M ammonium acetate at pH 7.0, pretreatment for soluble salts; 
	manual leach
	15D1_MG	Exchangeable bases and CEC - 1M ammonium acetate at pH 7.0, pretreatment for soluble salts; 
	manual leach
	15D1_NA	Exchangeable bases and CEC - 1M ammonium acetate at pH 7.0, pretreatment for soluble salts; 
	manual leach
	15G_C_AL2	Exchangeable aluminium - meq per 100g of soil - Aluminium By KCl extraction and detremination By
	 AAS
	4A_C_1	pH of soil - pH of 1:1 soil/water suspension
	4C_C_1	pH of 1:1 soil/1M potassium chloride suspension
	6A1	Organic carbon - Walkley and Black
	7A1	Total nitrogen - semimicro Kjeldahl, steam distillation
	9A_NR	Total element - P(%) - Not recorded
	P10_GRAV	Gravel (%)