Project Name:	BAGO-MARAGLE ESM
	Project Code:	BGM_ESM	Site ID:	1009	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Site Information
	Desc. By:	P. Ryan	Locality:
	Date Desc.:	16/12/94	Elevation:	1210 metres
	Map Ref.:	Sheet No. : 8526   DGPS	Rainfall:	No Data
	Northing/Long.:	6044736 AMG zone: 55	Runoff:	Very slow
	Easting/Lat.:	598679  Datum: AGD66	Drainage:	Well drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	Probable
	Geol. Ref.:	SGGH	Substrate Material:	Granodiorite 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	No Data
	Morph. Type:	Upper-slope	Relief:	No Data
	Elem. Type:	Hillslope	Slope Category:	No Data
	Slope:	3 % 	Aspect:	225 degrees
	Surface Soil Condition (dry):	Firm
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Acidic Dystrophic Red Kandosol Thin Non-gravelly Clay-	Principal Profile Form:	Um7.11
	loamy Clay-loamy Deep
	ASC Confidence:	Great Soil Group:	Red earth
	All necessary analytical data are available.
	Site Disturbance:	No effective disturbance. Natural
	Vegetation:
	Surface Coarse Fragments:
	Profile Morphology
	O1	0 - 0.01 m	Organic Layer; ; 
	A1	0.01 - 0.1 m	Dark reddish brown (5YR3/2-Moist); Biological mixing, 2-10% , Faint; Clay loam; Strong grade of 
	structure, 5-10 mm, Polyhedral; 100-200 mm, Lenticular; Rough-ped fabric; Moderately moist; 
	Firm consistence; Slightly plastic; Moderately sticky; Field pH 6 (pH meter); Many, very fine (0-
	1mm) roots; Common, fine (1-2mm) roots; Clear, Smooth change to - 
	A3	0.1 - 0.22 m	Dark reddish brown (5YR3/3-Moist); Biological mixing, 10-20% , Faint; Clay loam, sandy; Strong 
	grade of structure, 5-10 mm, Polyhedral; 100-200 mm, Lenticular; Rough-ped fabric; Moderately 
	moist; Weak consistence; Moderately plastic; Slightly sticky; Field pH 5.5 (pH meter); Common, 
	very fine (0-1mm) roots; Few, fine (1-2mm) roots; Few, medium (2-5mm) roots; Few, coarse 
	(>5mm) roots; Clear, Wavy change to - 
	B21	0.22 - 0.46 m	Dark reddish brown (2.5YR3/4-Moist); Biological mixing, 2-10% , Faint; Clay loam, sandy; 
	Moderate grade of structure, 5-10 mm, Subangular blocky; 100-200 mm, Lenticular; Rough-ped 
	fabric; Moderately moist; Weak consistence; Moderately plastic; Slightly sticky; Field pH 5 (pH 
	meter); Common, very fine (0-1mm) roots; Few, fine (1-2mm) roots; Few, medium (2-5mm) roots; 
	Common, coarse (>5mm) roots; Gradual, Smooth change to - 
	B22	0.46 - 0.81 m	Red (2.5YR4/6-Moist); Biological mixing, 0-2% , Faint; Clay loam, sandy; Massive grade of 
	structure; Earthy fabric; Moderately moist; Weak consistence; Moderately plastic; Slightly sticky;
	 Field pH 5 (pH meter); Few, very fine (0-1mm) roots; Few, fine (1-2mm) roots; Few, medium (2-
	5mm) roots; Diffuse, Smooth change to - 
	B3	0.81 - 1.16 m	Yellowish red (5YR4/6-Moist); ; Coarse sandy clay loam; Massive grade of structure; Earthy 
	fabric; Moderately moist; Weak consistence; Slightly plastic; Slightly sticky; Field pH 5 (pH 
	meter); 
	C	1.16 - 1.41 m	Light yellowish brown (10YR6/4-Moist); ; Clayey coarse sand; Non-plastic; Non-sticky; Field pH 
	6 (pH meter); 
	Morphological Notes
	B3	Muscovite mica common in sand fraction.
	C	Augered to substrate to 1.4m.
	Observation Notes
	Pit located between plots. Ash seedling.Trial planted off-site into predominantly mountain gum forest type.

	Project Name:	BAGO-MARAGLE ESM
	Project Code:	BGM_ESM	Site ID:	1009	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Site Notes
	VI/1.17, ALPINE ASH SPACING TRIAL

	Project Name:	BAGO-MARAGLE ESM
	Project Code:	BGM_ESM	Site ID:	1009	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0.01 - 0.09	4.46C	5.75H	2.25	1	0.09	2.15J	11.24E
	5.25A	0K
	0.11 - 0.21	4.2C	1.6H	1.12	0.66	0.07	2.98J	6.42E
	5.13A	0K
	0.31 - 0.39	3.87C	0.16H	0.58	0.63	0.07	4.09J	5.53E
	4.79A	0K
	0.61 - 0.71	3.77C	0.06H	0.5	0.46	0.07	3.55J	4.64E
	4.78A	0K
	0.91 - 1.01	3.77C	0.04H	0.28	0.36	0.08	2.67J	3.43E
	4.76A	0K
	1.31 - 1.41	4.33C	0.06H	0.05	0.28	0.06	0.33J	0.78E
	5.17A	0K
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0.01 - 0.09	7.24B	867.8B	0.3A	0.95	3.12
	0.11 - 0.21	3.4B	715.5B	0.14A	1.02	0.22
	0.31 - 0.39	1.31B	494B	0.07A	1.20	1.94
	0.61 - 0.71	0.41B	404.7B	0.03A	1.43	0.56
	0.91 - 1.01	0.15B	356.7B	0.02A	1.58	4.66
	1.31 - 1.41	0.14B	492.6B	0.01A	17.96
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0.01 - 0.09
	0.11 - 0.21
	0.31 - 0.39
	0.61 - 0.71
	0.91 - 1.01
	1.31 - 1.41

	Project Name:	BAGO-MARAGLE ESM
	Project Code:	BGM_ESM	Site ID:	1009	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Analyses Completed for this profile
	15_NR	Sum of Ex. cations + Ex. acidity - Not recorded
	15E1_AL	Exchangeable Al - by compulsive exchange, no pretreatment for soluble salts
	15E1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) by compulsive exchange, no pretreatment for soluble 
	15E1_H	Exchangeable H - by compulsive exchange, no pretreatment for soluble salts
	15E1_K	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MG	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_NA	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	2A1	Air-dry moisture content
	4A1	pH of 1:5 soil/water suspension
	4B2	pH of 1:5 soil/0.01M calcium chloride extract - following Method 4A1
	6B2	Total organic carbon - high frequency induction furnace, volumetric
	7A2	Total nitrogen - semimicro Kjeldahl , automated colour
	9A3	Total Phosphorus (ppm) - semimicro kjeldahl, automated colour
	P10_GRAV	Gravel (%)
	P3A1	Bulk density - g/cm3