Project Name:	BAGO-MARAGLE ESM
	Project Code:	BGM_ESM	Site ID:	1020	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Site Information
	Desc. By:	P. Ryan	Locality:
	Date Desc.:	04/04/95	Elevation:	1173 metres
	Map Ref.:	Sheet No. : 8526   DGPS	Rainfall:	No Data
	Northing/Long.:	6053686 AMG zone: 55	Runoff:	Slow
	Easting/Lat.:	609177  Datum: AGD66	Drainage:	Well drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	TB	Substrate Material:	Tuff 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	No Data
	Morph. Type:	Upper-slope	Relief:	No Data
	Elem. Type:	Hillslope	Slope Category:	No Data
	Slope:	12 % 	Aspect:	135 degrees
	Surface Soil Condition (dry):	Self-mulching
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Humose-Acidic Mesotrophic Red Dermosol Medium Non-	Principal Profile Form:	Gn3.11
	gravelly Clay-loamy Clayey Very deep
	ASC Confidence:	Great Soil Group:	Krasnozem
	All necessary analytical data are available.
	Site Disturbance:	No effective disturbance. Natural
	Vegetation:
	Surface Coarse Fragments:
	Profile Morphology
	O1	0 - 0.01 m	Organic Layer; ; 
	A11	0.01 - 0.06 m	Black (5YR2.5/1-Moist); ; Loam; Weak grade of structure, 2-5 mm, Granular; Rough-ped fabric; 
	Dry; Very weak consistence; Field pH 6 (pH meter); Many, very fine (0-1mm) roots; Common, fine 
	(1-2mm) roots; Common, medium (2-5mm) roots; Few, coarse (>5mm) roots; Abrupt, Smooth 
	change to - 
	A12p	0.06 - 0.16 m	Dark reddish brown (5YR3/2-Moist); Mechanical, 2-10% , Distinct; Biological mixing, 2-10% , 
	Faint; Clay loam; Moderate grade of structure, 10-20 mm, Subangular blocky; 100-200 mm, 
	Lenticular; Rough-ped fabric; Dry; Firm consistence; Few cutans, <10% of ped faces or walls 
	coated, faint; Field pH 6 (pH meter); Common, very fine (0-1mm) roots; Few, fine (1-2mm) roots; 
	Common, medium (2-5mm) roots; Abrupt, Irregular change to - 
	A3	0.16 - 0.28 m	Dark reddish brown (5YR3/3-Moist); Biological mixing, 2-10% , Faint; Clay loam; Moderate grade 
	of structure, 10-20 mm, Subangular blocky; 100-200 mm, Lenticular; Smooth-ped fabric; Dry; 
	Firm consistence; 0-2%, coarse gravelly, 20-60mm, subangular tabular, dispersed, Basalt, 
	coarse fragments; Few cutans, <10% of ped faces or walls coated, faint; Field pH 5.5 (pH 
	meter); Few, very fine (0-1mm) roots; Common, fine (1-2mm) roots; Common, medium (2-5mm) 
	roots; Few, coarse (>5mm) roots; Clear, Wavy change to - 
	B1	0.28 - 0.44 m	Dark reddish brown (5YR3/3-Moist); Biological mixing, 2-10% , Faint; Clay loam; Moderate grade 
	of structure, 10-20 mm, Subangular blocky; 100-200 mm, Lenticular; Smooth-ped fabric; 
	Moderately moist; Firm consistence; 0-2%, coarse gravelly, 20-60mm, subangular tabular, 
	dispersed, Basalt, coarse fragments; Few cutans, <10% of ped faces or walls coated, faint; 
	Field pH 5.5 (pH meter); Few, very fine (0-1mm) roots; Few, fine (1-2mm) roots; Few, medium (2-
	5mm) roots; Gradual, Wavy change to - 
	B21	0.44 - 1.41 m	Dark reddish brown (2.5YR3/4-Moist); Biological mixing, 2-10% , Faint; Clay loam; Strong grade 
	of structure, 10-20 mm, Polyhedral; 100-200 mm, Lenticular; Smooth-ped fabric; Moderately 
	moist; Firm consistence; 0-2%, coarse gravelly, 20-60mm, subangular tabular, dispersed, 
	Basalt, coarse fragments; Common cutans, 10-50% of ped faces or walls coated, distinct; Field
	 pH 5 (pH meter); Few, very fine (0-1mm) roots; Diffuse change to - 
	B22	1.41 - 1.96 m	Yellowish red (5YR4/6-Moist); ; Silty clay; Smooth-ped fabric; Moderately moist; 0-2%, coarse 
	gravelly, 20-60mm, subangular tabular, dispersed, Basalt, coarse fragments; Field pH 5 (pH 
	meter); Clear change to - 

	Project Name:	BAGO-MARAGLE ESM
	Project Code:	BGM_ESM	Site ID:	1020	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	B31	1.96 - 2.76 m	Strong brown (7.5YR4/6-Moist); ; Clay loam; Moderately moist; 2-10%, medium gravelly, 6-20mm,
	 subrounded, dispersed, Tuff, coarse fragments; Few (2 - 10 %), Manganiferous, Medium (2 -6 
	mm), Fragments, strong, segregations;Few (2 - 10 %), Manganiferous, Medium (2 -6 mm), 
	Concretions, strong, segregations;Field pH 4.5 (pH meter); Clear change to - 
	B32	2.76 - 2.91 m	Strong brown (7.5YR4/6-Moist); ; Clay loam; Moderately moist; 2-10%, medium gravelly, 6-20mm,
	 subangular, dispersed, Tuff, coarse fragments; Few (2 - 10 %), Manganiferous, Medium (2 -6 
	mm), Fragments, strong, segregations;Few (2 - 10 %), Manganiferous, Medium (2 -6 mm), 
	Concretions, strong, segregations;Field pH 4.5 (pH meter); 
	Morphological Notes
	B32	Dense layer could not be augered. Course fragments has phenocrysts of feldspar and 
	vesicles. RM tuffaceous or trachyte.
	Observation Notes
	PGP centre peg 2m north east of pit.
	Site Notes
	PGP4, BAGO S.F., COMPT 29

	Project Name:	BAGO-MARAGLE ESM
	Project Code:	BGM_ESM	Site ID:	1020	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0.01 - 0.09	4.92C	29.09H	10.34	2.63	0.11	0.98J	43.15E
	5.48A	0K
	0.06 - 0.16	4.91C	9.41H	3.11	2.41	0.04	1.3J	16.27E
	5.76A	0K
	0.16 - 0.28	4.79C	7.57H	2.5	2.25	0.06	1.83J	14.2E
	5.58A	0K
	0.31 - 0.39	4.56C	4.13H	1.92	1.24	0.06	1.9J	9.25E
	5.49A	0K
	0.61 - 0.81	4.13C	1.12H	1.06	0.85	0.04	5.8J	8.86E
	5.21A	0K
	1.61 - 1.81	3.94C	0.15H	0.34	0.69	0.05	8.74J	9.97E
	4.84A	0K
	2.21 - 2.51	3.84C	0.14H	1.06	0.54	0.06	23.13J	24.94E
	4.77A	0K
	2.76 - 2.91	3.76C	0.1H	0.92	0.48	0.11	35.23J	36.85E
	4.48A	0K
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0.01 - 0.09	17.57B	1849.9B	0.88A	0.61	8.16
	0.06 - 0.16	5.36B	534.3B	0.28A	0.75	19.87
	0.16 - 0.28	3.96B	412.9B	0.25A	1.08	37.34
	0.31 - 0.39	2.41B	968.1B	0.13A	1.12	14.54
	0.61 - 0.81	0.52B	687B	0.06A	1.15	32.61
	1.61 - 1.81	0.46B	720.7B	0.06A	40.94
	2.21 - 2.51	0.19B	2343.5B	0.02A	26.87
	2.76 - 2.91	0.25B	2636.7B	0.01A	21.11
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0.01 - 0.09
	0.06 - 0.16
	0.16 - 0.28
	0.31 - 0.39
	0.61 - 0.81
	1.61 - 1.81
	2.21 - 2.51
	2.76 - 2.91

	Project Name:	BAGO-MARAGLE ESM
	Project Code:	BGM_ESM	Site ID:	1020	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Analyses Completed for this profile
	13C1_AL	Citrate/dithionite-extractable iron, aluminium, Manganese and Silicon
	13C1_FE	Citrate/dithionite-extractable iron, aluminium, Manganese and Silicon
	15_NR	Sum of Ex. cations + Ex. acidity - Not recorded
	15E1_AL	Exchangeable Al - by compulsive exchange, no pretreatment for soluble salts
	15E1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) by compulsive exchange, no pretreatment for soluble 
	15E1_H	Exchangeable H - by compulsive exchange, no pretreatment for soluble salts
	15E1_K	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MG	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_NA	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	2A1	Air-dry moisture content
	4A1	pH of 1:5 soil/water suspension
	4B2	pH of 1:5 soil/0.01M calcium chloride extract - following Method 4A1
	6B2	Total organic carbon - high frequency induction furnace, volumetric
	7A2	Total nitrogen - semimicro Kjeldahl , automated colour
	9A3	Total Phosphorus (ppm) - semimicro kjeldahl, automated colour
	P10_GRAV	Gravel (%)
	P3A1	Bulk density - g/cm3