Project Name:	BAGO-MARAGLE ESM
	Project Code:	BGM_ESM	Site ID:	1022	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Site Information
	Desc. By:	P. Ryan	Locality:
	Date Desc.:	04/04/95	Elevation:	1303 metres
	Map Ref.:	Sheet No. : 8526   DGPS	Rainfall:	No Data
	Northing/Long.:	6048604 AMG zone: 55	Runoff:	Slow
	Easting/Lat.:	609183  Datum: AGD66	Drainage:	Well drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	Probable
	Geol. Ref.:	No Data	Substrate Material:	Granodiorite 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	No Data
	Morph. Type:	Upper-slope	Relief:	No Data
	Elem. Type:	Hillslope	Slope Category:	No Data
	Slope:	8 % 	Aspect:	90 degrees
	Surface Soil Condition (dry):	Firm
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Melacic Dystrophic Red Kandosol Medium Non-gravelly Clay-	Principal Profile Form:	Um6.13
	loamy Clay-loamy Very deep
	ASC Confidence:	Great Soil Group:	No suitable group
	All necessary analytical data are available.
	Site Disturbance:	No effective disturbance. Natural
	Vegetation:
	Surface Coarse Fragments:	2-10%, coarse gravelly, 20-60mm, subrounded platy, Granodiorite
	Profile Morphology
	O1	0 - 0.02 m	Organic Layer; ; 
	A1	0.02 - 0.13 m	Dark reddish brown (5YR2.5/2-Moist); ; Clay loam; Strong grade of structure, 2-5 mm, Polyhedral;
	 100-200 mm, Prismatic; Rough-ped fabric; Dry; Firm consistence; Field pH 6 (pH meter); Many, 
	very fine (0-1mm) roots; Common, fine (1-2mm) roots; Abrupt, Wavy change to - 
	A3	0.13 - 0.23 m	Dark reddish brown (5YR3/2-Moist); Biological mixing, 2-10% , Distinct; Clay loam; Strong grade
	 of structure, 5-10 mm, Polyhedral; 100-200 mm, Lenticular; Rough-ped fabric; Dry; Firm 
	consistence; Field pH 6 (pH meter); Common, very fine (0-1mm) roots; Few, fine (1-2mm) roots; 
	Clear, Irregular change to - 
	B21	0.23 - 0.37 m	Dark reddish brown (5YR3/4-Moist); Biological mixing, 2-10% , Distinct; Clay loam; Moderate 
	grade of structure, 5-10 mm, Subangular blocky; 50-100 mm, Columnar; Rough-ped fabric; Dry; 
	Firm consistence; Few cutans, <10% of ped faces or walls coated, faint; Field pH 5.5 (pH 
	meter); Few, very fine (0-1mm) roots; Gradual, Smooth change to - 
	B22	0.37 - 0.74 m	Yellowish red (5YR4/6-Moist); Biological mixing, 0-2% , Distinct; Clay loam; Weak grade of 
	structure, 5-10 mm, Subangular blocky; Smooth-ped fabric; Moderately moist; Weak 
	consistence; 2-10%, coarse gravelly, 20-60mm, subrounded tabular, dispersed, Granodiorite, 
	coarse fragments; Few cutans, <10% of ped faces or walls coated, faint; Field pH 5 (pH meter); 
	Few, very fine (0-1mm) roots; Few, fine (1-2mm) roots; Few, medium (2-5mm) roots; Few, coarse 
	(>5mm) roots; Diffuse, Smooth change to - 
	B23	0.74 - 1.02 m	Yellowish red (5YR4/6-Moist); ; Clay loam; Massive grade of structure; Earthy fabric; Moderately 
	moist; Weak consistence; 20-50%, stony, 200-600mm, subrounded, dispersed, Granodiorite, 
	coarse fragments; Field pH 5 (pH meter); Few, very fine (0-1mm) roots; Gradual change to - 
	C	1.02 - 1.77 m	Brown (10YR5/3-Moist); ; Clayey sand; Sandy (grains prominent) fabric; Moderately moist; Field 
	pH 6 (pH meter); 
	Morphological Notes
	B23	Large tors distributed through this horizon.
	Observation Notes
	PGP 12, centre post 4 m north of pit.
	Site Notes

	Project Name:	BAGO-MARAGLE ESM
	Project Code:	BGM_ESM	Site ID:	1022	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)

	Project Name:	BAGO-MARAGLE ESM
	Project Code:	BGM_ESM	Site ID:	1022	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0.02 - 0.1	4.73C	11.15H	2.64	1.11	0.04	1.65J	16.59E
	5.49A	0K
	0.02 - 0.15
	0.14 - 0.23	4.36C	2.94H	1.31	0.78	0.02	2.57J	7.62E
	5.37A	0K
	0.25 - 0.45
	0.32 - 0.4	3.98C	0.51H	0.47	0.56	0.01	4.86J	6.41E
	4.96A	0K
	0.47 - 0.67	3.93C	0.28H	0.52	0.49	0.01	4.33J	5.63E
	4.99A	0K
	0.5 - 0.7
	0.77 - 0.97	4.12C	0.6H	0.79	0.47	0.02	2.33J	4.21E
	5.11A	0K
	1.22 - 1.52	4.74C	0.14H	0.15	0.31	0.02	0.17J	0.8E
	5.3A	0K
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0.02 - 0.1	6.4B	836.1B	0.3A	1.00	10.36
	0.02 - 0.15	1.05
	1.09
	0.91
	0.14 - 0.23	2.29B	691.4B	0.14A	1.23	8.07
	0.25 - 0.45	1.15
	1.14
	0.32 - 0.4	1.12B	493.4B	0.08A	1.21	4.64
	0.47 - 0.67	0.56B	376.7B	0.04A	1.41	1.71
	0.5 - 0.7	1.26
	1.22
	1.18
	0.77 - 0.97	0.16B	341.2B	0.02A	1.58	5.26
	1.22 - 1.52	0.15B	693.7B	0.01A	22.87
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0.02 - 0.1
	0.02 - 0.15	0.47E	0.42E	0.28E	0.24F	0.2F	1994D	81B
	0.46E	0.43E	0.28E	0.23F	0.18F	471D	98B
	0.44E	0.39E	0.24E	0.21F	0.18F	4792D	220B
	0.14 - 0.23
	0.25 - 0.45	0.42E	0.38E	0.27E	0.2F	0.17F	651D	56B
	0.41E	0.38E	0.27E	0.21F	0.18F	560D	95B
	0.32 - 0.4
	0.47 - 0.67
	0.5 - 0.7	0.42E	0.39E	0.27E	0.2F	0.17F	367D	63B
	0.42E	0.38E	0.25E	0.19F	0.16F	144D	35B
	0.4E	0.25E	0.26E	0.19F	0.16F	792D	74B
	0.77 - 0.97

	Project Name:	BAGO-MARAGLE ESM
	Project Code:	BGM_ESM	Site ID:	1022	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	1.22 - 1.52

	Project Name:	BAGO-MARAGLE ESM
	Project Code:	BGM_ESM	Site ID:	1022	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Analyses Completed for this profile
	15_NR	Sum of Ex. cations + Ex. acidity - Not recorded
	15E1_AL	Exchangeable Al - by compulsive exchange, no pretreatment for soluble salts
	15E1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) by compulsive exchange, no pretreatment for soluble 
	15E1_H	Exchangeable H - by compulsive exchange, no pretreatment for soluble salts
	15E1_K	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MG	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_NA	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	2A1	Air-dry moisture content
	4A1	pH of 1:5 soil/water suspension
	4B2	pH of 1:5 soil/0.01M calcium chloride extract - following Method 4A1
	6B2	Total organic carbon - high frequency induction furnace, volumetric
	7A2	Total nitrogen - semimicro Kjeldahl , automated colour
	9A3	Total Phosphorus (ppm) - semimicro kjeldahl, automated colour
	P10_GRAV	Gravel (%)
	P3A1	Bulk density - g/cm3
	P3B2VL_1	1 BAR Moisture m3/m3 - Volumetric using disturbed sample on pressure plate
	P3B2VL_15	15 BAR Moisture m3/m3 - Volumetric using disturbed sample on pressure plate
	P3B2VL_5	5 BAR Moisture m3/m3 - Volumetric using disturbed sample on pressure plate
	P3B3VLb001	0.01 BAR Moisture m3/m3 - Volumetric using undisturbed 73mm diameter and 75mm height core on 
	suction plate taken from center of large core (CSIRO Div of Soil, DR 125, McKenzie and Jacquier, 
	1996)
	P3B3VLb005	0.05 BAR Moisture m3/m3 - Volumetric using undisturbed 73mm diameter and 75mm height core on 
	suction plate taken from center of large core (CSIRO Div of Soil, DR 125, McKenzie and Jacquier, 
	1996)
	P3B3VLb01	0.1 BAR Moisture m3/m3 - Volumetric using undisturbed 73mm diameter and 75mm height core on 
	suction plate taken from center of large core (CSIRO Div of Soil, DR 125, McKenzie and Jacquier, 
	1996)
	P3B3VLb06	0.66 BAR Moisture m3/m3 - Volumetric using undisturbed 73mm diameter and 75mm height core on 
	suction plate taken from center of large core (CSIRO Div of Soil, DR 125, McKenzie and Jacquier, 
	1996)
	P4_100DMcK	Unsaturated Hydraulic Conductivity - 100mm potential - Using disk permeameter with method CSIRO 
	Div of Soil, DR 125, McKenzie and Jacquier, 1996
	P4_10DMcK	Unsaturated Hydraulic Conductivity - 10mm potential - Using disk permeameter with method CSIRO 
	Div of Soil, DR 125, McKenzie and Jacquier, 1996
	P4_50DMcK	Unsaturated Hydraulic Conductivity - 50mm potential - Using disk permeameter with method CSIRO 
	Div of Soil, DR 125, McKenzie and Jacquier, 1996
	P4_sat_McK	Saturated Hydraulic Conductivity (CSIRO Div of Soil, DR 125, McKenzie and Jacquier, 1996)