Project Name:	BAGO-MARAGLE FOREST SOIL SURVEY         
	Project Code:	BGM_FSS	Site ID:	0010	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Site Information
	Desc. By:	N.J. McKenzie	Locality:
	Date Desc.:	19/12/95	Elevation:	1070 metres
	Map Ref.:	Sheet No. : 8526   DGPS	Rainfall:	No Data
	Northing/Long.:	6031874 AMG zone: 55	Runoff:	No Data
	Easting/Lat.:	619919  Datum: AGD66	Drainage:	Well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	Probable
	Geol. Ref.:	Os	Substrate Material:	Sandstone 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	No Data
	Morph. Type:	Mid-slope	Relief:	No Data
	Elem. Type:	Hillslope	Slope Category:	No Data
	Slope:	23 % 	Aspect:	45 degrees
	Surface Soil Condition (dry):	Firm
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Acidic Magnesic Red Kandosol Medium Slightly gravelly 	Principal Profile Form:	N/A
	Loamy Clay-loamy Very deep
	ASC Confidence:	Great Soil Group:	N/A
	All necessary analytical data are available.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:
	Surface Coarse Fragments:
	Profile Morphology
	A11	0 - 0.12 m	Dark reddish brown (5YR3/2-Moist); ; Loam; Moderate grade of structure, 10-20 mm, Polyhedral; 
	Rough-ped fabric; Moderately moist; Weak consistence; 2-10%, medium gravelly, 6-20mm, 
	angular tabular, Sandstone, coarse fragments; Common cutans, 10-50% of ped faces or walls 
	coated, faint; Field pH 6 (Raupach); Many, very fine (0-1mm) roots; Common, fine (1-2mm) roots; 
	Few, medium (2-5mm) roots; Clear, Smooth change to - 
	AB	0.12 - 0.32 m	Reddish brown (5YR4/4-Moist); Biological mixing, 5YR42, 20-50% , Distinct; Clay loam; 
	Moderate grade of structure, 10-20 mm, Polyhedral; Rough-ped fabric; Moist; Weak consistence;
	 10-20%, medium gravelly, 6-20mm, angular tabular, Sandstone, coarse fragments; Common 
	cutans, 10-50% of ped faces or walls coated, faint; Field pH 6 (Raupach); Common, very fine (0-
	1mm) roots; Few, fine (1-2mm) roots; Few, medium (2-5mm) roots; Few, coarse (>5mm) roots; 
	Clear, Smooth change to - 
	B21	0.32 - 0.63 m	Red (2.5YR4/6-Moist); Biological mixing, 5YR43, 10-20% , Distinct; Clay loam; Massive grade of
	 structure; Earthy fabric; Moist; Weak consistence; 10-20%, medium gravelly, 6-20mm, angular 
	tabular, Sandstone, coarse fragments; Common cutans, 10-50% of ped faces or walls coated, 
	faint; Field pH 5.5 (Raupach); Common, very fine (0-1mm) roots; Few, fine (1-2mm) roots; Few, 
	medium (2-5mm) roots; Few, coarse (>5mm) roots; Diffuse, Smooth change to - 
	B22	0.63 - 1.2 m	Red (2.5YR5/6-Moist); Biological mixing, 2.5YR56, 2-10% , Distinct; Clay loam; Massive grade 
	of structure; Earthy fabric; Moderately moist; Weak consistence; 10-20%, medium gravelly, 6-
	20mm, angular tabular, Sandstone, coarse fragments; Common cutans, 10-50% of ped faces or
	 walls coated, faint; Field pH 5.5 (Raupach); Few, very fine (0-1mm) roots; Few, fine (1-2mm) 
	roots; Clear, Smooth change to - 
	C1	1.2 - 1.4 m	Brownish yellow (10YR6/8-Moist); Substrate influence, 2.5YR46, 10-20% , Distinct; Medium 
	sandy clay loam; Earthy fabric; Moderately moist; Few cutans, <10% of ped faces or walls 
	coated, faint; Field pH 5.5 (Raupach); Clear, Smooth change to - 
	C2	1.4 - 1.85 m	Red (2.5YR4/6-Moist); ; Medium sandy clay loam; Earthy fabric; Moderately moist; Few cutans, 
	<10% of ped faces or walls coated, faint; Field pH 5.5 (Raupach); Clear, Smooth change to - 
	Morphological Notes
	AB	B horizon redness not as pronounced as  other Ordovician sites.                                       

	Project Name:	BAGO-MARAGLE FOREST SOIL SURVEY         
	Project Code:	BGM_FSS	Site ID:	0010	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	B21	Same as layer 2.                                                                                                                   
	                                                                     
	Observation Notes
	Site Notes
	COMP 15H, 2811-1,BRG 13, 368M FR 3044 

	Project Name:	BAGO-MARAGLE FOREST SOIL SURVEY         
	Project Code:	BGM_FSS	Site ID:	0010	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.12	4.26C	4.78H	0.81	0.56	0.04	2.86J	9.05E
	0K
	0.12 - 0.32	4.31C	0.34H	0.24	0.38	0.02	1.37J	2.35E
	0K
	0.32 - 0.63	4.4C	0.14H	0.23	0.32	0.01	0.66J	1.37E
	0K
	0.63 - 1.2	4.17C	0H	0.13	0.21	0.04	1J	1.38E
	0K
	1.2 - 1.4	4.15C	0H	0.06	0.17	0.01	0.65J	0.88E
	0K
	1.4 - 1.85	4.12C	0H	0.05	0.13	0	0.83J	1.01E
	0K
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.12	5.91B	351.6B	0.25A	1.07	49.29
	0.12 - 0.32	1.5B	467.1B	0.08A	1.34	29.62
	0.32 - 0.63	0.76B	360.4B	0.03A	1.27	33.11
	0.63 - 1.2	0.3B	404.8B	0.02A	1.53	36.01
	1.2 - 1.4	0.12B	201.5B	0.01A	16.31
	1.4 - 1.85	0.07B	264.9B	0.01A	29.8
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.12
	0.12 - 0.32
	0.32 - 0.63
	0.63 - 1.2
	1.2 - 1.4
	1.4 - 1.85

	Project Name:	BAGO-MARAGLE FOREST SOIL SURVEY         
	Project Code:	BGM_FSS	Site ID:	0010	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Analyses Completed for this profile
	15_NR	Sum of Ex. cations + Ex. acidity - Not recorded
	15E1_AL	Exchangeable Al - by compulsive exchange, no pretreatment for soluble salts
	15E1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) by compulsive exchange, no pretreatment for soluble 
	15E1_H	Exchangeable H - by compulsive exchange, no pretreatment for soluble salts
	15E1_K	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MG	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_NA	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	2A1	Air-dry moisture content
	4B2	pH of 1:5 soil/0.01M calcium chloride extract - following Method 4A1
	6B2	Total organic carbon - high frequency induction furnace, volumetric
	7A2	Total nitrogen - semimicro Kjeldahl , automated colour
	9A3	Total Phosphorus (ppm) - semimicro kjeldahl, automated colour
	P10_GRAV	Gravel (%)
	P3A1	Bulk density - g/cm3