Project Name:	BAGO-MARAGLE FOREST SOIL SURVEY         
	Project Code:	BGM_FSS	Site ID:	0030	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Site Information
	Desc. By:	N.J. McKenzie	Locality:
	Date Desc.:	16/02/96	Elevation:	1044 metres
	Map Ref.:	Sheet No. : 8526   DGPS	Rainfall:	No Data
	Northing/Long.:	6027594 AMG zone: 55	Runoff:	No Data
	Easting/Lat.:	614208  Datum: AGD66	Drainage:	Poorly drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	SGG	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	No Data
	Morph. Type:	Open depression (vale)	Relief:	No Data
	Elem. Type:	Drainage depression	Slope Category:	No Data
	Slope:	8 % 	Aspect:	0 degrees
	Surface Soil Condition (dry):	Soft
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Acidic Kandosolic Redoxic Hydrosol Medium Non-gravelly 	Principal Profile Form:	Um5.52
	Clay-loamy Clay-loamy Very deep
	ASC Confidence:	Great Soil Group:	N/A
	All necessary analytical data are available.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:
	Surface Coarse Fragments:
	Profile Morphology
	A1	0 - 0.18 m	Very dark grey (10YR3/1-Moist); ; Medium sandy clay loam (Sapric); Rough-ped fabric; Wet; 
	Weak consistence; Field pH 5 (Raupach); Many, very fine (0-1mm) roots; Common, fine (1-2mm) 
	roots; Few, medium (2-5mm) roots; Clear, Smooth change to - 
	B21	0.18 - 0.48 m	Grey (10YR5/1-Moist); Substrate influence, 10YR54, 2-10% , Distinct; Substrate influence, 
	7.5YR46, 0-2% , Distinct; Clay loam, sandy; Massive grade of structure; Sandy (grains 
	prominent) fabric; Wet; Weak consistence; Few cutans, <10% of ped faces or walls coated, 
	faint; Field pH 4.5 (Raupach); Many, very fine (0-1mm) roots; Few, fine (1-2mm) roots; Diffuse, 
	Smooth change to - 
	B22	0.48 - 0.8 m	Grey (10YR5/1-Moist); Substrate influence, 10YR54, 0-2% , Distinct; Clay loam, sandy; Massive 
	grade of structure; Sandy (grains prominent) fabric; Wet; Weak consistence; Few cutans, <10% 
	of ped faces or walls coated, faint; Field pH 5.5 (Raupach); Common, very fine (0-1mm) roots; 
	Few, fine (1-2mm) roots; Diffuse, Smooth change to - 
	B23	0.8 - 1.4 m	Grey (10YR6/1-Moist); Substrate influence, 10YR72, 20-50% , Faint; Substrate influence, 
	7.5YR68, 10-20% , Prominent; Clay loam, coarse sandy; Massive grade of structure; Sandy 
	(grains prominent) fabric; Wet; Weak consistence; Few cutans, <10% of ped faces or walls 
	coated, faint; Field pH 5.5 (Raupach); Few, very fine (0-1mm) roots; Few, fine (1-2mm) roots; 
	Abrupt, Smooth change to - 
	2A	1.4 - 1.5 m	Grey (10YR5/1-Moist); Substrate influence, 10YR63, 20-50% , Faint; Substrate influence, 
	7.5YR68, 10-20% , Prominent; Medium sandy clay loam; Massive grade of structure; Sandy 
	(grains prominent) fabric; Wet; Very weak consistence; 20-50%, fine gravelly, 2-6mm, angular, 
	dispersed, Quartz, coarse fragments; Field pH 5.5 (Raupach); Few, very fine (0-1mm) roots; Few,
	 fine (1-2mm) roots; Clear, Smooth change to - 
	2B	1.5 - 1.7 m	Grey (10YR6/1-Moist); ; Medium clay; Rough-ped fabric; Wet; Weak consistence; Few cutans, 
	<10% of ped faces or walls coated, faint; Field pH 5.5 (Raupach); 
	Morphological Notes
	A1	Very organic, saturated with gentle overland flow.
	B21	Gleyed, gritty adamellite, colluvial origin.
	B22	Same as layer 2.                                                                                                                   

	Project Name:	BAGO-MARAGLE FOREST SOIL SURVEY         
	Project Code:	BGM_FSS	Site ID:	0030	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	B23	Medium clay prisms, with gritty clay loam material in between clay having  more mottles. 
	Is this hexagonal pattern periglacial? Coarse material has        colluvial origin, med. clay
	 alluvial.
	2A	Medium clay base connected to medium clay in layer 4.
	2B	Layer continues - equipment refusal. Very coarse sandy layer - may be very thin but very 
	difficult due to slurry in the auger hole.
	Observation Notes
	Edge of swamp with overland and throughflow in upper part of the profile
	Site Notes
	COMP38H,76921-1,BRG199,325M FR 76618-1

	Project Name:	BAGO-MARAGLE FOREST SOIL SURVEY         
	Project Code:	BGM_FSS	Site ID:	0030	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.18	3.98C	1.43H	1.55	0.41	0.1	1.84J	5.35E
	0.02K
	0.18 - 0.48	3.79C	0.13H	0.37	0.26	0.05	1.32J	2.13E
	0K
	0.48 - 0.8	3.75C	0.11H	0.26	0.24	0	1.38J	1.99E
	0K
	0.8 - 1.4	3.88C	0.13H	0.32	0.21	0.02	1.45J	2.13E
	0K
	1.4 - 1.5	3.82C	0.69H	0.91	0.46	0.06	2.62J	4.73E
	0K
	1.5 - 1.7	4C	1.35H	1.25	0.53	0.09	1.27J	4.5E
	0K
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.18	3.32B	194.1B	0.15A	23.18
	0.18 - 0.48	0.8B	69.9B	0.04A	0.92	23.48
	0.48 - 0.8	0.54B	75.5B	0.03A	1.50	19.35
	0.8 - 1.4	0.41B	39.2B	0.02A	1.50	23.37
	1.4 - 1.5	0.48B	75.3B	0.02A	31.34
	1.5 - 1.7	0.24B	49.3B	0.01A	30.12
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.18
	0.18 - 0.48
	0.48 - 0.8
	0.8 - 1.4
	1.4 - 1.5
	1.5 - 1.7

	Project Name:	BAGO-MARAGLE FOREST SOIL SURVEY         
	Project Code:	BGM_FSS	Site ID:	0030	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Analyses Completed for this profile
	15_NR	Sum of Ex. cations + Ex. acidity - Not recorded
	15E1_AL	Exchangeable Al - by compulsive exchange, no pretreatment for soluble salts
	15E1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) by compulsive exchange, no pretreatment for soluble 
	15E1_H	Exchangeable H - by compulsive exchange, no pretreatment for soluble salts
	15E1_K	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MG	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_NA	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	2A1	Air-dry moisture content
	4B2	pH of 1:5 soil/0.01M calcium chloride extract - following Method 4A1
	6B2	Total organic carbon - high frequency induction furnace, volumetric
	7A2	Total nitrogen - semimicro Kjeldahl , automated colour
	9A3	Total Phosphorus (ppm) - semimicro kjeldahl, automated colour
	P10_GRAV	Gravel (%)
	P3A1	Bulk density - g/cm3