Project Name:	BAGO-MARAGLE FOREST SOIL SURVEY         
	Project Code:	BGM_FSS	Site ID:	0032	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Site Information
	Desc. By:	P. Ryan	Locality:
	Date Desc.:	20/12/95	Elevation:	1051 metres
	Map Ref.:	Sheet No. : 8526   DGPS	Rainfall:	No Data
	Northing/Long.:	6027537 AMG zone: 55	Runoff:	No Data
	Easting/Lat.:	619389  Datum: AGD66	Drainage:	Well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	Probable
	Geol. Ref.:	Dga	Substrate Material:	Granodiorite 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	No Data
	Morph. Type:	Mid-slope	Relief:	No Data
	Elem. Type:	No Data	Slope Category:	No Data
	Slope:	18 % 	Aspect:	315 degrees
	Surface Soil Condition (dry):	Firm
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Acidic Magnesic Red Kandosol Thin Gravelly Loamy Clay-	Principal Profile Form:	Gn2.11
	loamy Very deep
	ASC Confidence:	Great Soil Group:	Red earth
	All necessary analytical data are available.
	Site Disturbance:	No effective disturbance. Natural
	Vegetation:
	Surface Coarse Fragments:	2-10%, , , 
	Profile Morphology
	O1	0 - 0.02 m	Organic Layer; ; 
	A11	0.02 - 0.08 m	Dark reddish brown (5YR3/3-Moist); Mechanical, 2.5YR48, 20-50% , Prominent; Loam; Massive 
	grade of structure; Earthy fabric; Moist; Weak consistence; 10-20%, fine gravelly, 2-6mm, 
	subangular, coarse fragments; Field pH 6 (Raupach); Many, very fine (0-1mm) roots; Common, 
	fine (1-2mm) roots; Few, medium (2-5mm) roots; Broken change to - 
	A12	0.08 - 0.18 m	Dark reddish brown (5YR3/2-Moist); Biological mixing, 5YR33, 10-20% , Faint; Loam; Moderate 
	grade of structure, 2-5 mm, Polyhedral; 10-20 mm, Subangular blocky; Rough-ped fabric; Moist; 
	Weak consistence; 2-10%, fine gravelly, 2-6mm, subangular, Coal, coarse fragments; Field pH 
	5.5 (Raupach); Many, very fine (0-1mm) roots; Few, fine (1-2mm) roots; Few, medium (2-5mm) 
	roots; Clear, Wavy change to - 
	B21	0.18 - 0.52 m	Dark reddish brown (2.5YR3/4-Moist); Biological mixing, 2.5YR33, 2-10% , Faint; Clay loam; 
	Weak grade of structure, 2-5 mm, Polyhedral; Rough-ped fabric; Moist; Weak consistence; Field
	 pH 4.5 (Raupach); Common, very fine (0-1mm) roots; Few, fine (1-2mm) roots; Common, 
	medium (2-5mm) roots; Common, coarse (>5mm) roots; Smooth change to - 
	B22	0.52 - 1.02 m	Dark reddish brown (2.5YR3/4-Moist); ; Clay loam; Massive grade of structure; Earthy fabric; 
	Moist; Weak consistence; Field pH 4.5 (Raupach); Few, very fine (0-1mm) roots; Few, fine (1-
	2mm) roots; Few, medium (2-5mm) roots; Few, coarse (>5mm) roots; 
	B22	1.02 - 1.47 m	Red (2.5YR4/6-Moist); ; Clay loam; Earthy fabric; Moist; Weak consistence; Field pH 4.5 
	(Raupach); Diffuse change to - 
	B3	1.47 - 2.02 m	Dark reddish brown (2.5YR3/4-Moist); ; Earthy fabric; Moist; Weak consistence; 10-20%, coarse 
	gravelly, 20-60mm, Granodiorite, coarse fragments; Field pH 4.5 (Raupach); 
	Morphological Notes
	A11	A mixture of surface and weathered      gravel. Possibly infilling a hollow or  mixed into A
	 horizon. Layer is not      continuous.                                                                     
	A12	Layer may be partially buried.                                                                                               
	                                                                           
	B3	Small amounts of weathered parent material above substrate.
	Observation Notes

	Project Name:	BAGO-MARAGLE FOREST SOIL SURVEY         
	Project Code:	BGM_FSS	Site ID:	0032	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Site Notes
	COMP 20H,3496-1,255DEG,375M FROM RD   

	Project Name:	BAGO-MARAGLE FOREST SOIL SURVEY         
	Project Code:	BGM_FSS	Site ID:	0032	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.02
	0.02 - 0.08	4.66C	1.67H	1.05	1.45	0.05	1.3J	5.52E
	0K
	0.08 - 0.18	4.3C	0.09H	0.52	1.05	0.08	2.49J	4.22E
	0K
	0.18 - 0.52	3.95C	0H	0.63	0.54	0.08	4.13J	5.37E
	0K
	0.52 - 1.02	3.96C	0H	0.6	0.75	0.07	3.89J	5.31E
	0K
	1.02 - 1.47	3.96C	0H	0.54	0.83	0.09	4.74J	6.2E
	0K
	1.47 - 2.02	3.95C	0H	0.33	0.95	0.13	5.02J	6.44E
	0K
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.02
	0.02 - 0.08	3.55B	252.7B	0.14A	18.5
	0.08 - 0.18	1.93B	178.1B	0.08A	21.2
	0.18 - 0.52	0.77B	116.2B	0.04A	15.33
	0.52 - 1.02	0.28B	106.9B	0.02A	19.54
	1.02 - 1.47	0.24B	131B	0.02A	29.52
	1.47 - 2.02	0.23B	131.6B	0.02A	4.03
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.02
	0.02 - 0.08
	0.08 - 0.18
	0.18 - 0.52
	0.52 - 1.02
	1.02 - 1.47
	1.47 - 2.02

	Project Name:	BAGO-MARAGLE FOREST SOIL SURVEY         
	Project Code:	BGM_FSS	Site ID:	0032	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Analyses Completed for this profile
	15_NR	Sum of Ex. cations + Ex. acidity - Not recorded
	15E1_AL	Exchangeable Al - by compulsive exchange, no pretreatment for soluble salts
	15E1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) by compulsive exchange, no pretreatment for soluble 
	15E1_H	Exchangeable H - by compulsive exchange, no pretreatment for soluble salts
	15E1_K	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MG	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_NA	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	2A1	Air-dry moisture content
	4B2	pH of 1:5 soil/0.01M calcium chloride extract - following Method 4A1
	6B2	Total organic carbon - high frequency induction furnace, volumetric
	7A2	Total nitrogen - semimicro Kjeldahl , automated colour
	9A3	Total Phosphorus (ppm) - semimicro kjeldahl, automated colour
	P10_GRAV	Gravel (%)