Project Name:	BAGO-MARAGLE FOREST SOIL SURVEY         
	Project Code:	BGM_FSS	Site ID:	0041	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Site Information
	Desc. By:	N.J. McKenzie	Locality:
	Date Desc.:	11/12/95	Elevation:	1064 metres
	Map Ref.:	Sheet No. : 8526   DGPS	Rainfall:	No Data
	Northing/Long.:	6036584 AMG zone: 55	Runoff:	No Data
	Easting/Lat.:	619810  Datum: AGD66	Drainage:	Rapidly drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	Probable
	Geol. Ref.:	Sgg	Substrate Material:	Granodiorite 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	No Data
	Morph. Type:	Upper-slope	Relief:	No Data
	Elem. Type:	Hillslope	Slope Category:	No Data
	Slope:	23 % 	Aspect:	45 degrees
	Surface Soil Condition (dry):	Firm
	Erosion:	Stable, Minor (sheet) 
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Acidic Magnesic Red Kandosol Medium Slightly gravelly 	Principal Profile Form:	Um6.
	Clay-loamy Clay-loamy Very deep
	ASC Confidence:	Great Soil Group:	N/A
	All necessary analytical data are available.
	Site Disturbance:	No effective disturbance. Natural
	Vegetation:
	Surface Coarse Fragments:
	Profile Morphology
	A11	0 - 0.06 m	Reddish brown (5YR4/3-Moist); Biological mixing, 5YR32, 20-50% , Distinct; Clay loam; 
	Moderate grade of structure, 5-10 mm, Granular; Rough-ped fabric; Moderately moist; Weak 
	consistence; 2-10%, fine gravelly, 2-6mm, angular, dispersed, Quartz, coarse fragments; Few 
	cutans, <10% of ped faces or walls coated, faint; Field pH 5.5 (Raupach); Many, very fine (0-
	1mm) roots; Abrupt, Smooth change to - 
	A12	0.06 - 0.18 m	Dark reddish brown (5YR3/3-Moist); Biological mixing, 5YR44, 20-50% , Faint; Clay loam; 
	Moderate grade of structure, 5-10 mm, Polyhedral; Rough-ped fabric; Moist; Weak consistence; 
	2-10%, fine gravelly, 2-6mm, angular, dispersed, Quartz, coarse fragments; Few cutans, <10% of
	 ped faces or walls coated, faint; Field pH 5.5 (Raupach); Common, very fine (0-1mm) roots; 
	Clear, Smooth change to - 
	B1	0.18 - 0.4 m	Red (2.5YR4/6-Moist); Biological mixing, 5YR42, 10-20% , Distinct; Clay loam; Weak grade of 
	structure, 10-20 mm, Polyhedral; Earthy fabric; Moist; Weak consistence; 2-10%, fine gravelly, 2-
	6mm, angular, dispersed, Quartz, coarse fragments; Few cutans, <10% of ped faces or walls 
	coated, faint; Field pH 5.5 (Raupach); Common, very fine (0-1mm) roots; Diffuse, Smooth 
	change to - 
	B21	0.4 - 0.7 m	Red (2.5YR4/6-Moist); Biological mixing, 5YR42, 2-10% , Distinct; Clay loam; Weak grade of 
	structure, 20-50 mm, Polyhedral; 5-10 mm, Polyhedral; Earthy fabric; Moist; Weak consistence; 
	2-10%, fine gravelly, 2-6mm, angular, dispersed, Quartz, coarse fragments; Few cutans, <10% of
	 ped faces or walls coated, faint; Field pH 5 (Raupach); Common, very fine (0-1mm) roots; 
	Diffuse, Smooth change to - 
	B22	0.7 - 0.9 m	Red (2.5YR4/6-Moist); Mottles, 7.5YR66, 2-10% , Faint; Clay loam; Massive grade of structure; 
	Earthy fabric; Moist; Weak consistence; 2-10%, fine gravelly, 2-6mm, angular, dispersed, Quartz,
	 coarse fragments; Few cutans, <10% of ped faces or walls coated, faint; Field pH 5 (Raupach);
	 Few, very fine (0-1mm) roots; Gradual, Smooth change to - 
	C11	0.9 - 1.5 m	Yellowish brown (10YR5/4-Moist); Substrate influence, 10YR74, 20-50% , Distinct; Substrate 
	influence, 7.5YR66, 10-20% , Distinct; Sandy loam; Massive grade of structure; Earthy fabric; 
	Moderately moist; Very weak consistence; 10-20%, fine gravelly, 2-6mm, angular, dispersed, 
	Quartz, coarse fragments; Field pH 5.5 (Raupach); Diffuse, Smooth change to - 

	Project Name:	BAGO-MARAGLE FOREST SOIL SURVEY         
	Project Code:	BGM_FSS	Site ID:	0041	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	C12	1.5 - 1.95 m	Yellowish brown (10YR5/4-Moist); Substrate influence, 10YR74, 20-50% , Distinct; Substrate 
	influence, 10YR82, 2-10% , Distinct; Medium sandy clay loam; Massive grade of structure; 
	Moderately moist; Very weak consistence; 10-20%, medium gravelly, 6-20mm, angular, 
	dispersed, Quartz, coarse fragments; Field pH 5.5 (Raupach); Diffuse, Smooth change to - 
	C13	1.95 - 2.45 m	Yellowish brown (10YR5/4-Moist); Substrate influence, 10YR74, 20-50% , Distinct; Substrate 
	influence, 10YR82, 2-10% , Distinct; Medium sandy clay loam; Massive grade of structure; 
	Moderately moist; Very weak consistence; 10-20%, medium gravelly, 6-20mm, angular, 
	dispersed, Quartz, coarse fragments; Field pH 5.5 (Raupach); Gradual, Smooth change to - 
	C2	2.45 - 3 m	Brown (7.5YR5/4-Moist); Substrate influence, 10YR54, 20-50% , Distinct; Loam; Massive grade 
	of structure; Moderately moist; Very weak consistence; 10-20%, medium gravelly, 6-20mm, 
	angular, dispersed, Quartz, coarse fragments; Field pH 5.5 (Raupach); 
	Morphological Notes
	A11	Peds are largely cast no O horizon dev.                                                                               
	                                                                                  
	C2	Increasing reduces at base coarse sand  drops off/clay increases.                                   
	                                                                                                    
	Observation Notes
	Site Notes
	COMP 10H,62264-1,B 156D 1M FR RD/CK   

	Project Name:	BAGO-MARAGLE FOREST SOIL SURVEY         
	Project Code:	BGM_FSS	Site ID:	0041	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.06	4.14C	1.35H	0.63	0.5	0.02	2.41J	4.92E
	0K
	0.06 - 0.18	4.17C	0.25H	0.37	0.66	0	2.78J	4.07E
	0K
	0.18 - 0.4	4.1C	0H	0.34	0.64	0	2.25J	3.23E
	0K
	0.4 - 0.7	4.09C	0H	0.6	0.67	0.01	1.9J	3.18E
	0K
	0.7 - 0.9	4.07C	0H	0.59	0.6	0	2.05J	3.23E
	0K
	0.9 - 1.5	4.28C	0H	0.25	0.47	0	0.53J	1.25E
	0K
	1.5 - 1.95	4.25C	0H	0.26	0.44	0	0.63J	1.33E
	0K
	1.95 - 2.45	4.24C	0H	0.26	0.4	0	0.75J	1.42E
	0K
	2.45 - 3	4.2C	0H	0.29	0.35	0	1J	1.64E
	0K
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.06	5.04B	198.7B	0.18A	35.43
	0.06 - 0.18	2.42B	153.9B	0.1A	1.23	37.11
	0.18 - 0.4	0.96B	56.4B	0.05A	1.29	24.3
	0.4 - 0.7	0.42B	32.7B	0.02A	1.29	39.06
	0.7 - 0.9	0.2B	20.6B	0.01A	1.33	35.3
	0.9 - 1.5	0.06B	161.9B	0A	20.4
	1.5 - 1.95	0.04B	130.3B	0A	17.5
	1.95 - 2.45	0.03B	154B	0A	12.89
	2.45 - 3	0.04B	234.1B	0A	6.81
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.06
	0.06 - 0.18
	0.18 - 0.4
	0.4 - 0.7
	0.7 - 0.9
	0.9 - 1.5
	1.5 - 1.95
	1.95 - 2.45
	2.45 - 3

	Project Name:	BAGO-MARAGLE FOREST SOIL SURVEY         
	Project Code:	BGM_FSS	Site ID:	0041	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Analyses Completed for this profile
	15_NR	Sum of Ex. cations + Ex. acidity - Not recorded
	15E1_AL	Exchangeable Al - by compulsive exchange, no pretreatment for soluble salts
	15E1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) by compulsive exchange, no pretreatment for soluble 
	15E1_H	Exchangeable H - by compulsive exchange, no pretreatment for soluble salts
	15E1_K	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MG	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_NA	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	2A1	Air-dry moisture content
	4B2	pH of 1:5 soil/0.01M calcium chloride extract - following Method 4A1
	6B2	Total organic carbon - high frequency induction furnace, volumetric
	7A2	Total nitrogen - semimicro Kjeldahl , automated colour
	9A3	Total Phosphorus (ppm) - semimicro kjeldahl, automated colour
	P10_GRAV	Gravel (%)
	P3A1	Bulk density - g/cm3