Project Name:	BAGO-MARAGLE FOREST SOIL SURVEY         
	Project Code:	BGM_FSS	Site ID:	0044	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Site Information
	Desc. By:	P. Ryan	Locality:
	Date Desc.:	13/03/96	Elevation:	1182 metres
	Map Ref.:	Sheet No. : 8526   DGPS	Rainfall:	No Data
	Northing/Long.:	6040005 AMG zone: 55	Runoff:	No Data
	Easting/Lat.:	615167  Datum: AGD66	Drainage:	Moderately well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	Probable
	Geol. Ref.:	Tb	Substrate Material:	Basalt 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	No Data
	Morph. Type:	Crest	Relief:	No Data
	Elem. Type:	Hillcrest	Slope Category:	No Data
	Slope:	1 % 	Aspect:	0 degrees
	Surface Soil Condition (dry):	Firm
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Eutrophic Red Ferrosol Medium Slightly gravelly 	Principal Profile Form:	Gn3.21
	Loamy Clayey Deep
	ASC Confidence:	Great Soil Group:	Chocolate soil
	All necessary analytical data are available.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:
	Surface Coarse Fragments:
	Profile Morphology
	O1	0 - 0.01 m	Organic Layer; ; 
	A1	0.01 - 0.14 m	Dark reddish brown (5YR3/2-Moist); Biological mixing, 10YR44, 2-10% , Faint; Loam; Strong 
	grade of structure, 2-5 mm, Polyhedral; 5-10 mm, Polyhedral; Rough-ped fabric; Moderately 
	moist; Very weak consistence; 2-10%, fine gravelly, 2-6mm, subrounded, coarse fragments; 
	Field pH 4.5 (Raupach); Many, very fine (0-1mm) roots; Common, fine (1-2mm) roots; Common, 
	medium (2-5mm) roots; Common, coarse (>5mm) roots; Clear, Wavy change to - 
	B21	0.14 - 0.4 m	Dark reddish brown (5YR3/4-Moist); Biological mixing, 7.5YR32, 2-10% , Faint; Clay loam; 
	Moderate grade of structure, Subangular blocky; 10-20 mm, Subangular blocky; Rough-ped 
	fabric; Moderately moist; Weak consistence; 2-10%, fine gravelly, 2-6mm, subrounded, coarse 
	fragments; Field pH 6 (Raupach); Common, very fine (0-1mm) roots; Few, fine (1-2mm) roots; 
	Few, medium (2-5mm) roots; Few, coarse (>5mm) roots; Clear, Smooth change to - 
	B22	0.4 - 0.56 m	Dark brown (7.5YR3/4-Moist); ; Light clay; Moderate grade of structure, 10-20 mm, Subangular 
	blocky; 5-10 mm, Polyhedral; Rough-ped fabric; Moderately moist; Weak consistence; 10-20%, 
	fine gravelly, 2-6mm, subrounded, coarse fragments; Few cutans, <10% of ped faces or walls 
	coated, faint; Field pH 5.5 (Raupach); Common, very fine (0-1mm) roots; Few, fine (1-2mm) 
	roots; Gradual, Irregular change to - 
	B23	0.56 - 0.78 m	Dark brown (7.5YR3/4-Moist); ; Light clay; Strong grade of structure, 10-20 mm, Subangular 
	blocky; 2-5 mm, Polyhedral; Smooth-ped fabric; Moderately moist; Firm consistence; 20-50%, 
	fine gravelly, 2-6mm, subrounded, coarse fragments; Common cutans, 10-50% of ped faces or 
	walls coated, distinct; Field pH 5.5 (Raupach); Few, very fine (0-1mm) roots; Gradual, Tongued 
	change to - 
	B3	0.78 - 1.36 m	Dark brown (7.5YR3/4-Moist); ; Light clay; Strong grade of structure, 10-20 mm, Subangular 
	blocky; 2-5 mm, Polyhedral; Smooth-ped fabric; Moist; Firm consistence; 20-50%, medium 
	gravelly, 6-20mm, subrounded tabular, coarse fragments; Common cutans, 10-50% of ped faces
	 or walls coated, distinct; Field pH 5 (Raupach); Few, very fine (0-1mm) roots; Few, fine (1-2mm) 
	roots; 
	Morphological Notes
	A1	Strong aggregration gives sub-plasticfeatures. Possibly colluvial origin.
	B21	A light, friable layer which may have had a lot of faunal pedoturbation. Possibly of 
	colluvial origin.

	Project Name:	BAGO-MARAGLE FOREST SOIL SURVEY         
	Project Code:	BGM_FSS	Site ID:	0044	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	B22	Texture and consistence increase gravel content also increases indicating less  
	disturbance.                                                                                                            
	B23	Basalt floaters common in this layer.                                                                                   
	                                                                                
	B3	Auger stopped by floaters, layer could continue.
	Observation Notes
	Basalt pm has a near - pisolithic structure producing common small gravel.
	Site Notes
	COMP1174H 9356-1,316D 240M fr 9602-1  

	Project Name:	BAGO-MARAGLE FOREST SOIL SURVEY         
	Project Code:	BGM_FSS	Site ID:	0044	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.01
	0.01 - 0.14	4.31C	2.96H	1.37	0.89	0.05	5.39J	10.66E
	0K
	0.14 - 0.4	4.78C	2.34H	1.51	0.68	0.03	0.93J	5.49E
	0K
	0.4 - 0.56	5.03C	3.74H	2.89	1.33	0.02	0.2J	8.18E
	0K
	0.56 - 0.78	4.84C	3.35H	3.27	1.3	0.04	0.45J	8.42E
	0K
	0.78 - 1.36	4.63C	3.35H	2.76	0.88	0.17	0.98J	8.14E
	0K
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.01
	0.01 - 0.14	8.45B	4742.9B	0.33A	0.68	37.37
	0.14 - 0.4	2.98B	3952.3B	0.12A	1.08	15.88
	0.4 - 0.56	0.75B	3661.8B	0.03A	1.01	28.63
	0.56 - 0.78	0.64B	3546.7B	0.01A	36.19
	0.78 - 1.36	0.38B	3099.4B	0A	34.71
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.01
	0.01 - 0.14
	0.14 - 0.4
	0.4 - 0.56
	0.56 - 0.78
	0.78 - 1.36

	Project Name:	BAGO-MARAGLE FOREST SOIL SURVEY         
	Project Code:	BGM_FSS	Site ID:	0044	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Analyses Completed for this profile
	13C1_AL	Citrate/dithionite-extractable iron, aluminium, Manganese and Silicon
	13C1_FE	Citrate/dithionite-extractable iron, aluminium, Manganese and Silicon
	15_NR	Sum of Ex. cations + Ex. acidity - Not recorded
	15E1_AL	Exchangeable Al - by compulsive exchange, no pretreatment for soluble salts
	15E1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) by compulsive exchange, no pretreatment for soluble 
	15E1_H	Exchangeable H - by compulsive exchange, no pretreatment for soluble salts
	15E1_K	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MG	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_NA	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	2A1	Air-dry moisture content
	4B2	pH of 1:5 soil/0.01M calcium chloride extract - following Method 4A1
	6B2	Total organic carbon - high frequency induction furnace, volumetric
	7A2	Total nitrogen - semimicro Kjeldahl , automated colour
	9A3	Total Phosphorus (ppm) - semimicro kjeldahl, automated colour
	P10_GRAV	Gravel (%)
	P10_S_0.48	0.48 micron (cumulative %) - Sedigraph
	P10_S_1	1 micron (cumulative %) - Sedigraph
	P10_S_1000	1000 micron (cumulative %) - Sedigraph
	P10_S_125	125 micron (cumulative %) - Sedigraph
	P10_S_15.6	15.6 micron (cumulative %) - Sedigraph
	P10_S_2	2 micron (cumulative %) - Sedigraph
	P10_S_20	20 micron (cumulative %) - Sedigraph
	P10_S_2000	2000 micron (cumulative %) - Sedigraph
	P10_S_250	250 micron (cumlative %) - Sedigraph
	P10_S_3.9	3.9 micron (cumulative %) - Sedigraph
	P10_S_31.2	31.2 micron (cumulative %) - Sedigraph
	P10_S_500	500 micron (cumulative %) - Sedigraph
	P10_S_53	53 micron (cumulative %) - Sedigraph
	P10_S_63	63 micron (cumulative %) - Sedigraph
	P10_S_7.8	7.8 micron (cumulative %) - Sedigraph
	P3A1	Bulk density - g/cm3