Project Name:	BAGO-MARAGLE FOREST SOIL SURVEY         
	Project Code:	BGM_FSS	Site ID:	0051	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Site Information
	Desc. By:	N.J. McKenzie	Locality:
	Date Desc.:	09/01/96	Elevation:	1117 metres
	Map Ref.:	Sheet No. : 8526   DGPS	Rainfall:	No Data
	Northing/Long.:	6027336 AMG zone: 55	Runoff:	No Data
	Easting/Lat.:	616180  Datum: AGD66	Drainage:	Rapidly drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	Probable
	Geol. Ref.:	Dga	Substrate Material:	Adamellite 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	No Data
	Morph. Type:	Upper-slope	Relief:	No Data
	Elem. Type:	No Data	Slope Category:	No Data
	Slope:	17 % 	Aspect:	180 degrees
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Acidic Mesotrophic Red Kandosol Medium Non-gravelly Clay-	Principal Profile Form:	Gn4.11
	loamy Clayey Very deep
	ASC Confidence:	Great Soil Group:	N/A
	All necessary analytical data are available.
	Site Disturbance:
	Vegetation:
	Surface Coarse Fragments:
	Profile Morphology
	A11	0 - 0.11 m	Very dark grey (5YR3/1-Moist); ; Clay loam, coarse sandy; Moderate grade of structure, 5-10 mm, 
	Granular; 20-50 mm, Subangular blocky; Rough-ped fabric; Moderately moist; Very weak 
	consistence; Few cutans, <10% of ped faces or walls coated, faint; Field pH 6.5 (Raupach); 
	Many, very fine (0-1mm) roots; Few, fine (1-2mm) roots; Few, medium (2-5mm) roots; Few, coarse
	 (>5mm) roots; Clear, Smooth change to - 
	A12	0.11 - 0.21 m	Dark reddish brown (5YR3/2-Moist); Biological mixing, 5YR54, 20-50% , Distinct; Light clay; 
	Moderate grade of structure, 10-20 mm, Polyhedral; Rough-ped fabric; Moderately moist; Weak 
	consistence; 0-2%, cobbly, 60-200mm, subrounded, dispersed, Adamellite, coarse fragments; 
	Few cutans, <10% of ped faces or walls coated, faint; Field pH 6 (Raupach); Many, very fine (0-
	1mm) roots; Few, fine (1-2mm) roots; Few, medium (2-5mm) roots; Few, coarse (>5mm) roots; 
	Clear, Smooth change to - 
	B21	0.21 - 0.5 m	Reddish brown (5YR4/4-Moist); ; Light clay; Moderate grade of structure, 20-50 mm, Polyhedral; 
	Rough-ped fabric; Moderately moist; Weak consistence; Common cutans, 10-50% of ped faces 
	or walls coated, distinct; Field pH 6 (Raupach); Common, very fine (0-1mm) roots; Few, fine (1-
	2mm) roots; Common, medium (2-5mm) roots; Few, coarse (>5mm) roots; Diffuse, Smooth 
	change to - 
	B22	0.5 - 0.95 m	Yellowish red (5YR4/6-Moist); ; Clay loam; Massive grade of structure; Earthy fabric; Moderately 
	moist; Firm consistence; 0-2%, cobbly, 60-200mm, subrounded, dispersed, Adamellite, coarse 
	fragments; Few cutans, <10% of ped faces or walls coated, faint; Field pH 6 (Raupach); Few, 
	very fine (0-1mm) roots; Few, fine (1-2mm) roots; Clear, Smooth change to - 
	B3	0.95 - 1.2 m	Yellowish red (5YR5/6-Moist); ; Clay loam, coarse sandy; Massive grade of structure; Earthy 
	fabric; Moderately moist; Firm consistence; 2-10%, fine gravelly, 2-6mm, subangular, dispersed,
	 coarse fragments; 10-20%, fine gravelly, 2-6mm, subangular, dispersed, Quartz, coarse 
	fragments; Few cutans, <10% of ped faces or walls coated, faint; Field pH 5.5 (Raupach); Few, 
	very fine (0-1mm) roots; Clear, Smooth change to - 
	C11	1.2 - 1.55 m	Reddish yellow (5YR7/6-Moist); ; Sandy loam; Massive grade of structure; Sandy (grains 
	prominent) fabric; Moderately moist; 10-20%, fine gravelly, 2-6mm, subangular, undisturbed, 
	coarse fragments; 10-20%, fine gravelly, 2-6mm, subangular, undisturbed, Quartz, coarse 
	fragments; Field pH 5.5 (Raupach); Abrupt, Smooth change to - 

	Project Name:	BAGO-MARAGLE FOREST SOIL SURVEY         
	Project Code:	BGM_FSS	Site ID:	0051	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	C12	1.55 - 1.65 m	Reddish yellow (5YR6/6-Moist); ; Sandy loam; Massive grade of structure; Sandy (grains 
	prominent) fabric; Moderately moist; 10-20%, fine gravelly, 2-6mm, subangular, undisturbed, 
	Quartz, coarse fragments; 10-20%, fine gravelly, 2-6mm, subangular, undisturbed, coarse 
	fragments; Field pH 5.5 (Raupach); Abrupt change to - 
	C21	1.65 - 2.1 m	Reddish yellow (5YR7/6-Moist); ; Sandy loam; Massive grade of structure; Sandy (grains 
	prominent) fabric; Moderately moist; 10-20%, fine gravelly, 2-6mm, subangular, undisturbed, 
	Quartz, coarse fragments; 10-20%, fine gravelly, 2-6mm, subangular, undisturbed, coarse 
	fragments; Field pH 5 (Raupach); Abrupt change to - 
	C22	2.1 - 2.2 m	Reddish yellow (5YR6/8-Moist); ; Sandy loam; Massive grade of structure; Sandy (grains 
	prominent) fabric; Moderately moist; 10-20%, fine gravelly, 2-6mm, subangular, undisturbed, 
	Quartz, coarse fragments; 10-20%, fine gravelly, 2-6mm, subangular, undisturbed, coarse 
	fragments; Field pH 5 (Raupach); Abrupt change to - 
	C3	2.2 - 3 m	Reddish yellow (5YR7/6-Moist); ; Sandy loam; Massive grade of structure; Sandy (grains 
	prominent) fabric; Moderately moist; 10-20%, fine gravelly, 2-6mm, subangular, undisturbed, 
	Quartz, coarse fragments; 10-20%, fine gravelly, 2-6mm, subangular, undisturbed, coarse 
	fragments; Field pH 5 (Raupach); 
	Morphological Notes
	A12	slight hint of an A2 but abundant bioturbation counters development.
	B22	Massive and more dense.                                                                                                     
	                                                                            
	B3	Coarse frags increase - base of transportational zone.
	C11	Saprolite                                                                                                                               
	                                                                
	Observation Notes
	Site Notes
	COMP 40H,3545-1,110.5D,60M FR RIDGE   

	Project Name:	BAGO-MARAGLE FOREST SOIL SURVEY         
	Project Code:	BGM_FSS	Site ID:	0051	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.11	4.88C	10.84H	1.78	0.84	0	0.54J	13.99E
	0K
	0.11 - 0.21	4.54C	3.85H	0.92	0.6	0.01	1.21J	6.58E
	0K
	0.21 - 0.5	4.23C	3.43H	1.25	0.83	0.02	1.85J	7.38E
	0K
	0.5 - 0.95	4.03C	1.31H	0.99	0.61	0.01	3.07J	5.99E
	0K
	0.95 - 1.2	4.1C	1.2H	0.84	0.66	0.02	1.94J	4.66E
	0K
	1.2 - 1.55	4.25C	0.49H	0.33	0.74	0.02	0.71J	2.3E
	0K
	1.55 - 1.65	4.24C	0.33H	0.23	0.52	0	0.71J	1.8E
	0K
	1.65 - 2.1	4.21C	0.45H	0.26	0.41	0.05	0.7J	1.88E
	0K
	2.1 - 2.2	4.04C	0.31H	0.25	0.3	0.01	1.4J	2.27E
	0K
	2.2 - 3	4.03C	0.06H	0.16	0.3	0.02	1.42J	1.96E
	0K
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.11	4.8B	278.4B	0.19A	1.04	40.14
	0.11 - 0.21	1.82B	220B	0.08A	1.45	36.87
	0.21 - 0.5	0.99B	261.2B	0.06A	1.30	36.39
	0.5 - 0.95	0.36B	224.6B	0.03A	1.24	37.98
	0.95 - 1.2	0.27B	138.4B	0.02A	42.17
	1.2 - 1.55	0.1B	75.6B	0A	31.36
	1.55 - 1.65	0.09B	69.9B	0A	33.71
	1.65 - 2.1	0.08B	12B	0A	34.64
	2.1 - 2.2	0.12B	73.5B	0A	39.57
	2.2 - 3	0.06B	59.7B	0A	28.56
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.11
	0.11 - 0.21
	0.21 - 0.5
	0.5 - 0.95
	0.95 - 1.2
	1.2 - 1.55
	1.55 - 1.65
	1.65 - 2.1
	2.1 - 2.2
	2.2 - 3

	Project Name:	BAGO-MARAGLE FOREST SOIL SURVEY         
	Project Code:	BGM_FSS	Site ID:	0051	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Analyses Completed for this profile
	15_NR	Sum of Ex. cations + Ex. acidity - Not recorded
	15E1_AL	Exchangeable Al - by compulsive exchange, no pretreatment for soluble salts
	15E1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) by compulsive exchange, no pretreatment for soluble 
	15E1_H	Exchangeable H - by compulsive exchange, no pretreatment for soluble salts
	15E1_K	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MG	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_NA	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	2A1	Air-dry moisture content
	4B2	pH of 1:5 soil/0.01M calcium chloride extract - following Method 4A1
	6B2	Total organic carbon - high frequency induction furnace, volumetric
	7A2	Total nitrogen - semimicro Kjeldahl , automated colour
	9A3	Total Phosphorus (ppm) - semimicro kjeldahl, automated colour
	P10_GRAV	Gravel (%)
	P3A1	Bulk density - g/cm3