Project Name:	BAGO-MARAGLE FOREST SOIL SURVEY         
	Project Code:	BGM_FSS	Site ID:	0106	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Site Information
	Desc. By:	N.J. McKenzie	Locality:
	Date Desc.:	23/04/96	Elevation:	1085 metres
	Map Ref.:	Sheet No. : 8526   DGPS	Rainfall:	No Data
	Northing/Long.:	6048883 AMG zone: 55	Runoff:	No Data
	Easting/Lat.:	612151  Datum: AGD66	Drainage:	Rapidly drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	Probable
	Geol. Ref.:	Sgg	Substrate Material:	Granodiorite 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	No Data
	Morph. Type:	Lower-slope	Relief:	No Data
	Elem. Type:	Footslope	Slope Category:	No Data
	Slope:	7 % 	Aspect:	0 degrees
	Surface Soil Condition (dry):	Firm
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Acidic Dystrophic Red Kandosol Medium Non-gravelly Silty 	Principal Profile Form:	Gn2.11
	Clayey Very deep
	ASC Confidence:	Great Soil Group:	N/A
	All necessary analytical data are available.
	Site Disturbance:	No effective disturbance. Natural
	Vegetation:
	Surface Coarse Fragments:
	Profile Morphology
	A11	0 - 0.09 m	Dark reddish brown (5YR3/2-Moist); ; Silty clay loam; Moderate grade of structure, 20-50 mm, 
	Polyhedral; 10-20 mm, Polyhedral; Rough-ped fabric; Moderately moist; Firm consistence; Few 
	cutans, <10% of ped faces or walls coated, faint; Field pH 6 (Raupach); Many, very fine (0-1mm) 
	roots; Few, fine (1-2mm) roots; Clear, Smooth change to - 
	A12	0.09 - 0.2 m	Dark reddish brown (5YR3/3-Moist); Biological mixing, 5YR2.52, 20-50% , Faint; Light clay; 
	Moderate grade of structure, 10-20 mm, Polyhedral; 20-50 mm, Polyhedral; Rough-ped fabric; 
	Moderately moist; Firm consistence; Common cutans, 10-50% of ped faces or walls coated, 
	faint; Field pH 6.5 (Raupach); Common, very fine (0-1mm) roots; Few, fine (1-2mm) roots; Few, 
	medium (2-5mm) roots; Few, coarse (>5mm) roots; Diffuse, Smooth change to - 
	B21	0.2 - 0.6 m	Dark red (2.5YR3/6-Moist); Biological mixing, 5YR33, 0-2% , Distinct; Light clay; Weak grade of 
	structure, 10-20 mm, Polyhedral; Rough-ped fabric; Moderately moist; Weak consistence; 
	Common cutans, 10-50% of ped faces or walls coated, faint; Field pH 6 (Raupach); Common, 
	very fine (0-1mm) roots; Few, fine (1-2mm) roots; Diffuse, Smooth change to - 
	B22	0.6 - 1.85 m	Dark red (2.5YR3/6-Moist); ; Light clay; Massive grade of structure; Earthy fabric; Moderately 
	moist; Firm consistence; Few cutans, <10% of ped faces or walls coated, faint; Field pH 4.5 
	(Raupach); Few, very fine (0-1mm) roots; Few, fine (1-2mm) roots; Diffuse, Smooth change to - 
	B23	1.85 - 2.75 m	Red (2.5YR4/6-Moist); ; Silty clay loam; Massive grade of structure; Earthy fabric; Moderately 
	moist; Firm consistence; Few cutans, <10% of ped faces or walls coated, faint; Field pH 5 
	(Raupach); Diffuse, Smooth change to - 
	B3	2.75 - 3 m	Red (2.5YR4/6-Moist); ; Silty clay loam; Massive grade of structure; Earthy fabric; Moderately 
	moist; Firm consistence; Few cutans, <10% of ped faces or walls coated, faint; Field pH 5 
	(Raupach); 
	Morphological Notes
	A11	Moderate density - may be due to grazing . Very silty.                                                          
	                                                                                        
	A12	Transitional horizon with mixing of colours  etc due to earthworms.
	B21	Whole coloured B2 with pedality diminishing with depth.
	B22	Clay content starts to decline but silt remains high and may even increase.                      

	Project Name:	BAGO-MARAGLE FOREST SOIL SURVEY         
	Project Code:	BGM_FSS	Site ID:	0106	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	B23	Micas are prevalent and increase slightly with depth.
	B3	Sllight change may be due to grittiness - hint of a BC. This layer is a B24 more than a 
	B31.                                                                                                            
	Observation Notes
	Extremely uniform deep red profile with mod. stong  weathering to depth. Siltiness is high . Stable surface and well drained. 
	Micas increase slightly with   depth.
	Site Notes
	COMP 60H 29858-1 18D 60M FROM TRACK   

	Project Name:	BAGO-MARAGLE FOREST SOIL SURVEY         
	Project Code:	BGM_FSS	Site ID:	0106	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.09	5C	19.39H	2.06	1.26	0.07	0.34J	23.11E
	0K
	0.09 - 0.2	5.14C	11.07H	1.75	0.55	0.16	0.1J	13.63E
	0K
	0.2 - 0.6	4.74C	4.66H	2.67	0.7	0.14	0.76J	8.93E
	0K
	0.6 - 1.85	3.98C	0.32H	0.45	0.34	0.12	5.47J	6.7E
	0K
	1.85 - 2.75	3.93C	0.03H	0.32	0.2	0.12	5.43J	6.11E
	0K
	2.75 - 3	3.96C	0H	0.22	0.15	0.12	4.71J	5.2E
	0K
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.09	6.92B	651.9B	0.3A	0.78	34.89
	0.09 - 0.2	2.36B	656.9B	0.18A	1.09	40.1
	0.2 - 0.6	0.81B	451.9B	0.08A	1.09	32.45
	0.6 - 1.85	0.25B	388.2B	0.04A	1.10	28.31
	1.85 - 2.75	0.19B	288.4B	0.03A	31.32
	2.75 - 3	0.15B	223.6B	0.03A	27.61
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.09
	0.09 - 0.2
	0.2 - 0.6
	0.6 - 1.85
	1.85 - 2.75
	2.75 - 3

	Project Name:	BAGO-MARAGLE FOREST SOIL SURVEY         
	Project Code:	BGM_FSS	Site ID:	0106	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Analyses Completed for this profile
	15_NR	Sum of Ex. cations + Ex. acidity - Not recorded
	15E1_AL	Exchangeable Al - by compulsive exchange, no pretreatment for soluble salts
	15E1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) by compulsive exchange, no pretreatment for soluble 
	15E1_H	Exchangeable H - by compulsive exchange, no pretreatment for soluble salts
	15E1_K	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MG	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_NA	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	2A1	Air-dry moisture content
	4B2	pH of 1:5 soil/0.01M calcium chloride extract - following Method 4A1
	6B2	Total organic carbon - high frequency induction furnace, volumetric
	7A2	Total nitrogen - semimicro Kjeldahl , automated colour
	9A3	Total Phosphorus (ppm) - semimicro kjeldahl, automated colour
	P10_GRAV	Gravel (%)
	P3A1	Bulk density - g/cm3