Project Name:	BAGO-MARAGLE FOREST SOIL SURVEY         
	Project Code:	BGM_FSS	Site ID:	0107	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Site Information
	Desc. By:	N.J. McKenzie	Locality:
	Date Desc.:	23/04/96	Elevation:	1078 metres
	Map Ref.:	Sheet No. : 8526   DGPS	Rainfall:	No Data
	Northing/Long.:	6052029 AMG zone: 55	Runoff:	No Data
	Easting/Lat.:	611588  Datum: AGD66	Drainage:	Rapidly drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	Probable
	Geol. Ref.:	Sgg	Substrate Material:	Granodiorite 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	No Data
	Morph. Type:	Mid-slope	Relief:	No Data
	Elem. Type:	Hillslope	Slope Category:	No Data
	Slope:	18 % 	Aspect:	0 degrees
	Surface Soil Condition (dry):	Firm
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Acidic Dystrophic Red Kandosol Medium Non-gravelly Silty 	Principal Profile Form:	Um6.
	Silty Very deep
	ASC Confidence:	Great Soil Group:	N/A
	All necessary analytical data are available.
	Site Disturbance:
	Vegetation:
	Surface Coarse Fragments:
	Profile Morphology
	A1	0 - 0.19 m	Dark reddish brown (5YR3/2-Moist); Biological mixing, 5YR44, 20-50% , Distinct; Silty clay 
	loam; Moderate grade of structure, 10-20 mm, Polyhedral; Rough-ped fabric; Moderately moist; 
	Firm consistence; Common cutans, 10-50% of ped faces or walls coated, distinct; Field pH 6 
	(Raupach); Many, very fine (0-1mm) roots; Common, fine (1-2mm) roots; Common, medium (2-
	5mm) roots; Common, coarse (>5mm) roots; Clear, Smooth change to - 
	B21	0.19 - 0.54 m	Red (2.5YR4/6-Moist); Biological mixing, 5YR32, 2-10% , Distinct; Silty clay loam; Weak grade 
	of structure, 10-20 mm, Polyhedral; Earthy fabric; Moderately moist; Weak consistence; Few 
	cutans, <10% of ped faces or walls coated, faint; Field pH 5 (Raupach); Common, very fine (0-
	1mm) roots; Few, fine (1-2mm) roots; Few, medium (2-5mm) roots; Few, coarse (>5mm) roots; 
	Diffuse, Smooth change to - 
	B22	0.54 - 1.3 m	Red (2.5YR4/6-Moist); ; Silty clay loam; Massive grade of structure; Earthy fabric; Moderately 
	moist; Weak consistence; 0-2%, coarse gravelly, 20-60mm, angular platy, dispersed, 
	Granodiorite, coarse fragments; Few cutans, <10% of ped faces or walls coated, faint; Field pH 
	5 (Raupach); Common, very fine (0-1mm) roots; Few, fine (1-2mm) roots; Few, medium (2-5mm) 
	roots; Few, coarse (>5mm) roots; Clear, Smooth change to - 
	C1	1.3 - 1.95 m	Yellow (10YR7/6-Moist); ; Loamy sand; Massive grade of structure; Moderately moist; Very weak 
	consistence; Field pH 7 (Raupach); Gradual, Smooth change to - 
	C2	1.95 - 2.7 m	Light yellowish brown (10YR6/4-Moist); Substrate influence, 10YR76, 20-50% , Distinct; Loamy 
	sand; Massive grade of structure; Moderately moist; Very weak consistence; Field pH 6 
	(Raupach); Diffuse, Smooth change to - 
	C3	2.7 - 3 m	Pale brown (10YR6/3-Moist); ; Loamy sand; Massive grade of structure; Moderately moist; Very 
	weak consistence; Field pH 7 (Raupach); 
	Morphological Notes
	A1	Mod. to strong structure due to abundant worm activity. Fair degree of B2 mixed in as 
	casts.                                                                                                            
	B21	Well developed marcropores through to layer 3. Much lighter colour/texture and more 
	earthy fabric than site BM106.
	B22	Earthy B22.                                                                                                                           

	Project Name:	BAGO-MARAGLE FOREST SOIL SURVEY         
	Project Code:	BGM_FSS	Site ID:	0107	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	C1	Sharp contrast into sandy C horizon with abundant mafic minerals.                                   
	                                                                                                    
	C2	Very similar to 4 but with slightly different colours.
	C3	Similar to 5 but slightly harder to auger.
	Observation Notes
	Ridgeline running north. Large worm population. Sharp contrast between B and C. Presume soil is quite young. Light texture 
	and more earthy fabric.
	Site Notes
	COMP 32H 17343-1 301D 300M FROM RD/CK 

	Project Name:	BAGO-MARAGLE FOREST SOIL SURVEY         
	Project Code:	BGM_FSS	Site ID:	0107	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.19	4.47C	5.94H	0.19	1.17	0.13	1.9J	9.34E
	0K
	0.19 - 0.54	4.18C	0.37H	0.33	0.42	0.12	2.67J	3.9E
	0K
	0.54 - 1.3	4.11C	0.23H	0.5	0.25	0.09	2.45J	3.53E
	0K
	1.3 - 1.95	4.45C	0H	0.09	0.06	0.08	0.22J	0.45E
	0K
	1.95 - 2.7	4.46C	0H	0.08	0.14	0.09	0.17J	0.47E
	0K
	2.7 - 3	4.58C	0H	0.06	0	0.08	0.09J	0.22E
	0K
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.19	3.98B	361.9B	0.2A	0.89	33.3
	0.19 - 0.54	0.82B	702.5B	0.06A	1.18	20.65
	0.54 - 1.3	0.3B	249.4B	0.02A	1.22	13.62
	1.3 - 1.95	0.06B	89.5B	0.01A	5.76
	1.95 - 2.7	0.05B	154.5B	0.01A	3.55
	2.7 - 3	0.04B	104.6B	0.01A	3.01
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.19
	0.19 - 0.54
	0.54 - 1.3
	1.3 - 1.95
	1.95 - 2.7
	2.7 - 3

	Project Name:	BAGO-MARAGLE FOREST SOIL SURVEY         
	Project Code:	BGM_FSS	Site ID:	0107	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Analyses Completed for this profile
	15_NR	Sum of Ex. cations + Ex. acidity - Not recorded
	15E1_AL	Exchangeable Al - by compulsive exchange, no pretreatment for soluble salts
	15E1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) by compulsive exchange, no pretreatment for soluble 
	15E1_H	Exchangeable H - by compulsive exchange, no pretreatment for soluble salts
	15E1_K	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MG	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_NA	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	2A1	Air-dry moisture content
	4B2	pH of 1:5 soil/0.01M calcium chloride extract - following Method 4A1
	6B2	Total organic carbon - high frequency induction furnace, volumetric
	7A2	Total nitrogen - semimicro Kjeldahl , automated colour
	9A3	Total Phosphorus (ppm) - semimicro kjeldahl, automated colour
	P10_GRAV	Gravel (%)
	P3A1	Bulk density - g/cm3